Memperkenalkan sebuah terobosan dalam analisis elemental logam, sebuah Optical Emission Spectrometer (OES) berdesain benchtop yang menggabungkan kekuatan analitis luar biasa dengan efisiensi ruang. Instrumen ini adalah solusi andal untuk pabrik pengecoran, industri fabrikasi logam, laboratorium kontrol kualitas, dan fasilitas daur ulang yang membutuhkan identifikasi komposisi kimia secara cepat dan akurat. Dengan waktu pengujian rata rata hanya 25 detik, Anda dapat secara dramatis mempercepat proses verifikasi material, memastikan setiap produk memenuhi spesifikasi yang paling ketat sekalipun.
Inti dari kinerja superior instrumen ini adalah sistem optik vakum penuh dengan konstruksi Paschen Runge. Desain canggih ini menjamin stabilitas jangka panjang dan sensitivitas deteksi yang superior di seluruh rentang panjang gelombang yang luas dari 130 hingga 800 nm. Dilengkapi dengan detektor CCD Array berkinerja tinggi, spektrometer ini mampu menangkap dan menganalisis spektrum emisi dari berbagai macam elemen dalam matriks substrat yang berbeda, termasuk Besi (Fe), Aluminium (Al), Tembaga (Cu), Nikel (Ni), Titanium (Ti), dan banyak lagi.
Teknologi inovatif menjadi tulang punggung dari setiap pengukuran yang akurat. Dengan teknologi pra pembakaran energi tinggi (HEPS) dan sumber cahaya digital baru yang dapat disesuaikan, instrumen ini memastikan eksitasi sampel yang optimal dan stabil. Hal ini menghasilkan data yang sangat dapat diulang dan akurat untuk analisis paduan logam yang kompleks. Elektroda injeksi berbahan tungsten yang tahan lama juga memastikan kinerja yang konsisten dan andal dalam jangka waktu yang panjang dengan kebutuhan perawatan yang minimal, menjadikannya sebuah investasi yang cerdas dan efisien.
Dirancang untuk kemudahan penggunaan dan keandalan operasional, spektrometer ini beroperasi dengan gas argon kemurnian tinggi untuk menciptakan lingkungan percikan yang ideal. Desainnya yang ringkas tidak mengorbankan kekuatan, memberikan kemampuan analisis layaknya instrumen berukuran besar namun dengan jejak yang jauh lebih kecil. Ini adalah alat kerja keras yang esensial untuk identifikasi material positif (PMI), grading paduan, dan penelitian metalurgi, memberikan Anda keyakinan penuh pada kualitas material Anda setiap saat.

Introducing a breakthrough in elemental metal analysis, a benchtop Optical Emission Spectrometer (OES) that combines exceptional analytical power with space efficiency. This instrument is the reliable solution for foundries, metal fabrication industries, quality control laboratories, and recycling facilities that require fast and accurate chemical composition identification. With an average testing time of just 25 seconds, you can dramatically accelerate your material verification process, ensuring every product meets the most stringent specifications.
At the core of this instrument's superior performance is its full vacuum optical system featuring a Paschen Runge construction. This advanced design guarantees long term stability and superior detection sensitivity across a wide wavelength coverage from 130 to 800 nm. Equipped with a high performance CCD Array detector, the spectrometer is capable of capturing and analyzing the emission spectra of a vast range of elements in different substrate matrices, including Iron (Fe), Aluminum (Al), Copper (Cu), Nickel (Ni), Titanium (Ti), and many more.
Innovative technology is the backbone of every accurate measurement. Featuring High Energy Pre-combustion Technology (HEPS) and a new digital adjustable light source, this instrument ensures optimal and stable sample excitation. This results in highly repeatable and precise data for the analysis of complex metal alloys. The durable Tungsten material injection electrode also ensures consistent, reliable performance over a long period with minimal maintenance requirements, making it a smart and efficient investment.
Engineered for ease of use and operational reliability, this spectrometer operates with high purity argon gas to create the ideal spark environment. Its compact, benchtop design does not compromise on power, delivering the analytical capabilities of larger floor standing instruments with a much smaller footprint. It is the essential workhorse for positive material identification (PMI), alloy grading, and metallurgical research, giving you complete confidence in your material quality every single time.

