Tinggalkan metode pengadukan satu per satu yang memakan waktu. Kini hadir solusi canggih untuk laboratorium modern, Pengaduk Magnetik Multi Posisi. Dirancang untuk efisiensi superior, alat ini memungkinkan Anda mengaduk beberapa sampel larutan secara serentak dalam kondisi yang seragam dan terkontrol, memastikan konsistensi dan reprodusibilitas hasil yang tak tertandingi.
Setiap posisi pengadukan bekerja secara independen namun sinkron, memberikan pusaran yang kuat dan stabil untuk berbagai viskositas cairan. Beberapa varian juga dilengkapi dengan fungsi pemanasan presisi tinggi (hotplate), memungkinkan Anda melakukan sintesis, disolusi, atau reaksi kimia yang sensitif terhadap suhu pada banyak sampel sekaligus. Ini adalah alat yang ideal untuk studi perbandingan, skrining, dan preparasi sampel dalam volume tinggi.
Dibangun untuk penggunaan jangka panjang di lingkungan lab yang menuntut, perangkat ini ditenagai oleh motor DC brushless yang andal, hening, dan bebas perawatan. Platform kerjanya terbuat dari material premium seperti stainless steel atau paduan aluminium, menawarkan ketahanan kimia yang sangat baik dan distribusi panas yang merata. Kendalikan kecepatan atau suhu dengan mudah melalui tombol putar (knob) atau tombol tekan (button) intuitif untuk pengaturan yang akurat.
Ideal untuk aplikasi dalam bidang kimia, biologi, farmasi, analisis lingkungan, dan quality control, pengaduk magnetik multi posisi ini adalah sebuah investasi cerdas. Hemat ruang berharga di meja lab Anda, kurangi waktu kerja, dan tingkatkan kapasitas pengujian secara dramatis. Ini bukan hanya sebuah alat, melainkan sebuah pusat efisiensi untuk laboratorium Anda.

Leave time consuming single sample stirring methods behind. Introducing an advanced solution for the modern laboratory: the Multi Position Magnetic Stirrer. Engineered for superior efficiency, this instrument allows you to stir multiple solution samples simultaneously under uniform and controlled conditions, ensuring unparalleled consistency and reproducibility of results.
Each stirring position operates independently yet synchronously, delivering a powerful and stable vortex for a wide range of liquid viscosities. Select variants are also equipped with a high precision heating function (hotplate), enabling you to perform temperature sensitive syntheses, dissolutions, or chemical reactions on many samples at once. It is the ideal tool for comparative studies, screening, and high volume sample preparation.
Built for long term use in demanding lab environments, this device is powered by a reliable, quiet, and maintenance free brushless DC motor. Its work platform is crafted from premium materials like stainless steel or aluminum alloy, offering excellent chemical resistance and even heat distribution. Easily control the speed or temperature via intuitive knobs or buttons for precise adjustments.
Ideal for applications in chemistry, biology, pharmaceuticals, environmental analysis, and quality control, this multi position magnetic stirrer is a smart investment. Save valuable bench space, reduce manual labor time, and dramatically increase your testing throughput. This is not just an instrument; it is an efficiency hub for your laboratory.

