Integritas struktural sebuah sepatu bergantung sepenuhnya pada kekuatan ikatan antara sol dan bagian atasnya (upper). Kegagalan pada sambungan ini, yang sering disebut 'sol jebol' atau 'sol copot', adalah salah satu cacat produk yang paling fatal dan langsung terlihat oleh konsumen, yang dapat secara instan merusak kepercayaan terhadap sebuah merek. Kami mempersembahkan sebuah instrumen presisi yang dirancang khusus untuk satu tujuan vital: mengukur secara akurat dan kuantitatif kekuatan kupas (peeling strength) pada titik sambungan krusial tersebut. Alat ini adalah garda terdepan Anda untuk memvalidasi kualitas proses pengeleman dan memastikan setiap pasang sepatu yang diproduksi memiliki daya tahan ikatan yang superior.
Mesin ini bekerja dengan metodologi yang sederhana namun sangat efektif. Menggunakan pisau pemotong dengan lebar yang terstandarisasi, alat ini secara sistematis mengupas bagian upper dari sol dengan kecepatan yang lambat dan terkontrol. Selama proses ini, gaya yang dibutuhkan untuk memisahkan kedua komponen tersebut diukur secara presisi. Nilai gaya inilah yang kemudian dikalkulasikan menjadi kekuatan kupas, memberikan Anda data numerik yang jelas tentang kualitas adhesi. Data ini memungkinkan Anda untuk menetapkan standar kualitas yang tegas, membandingkan performa perekat yang berbeda, dan mengoptimalkan proses produksi untuk hasil yang konsisten dan andal.
Setiap detail pada mesin ini dirancang untuk akurasi dan repetabilitas. Pilihan lebar pisau yang presisi (20±0.1mm atau 10±0.05mm) memastikan pengujian dilakukan sesuai parameter standar. Kecepatan gerak yang terkontrol dan dapat disesuaikan (20±2mm/menit) menghilangkan inkonsistensi yang disebabkan oleh pengujian manual, sehingga hasilnya dapat diandalkan dan dipercaya. Pengukuran dicatat oleh indikator dial dengan resolusi tinggi hingga 0.001mm, mampu menangkap variasi sekecil apa pun dalam kekuatan ikatan. Dengan kemampuan penyesuaian jarak dan rentang angkat, mesin ini dapat mengakomodasi berbagai desain dan ukuran sepatu dengan mudah.
Dengan bobot 45 Kg, instrumen ini menawarkan platform yang stabil untuk pengujian yang akurat di lingkungan laboratorium atau langsung di lini produksi. Pengoperasiannya yang mekanis dan lugas memastikan keandalan jangka panjang dengan perawatan minimal. Mengintegrasikan alat uji kekuatan kupas ini ke dalam protokol quality control Anda bukan lagi sebuah pilihan, melainkan sebuah keharusan. Ini adalah investasi cerdas untuk mencegah penarikan produk yang mahal, mengurangi klaim garansi, dan yang terpenting, membangun reputasi merek yang identik dengan kualitas dan daya tahan yang tak tergoyahkan.
The structural integrity of a shoe depends entirely on the bond strength between its sole and its upper. A failure at this joint, often resulting in sole separation, is one of the most catastrophic and publicly visible product defects, capable of instantly destroying consumer trust in a brand. We present a precision instrument designed for one vital purpose: to accurately and quantitatively measure the peeling strength at that crucial junction. This device is your frontline defense for validating the quality of your cementing process and ensuring every pair of shoes produced has superior bond durability.
This machine operates on a simple yet highly effective methodology. Using a standardized width cutting blade, the device systematically peels the upper from the sole at a slow, controlled speed. During this process, the force required to separate the two components is precisely measured. This force value is then calculated to determine the peeling strength, providing you with clear, numerical data on the quality of adhesion. This data allows you to set firm quality benchmarks, compare the performance of different adhesives, and optimize your production process for consistent, reliable results.
Every detail of this machine is engineered for accuracy and repeatability. The choice of precision blade widths (20±0.1mm or 10±0.05mm) ensures testing is conducted according to standard parameters. A controlled and adjustable moving speed (20±2mm/min) eliminates the inconsistencies of manual testing, making the results dependable and trustworthy. Measurements are recorded by a high-resolution dial indicator, capable of reading down to 0.001mm, capturing even the slightest variations in bond strength. With adjustable distances and an accommodating elevating range, this machine can easily handle various shoe designs and sizes.
Weighing a stable 45 Kg, this instrument provides a solid platform for accurate testing in a laboratory setting or directly on the production line. Its straightforward, mechanical operation ensures long term reliability with minimal maintenance. Integrating this peeling strength tester into your quality control protocol is no longer an option—it is a necessity. It is a smart investment to prevent costly product recalls, reduce warranty claims, and most importantly, build a brand reputation that is synonymous with unshakeable quality and durability.

