Daya tahan sebuah sepatu berawal dari fondasinya, yaitu sol. Sol yang retak atau pecah bukan hanya mengurangi nilai estetika, tetapi juga merupakan kegagalan fungsional total yang mengakhiri umur pakai produk. Kami mempersembahkan sebuah perangkat pengujian fundamental yang dirancang khusus untuk mengevaluasi ketahanan material sol terhadap keretakan akibat pelenturan berulang. Mesin ini adalah instrumen vital untuk produsen sol, kompon karet, dan merek alas kaki yang berkomitmen untuk memastikan komponen paling kritis dari produk mereka dapat menahan tekanan penggunaan sehari-hari tanpa mengalami kegagalan.
Keunggulan paling signifikan dari alat uji ini adalah kepatuhannya terhadap serangkaian standar desain internasional yang paling dihormati: EN344, SATRA TM161, dan ISO 17707. Kepatuhan multi-standar ini menjadikan mesin ini sebagai solusi pengujian yang sangat serbaguna dan diakui secara global. Artinya, dengan satu perangkat, Anda dapat memvalidasi produk Anda untuk pasar Eropa, memenuhi persyaratan klien internasional yang ketat, dan menerapkan protokol jaminan kualitas internal berbasis ISO. Mesin ini bekerja dengan membengkokkan sampel material seperti sol, karet, atau PU pada sudut 90 derajat secara terus-menerus dengan kecepatan tinggi untuk mensimulasikan keausan yang dipercepat, memungkinkan Anda mengamati inisiasi dan perambatan retak secara detail.
Dirancang untuk efisiensi dan keandalan, mesin ini memiliki kapasitas untuk menguji tiga buah sol secara bersamaan, meningkatkan throughput di lingkungan laboratorium yang sibuk. Proses pengujian berjalan pada kecepatan tinggi antara 125 hingga 150 siklus per menit, mempercepat perolehan hasil uji kelelahan material secara signifikan. Setiap siklus dicatat secara akurat oleh penghitung digital LCD yang mampu merekam hingga 999,999 siklus, ideal untuk pengujian daya tahan jangka panjang. Semua parameter pengujian, mulai dari sudut, diameter poros, hingga kecepatan, dirancang secara presisi untuk memenuhi spesifikasi ketat yang diuraikan dalam standar-standar internasional tersebut.
Dengan konstruksi yang kokoh dan bobot 98 Kg, mesin ini menjamin stabilitas operasional untuk hasil yang konsisten dan dapat diulang. Desainnya yang tertutup memastikan keamanan selama operasi kecepatan tinggi. Mengintegrasikan alat uji kelenturan sol ini ke dalam proses R&D material dan kontrol kualitas produksi Anda adalah langkah strategis. Ini tidak hanya mencegah kegagalan produk di tangan konsumen tetapi juga memberikan bukti kuantitatif bahwa material Anda memenuhi beberapa tolok ukur kualitas yang paling menuntut di dunia, membuka pintu ke pasar baru dan memperkuat reputasi merek Anda sebagai produsen berkualitas tinggi.
The durability of a shoe begins with its foundation: the sole. A cracked or broken sole is not just an aesthetic issue; it is a total functional failure that ends the product's service life. We present a fundamental testing device specifically designed to evaluate the resistance of sole materials to cracking caused by repeated flexing. This machine is a vital instrument for sole manufacturers, rubber compounders, and footwear brands committed to ensuring the most critical component of their products can withstand the stresses of daily use without failure.
The most significant advantage of this tester is its compliance with a suite of the most respected international design standards: EN344, SATRA TM161, and ISO 17707. This multi-standard compliance makes this machine a highly versatile and globally recognized testing solution. It means that with a single device, you can validate your products for the European market, meet stringent international client requirements, and implement ISO-based internal quality assurance protocols. The machine works by continuously bending material samples like soles, rubber, or PU at a 90-degree angle at high speed to simulate accelerated wear, allowing you to observe crack initiation and propagation in detail.
Engineered for efficiency and reliability, this machine has the capacity to test three soles simultaneously, increasing throughput in a busy laboratory environment. The testing process runs at a high speed of 125 to 150 cycles per minute, significantly accelerating the acquisition of material fatigue test results. Every cycle is accurately recorded by an LCD digital counter capable of logging up to 999,999 cycles, ideal for long-term endurance testing. All testing parameters, from the angle and shaft diameter to the speed, are precisely designed to meet the strict specifications outlined in these international standards.
With its robust construction and a weight of 98 Kg, the machine guarantees operational stability for consistent and repeatable results. Its enclosed design ensures safety during high-speed operation. Integrating this sole flexing tester into your material R&D and production quality control is a strategic move. It not only prevents product failures in the hands of the consumer but also provides quantitative proof that your materials meet some of the world's most demanding quality benchmarks, opening doors to new markets and cementing your brand's reputation for high quality.

