Dalam ilmu material karet dan plastik, penambahan karbon hitam (carbon black) adalah kunci untuk mencapai kekuatan mekanis, daya tahan, dan performa yang diinginkan. Namun, potensi penuh dari karbon hitam hanya dapat terwujud jika ia terdispersi secara merata dan sempurna di seluruh matriks polimer. Gumpalan atau aglomerat yang tidak terdispersi bertindak sebagai titik lemah, yang secara drastis menurunkan kualitas produk akhir. Kami mempersembahkan sebuah sistem analisis canggih yang bergerak melampaui inspeksi visual tradisional. Alat ini dirancang untuk menentukan tingkat dispersi karbon hitam secara kuantitatif dan objektif, memberikan Anda data yang Anda butuhkan untuk menyempurnakan proses pencampuran (mixing) Anda.
Sistem ini bekerja dengan menggabungkan optik presisi dengan perangkat lunak analisis gambar yang kuat. Sampel kompon ditempatkan pada platform pengukuran dan diterangi oleh cahaya dari sudut 30 derajat untuk menonjolkan kontras. Gambar kemudian ditangkap oleh lensa kamera CCD dengan perbesaran 100x, yang mampu mendeteksi aglomerat mikro yang tidak mungkin dievaluasi secara akurat dengan mata telanjang. Data gambar ini kemudian langsung dianalisis oleh komputer menggunakan metode analisis bi-level dan analisis diameter piksel. Hasilnya bukanlah opini subjektif, melainkan data numerik yang jelas tentang distribusi dan jumlah aglomerat, yang memungkinkan perbandingan kualitas antar batch secara konsisten.
Dibangun sebagai solusi laboratorium yang lengkap, sistem ini mencakup unit detektor gambar presisi yang terhubung dengan komputer yang telah dilengkapi perangkat lunak analisis gambar dan konverter khusus. Ini adalah solusi siap pakai yang memungkinkan Anda untuk segera mengimplementasikan protokol kontrol kualitas yang lebih canggih. Dengan menyediakan data kuantitatif tentang efektivitas proses pencampuran Anda, alat ini memungkinkan para insinyur proses untuk mengoptimalkan parameter seperti waktu, suhu, dan kecepatan rotor untuk mencapai tingkat dispersi terbaik dengan efisiensi maksimum.
Aplikasi alat ini sangat penting bagi setiap industri yang bergantung pada kompon karet dan plastik yang diperkuat. Ini termasuk produsen ban, selang industri, segel (seals) dan gasket, sabuk konveyor, insulasi kabel, serta produsen masterbatch hitam yang harus menjamin konsistensi produk mereka. Berinvestasi dalam sistem analisis dispersi ini berarti berinvestasi dalam keunggulan produk. Ini adalah alat esensial untuk mengurangi tingkat produk gagal, meningkatkan sifat mekanis produk, dan memastikan bahwa setiap batch kompon yang Anda produksi memenuhi spesifikasi kualitas yang paling ketat.
In the science of rubber and plastic materials, the addition of carbon black is key to achieving desired mechanical strength, durability, and performance. However, the full potential of carbon black is only realized when it is perfectly and evenly dispersed throughout the polymer matrix. Undispersed clumps, or agglomerates, act as weak points, drastically compromising the quality of the final product. We present an advanced analysis system that moves beyond traditional visual inspection. This instrument is designed to quantitatively and objectively determine the degree of carbon black dispersion, giving you the data you need to perfect your mixing process.
This system works by combining precision optics with powerful image analysis software. A compound specimen is placed on the measuring platform and illuminated by 30-degree angled light to enhance contrast. The image is then captured by a 100x magnification CCD camera lens, capable of detecting micro-agglomerates that are impossible to accurately evaluate with the naked eye. This image data is then directly processed by the computer using bi-level analysis and pixel diameter analysis methods. The result is not a subjective opinion, but clear numerical data on the distribution and count of agglomerates, allowing for consistent batch-to-batch quality comparisons.
Engineered as a complete laboratory solution, the system includes the precision image detector unit connected to a computer pre-installed with specialized image converter and analysis software. It is a turnkey solution that allows you to immediately implement a more sophisticated quality control protocol. By providing quantitative data on the effectiveness of your mixing process, this tool enables process engineers to optimize parameters such as time, temperature, and rotor speed to achieve the best possible dispersion with maximum efficiency.
The application for this instrument is critical for any industry that relies on reinforced rubber and plastic compounds. This includes manufacturers of tires, industrial hoses, seals and gaskets, conveyor belts, cable insulation, and producers of black masterbatch who must guarantee the consistency of their product. Investing in this dispersion analysis system means investing in product excellence. It is an essential tool for reducing scrap rates, improving the mechanical properties of your products, and ensuring that every batch of compound you produce meets the strictest quality specifications.

