Untuk melampaui standar dan menjadi pemimpin dalam inovasi kemasan, Anda memerlukan data yang lebih dalam daripada sekadar nilai lulus/gagal. Anda memerlukan presisi, kontrol, dan kemampuan analisis tingkat lanjut. Kami mempersembahkan Computer Control Box Compression Tester, sebuah sistem pengujian canggih yang dirancang untuk riset dan pengembangan serta kontrol kualitas yang paling menuntut. Ditenagai oleh sistem penggerak servo, alat ini memberikan tingkat akurasi dan repetabilitas yang tak tertandingi, memungkinkan Anda untuk benar-benar memahami perilaku struktural kemasan Anda di bawah tekanan.
Perbedaan fundamental terletak pada jantung mesin ini: sistem penggerak motor servo dan precision ball screw. Teknologi ini memberikan kontrol yang sangat halus dan akurat atas kecepatan dan posisi penekanan, jauh melampaui sistem konvensional. Dengan rentang kecepatan yang sangat lebar (mulai dari 0.5 mm/menit), Anda dapat melakukan pengujian kompleks seperti uji laju deformasi konstan, uji siklik, atau uji tahan beban (load holding) untuk mensimulasikan kondisi penumpukan di gudang dalam jangka waktu lama. Seluruh proses pengujian dikendalikan oleh komputer, memungkinkan pemrograman siklus tes yang rumit, akuisisi data real-time beresolusi tinggi, dan analisis mendalam.
Setiap spesifikasi dirancang untuk performa puncak. Dengan resolusi yang sangat tinggi mencapai 1/250,000, mesin ini mampu mendeteksi fluktuasi kekuatan sekecil apa pun, memberikan wawasan berharga untuk optimasi material dan desain. Ruang uji yang besar dan dapat disesuaikan memberikan fleksibilitas untuk menguji berbagai macam ukuran dan bentuk kontainer. Sistem keamanan yang komprehensif, termasuk proteksi langkah dan gaya, serta sensor yang mendeteksi kerusakan spesimen, memastikan operasi yang aman bagi pengguna dan melindungi instrumen dari kerusakan.
Instrumen ini adalah pilihan utama bagi departemen R&D, laboratorium universitas, dan fasilitas jaminan kualitas yang bertujuan untuk mengoptimalkan penggunaan material, mengurangi biaya tanpa mengorbankan keamanan, dan mengembangkan desain kemasan generasi berikutnya. Dengan data presisi tinggi dari sistem uji tekan berbasis servo ini, Anda tidak hanya memverifikasi kekuatan—Anda mendorong inovasi.
To move beyond standard compliance and become a leader in packaging innovation, you need deeper data than just a pass/fail value. You need precision, control, and advanced analytical capabilities. We present the Computer Control Box Compression Tester, a state-of-the-art testing system designed for the most demanding research and development and quality control applications. Powered by a servo drive system, this machine delivers an unparalleled level of accuracy and repeatability, allowing you to truly understand the structural behavior of your packaging under stress.
The fundamental difference lies at the heart of this machine: its servo motor and precision ball screw drive system. This technology provides exceptionally smooth and accurate control over speed and position, far surpassing conventional systems. With an extremely wide speed range (starting from 0.5 mm/min), you can perform complex tests like constant deformation rate tests, cyclic tests, or load-holding tests to simulate long-term warehouse stacking conditions. The entire test process is computer-controlled, enabling the programming of intricate test cycles, high-resolution real-time data acquisition, and in-depth analysis.
Every specification is engineered for peak performance. With an ultra-high resolution of 1/250,000, the machine can detect the slightest fluctuations in strength, providing invaluable insights for material and design optimization. The large, customizable test space offers the flexibility to test a vast range of container sizes and shapes. A comprehensive safety system, including stroke and force protection, as well as a sensor that detects specimen destruction, ensures safe operation for the user and protects the instrument from damage.
This instrument is the premier choice for R&D departments, university laboratories, and quality assurance facilities aiming to optimize material usage, reduce costs without sacrificing safety, and develop next-generation packaging designs. With high-precision data from this servo-driven compression test system, you are not just verifying strength—you are driving innovation.

