Kekuatan sebuah material lembaran tidak hanya ditentukan oleh kemampuannya menahan tarikan pada satu arah. Di dunia nyata, produk seperti kantong kertas, kotak kemasan, kain, dan kulit menghadapi tekanan dan benturan dari berbagai arah. Bursting strength atau kekuatan letup adalah ukuran pamungkas dari ketahanan multidireksional ini. Kami mempersembahkan Fully Automatic Bursting Tester, sebuah instrumen presisi yang dirancang untuk secara cepat, mudah, dan akurat menentukan titik di mana material Anda akan pecah di bawah tekanan hidrolik yang terkontrol.
Keunggulan utama dari mesin ini adalah operasinya yang sepenuhnya otomatis. Operator cukup memasang sampel dan menekan tombol start; mesin akan secara otomatis menjepit sampel dengan kekuatan pneumatik yang kuat dan konsisten, memberikan tekanan hidrolik pada kecepatan yang terstandarisasi, mendeteksi titik letup secara instan, dan mencatat nilai tekanan puncak. Otomatisasi ini secara drastis mengurangi waktu pengujian dan, yang terpenting, menghilangkan variabilitas akibat kesalahan operator, memastikan setiap hasil uji sangat konsisten dan dapat diulang. Dengan akurasi tinggi ±0.5% dari skala penuh, Anda dapat mempercayai data yang dihasilkan untuk keputusan kontrol kualitas yang paling kritis.
Instrumen ini adalah solusi serbaguna yang luar biasa, dirancang untuk memenuhi puluhan standar desain internasional dari berbagai industri. Baik Anda perlu mematuhi standar TAPPI dan ISO untuk industri kertas dan kemasan, standar ASTM untuk kulit, atau standar JIS untuk tekstil, mesin ini siap melakukannya. Rentang tekanannya yang sangat lebar, dari 250 hingga 5600 kPa, memungkinkannya untuk menguji berbagai macam material, mulai dari kertas tipis dan kain ringan hingga papan karton gelombang (corrugated board) yang paling kuat sekalipun.
Aplikasi dari alat uji ini sangat luas, menjadikannya aset berharga bagi laboratorium quality control di industri kertas, papan, dan kemasan bergelombang untuk menentukan spesifikasi dan kualitas. Selain itu, alat ini juga esensial bagi industri tekstil (untuk kain rajut dan non-anyaman), kulit dan kulit sintetis (rexine), serta material teknis seperti kain filter. Tingkatkan efisiensi laboratorium Anda dan perluas kemampuan pengujian Anda dengan satu instrumen otomatis, akurat, dan serbaguna ini.
The strength of a sheet material is not just determined by its ability to resist a pull in one direction. In the real world, products like paper sacks, packing boxes, fabrics, and leather face pressure and impacts from multiple directions. Bursting strength is the ultimate measure of this multidirectional resistance. We present the Fully Automatic Bursting Tester, a precision instrument designed to quickly, easily, and accurately determine the point at which your material will rupture under controlled hydraulic pressure.
The key advantage of this machine is its fully automatic operation. The operator simply inserts a sample and presses start; the machine will automatically clamp the sample with a powerful and consistent pneumatic force, apply hydraulic pressure at a standardized rate, instantly detect the bursting point, and record the peak pressure value. This automation drastically reduces testing time and, most importantly, eliminates variability from operator error, ensuring every test result is highly consistent and repeatable. With a high accuracy of ±0.5% of full scale, you can trust the data for your most critical quality control decisions.
This instrument is an incredibly versatile solution, designed to meet dozens of international design standards from various industries. Whether you need to comply with TAPPI and ISO standards for the paper and packaging industry, ASTM standards for leather, or JIS standards for textiles, this machine is ready. Its extremely wide pressure range, from 250 to 5600 kPa, allows it to test a vast array of materials, from thin paper and light fabrics to the strongest corrugated board.
The applications for this tester are extensive, making it a valuable asset for quality control labs in the paper, board, and corrugated packaging industries to determine grade and quality. Furthermore, it is essential for the textile (for knits and nonwovens), leather and synthetic leather (rexine), and technical materials (like filter cloth) industries. Improve your lab's efficiency and expand your testing capabilities with this single automatic, accurate, and versatile instrument.

