Untuk merekayasa kemasan yang tangguh, Anda memerlukan data dari simulasi jatuh yang paling akurat. Kunci dari akurasi ini adalah memastikan spesimen uji mengalami kondisi jatuh bebas (free-fall) yang murni, tanpa gesekan atau gangguan dari mekanisme pelepasan. Kami mempersembahkan Double Wings Drop Testing Machine, sebuah instrumen canggih yang menggunakan mekanisme "sayap ganda" untuk memastikan jatuhan yang paling bersih dan presisi, memberikan Anda data yang paling dapat diandalkan untuk validasi kemasan Anda.
Keunggulan dari mesin ini terletak pada struktur pelepasannya yang canggih. Spesimen ditempatkan di atas platform yang terdiri dari dua "sayap". Saat pengujian dimulai, kedua sayap ini secara simultan dan cepat berayun ke bawah dan ke samping, menjauh dari jalur jatuhan spesimen. Gerakan ini memastikan tidak ada kontak sekunder yang dapat menyebabkan rotasi atau hambatan yang tidak diinginkan, sehingga spesimen jatuh secara sempurna baik untuk pengujian permukaan datar, sisi (edge), maupun sudut (corner). Pengujian ini dilakukan sesuai dengan standar industri global yang esensial seperti ISO 2248, JIS Z0202, dan GB 4757.
Dengan kemampuan untuk mengangkat dan menjatuhkan paket dengan berat hingga 65 kg dari ketinggian yang dapat disesuaikan dari 400 hingga 1500 mm, mesin ini dapat mensimulasikan berbagai skenario penanganan dan kecelakaan dalam rantai pasok. Konstruksinya yang sangat kokoh dengan berat 500 kg menyediakan fondasi yang stabil, memastikan semua energi tumbukan terfokus pada kemasan uji untuk menghasilkan data yang akurat. Penggerak motor untuk mengangkat spesimen dan mekanisme pelepasan yang presisi menjamin setiap pengujian dapat diulang dengan konsistensi yang tinggi.
Ini adalah alat pilihan bagi para insinyur kemasan dan manajer jaminan kualitas yang tidak mau berkompromi pada akurasi. Sangat ideal untuk menguji produk bernilai tinggi atau rapuh seperti barang elektronik, peralatan medis, dan komponen industri, di mana data yang akurat sangat penting untuk merancang solusi pengemasan yang optimal. Dapatkan keyakinan tertinggi dalam desain kemasan Anda dengan data yang dihasilkan dari simulasi jatuh yang paling murni dan terkontrol.
To engineer robust packaging, you need data from the most accurate drop simulations. The key to this accuracy is ensuring the test specimen experiences a true, unobstructed free-fall, without any friction or interference from the release mechanism. We present the Double Wings Drop Testing Machine, an advanced instrument that utilizes a "double wings" mechanism to ensure the cleanest, most precise drop, providing you with the most reliable data for your packaging validation.
The superiority of this machine lies in its advanced release structure. The specimen is placed upon a platform comprised of two "wings". Upon test initiation, these two wings simultaneously and rapidly swing downwards and outwards, clearing the specimen's drop path. This movement ensures there is no secondary contact that could cause unwanted rotation or drag, allowing the specimen to fall perfectly for flat surface, edge, and corner tests. These tests are performed in accordance with essential global industry standards like ISO 2248, JIS Z0202, and GB 4757.
With the ability to lift and drop packages weighing up to 65 kg from an adjustable height of 400 to 1500 mm, this machine can simulate a wide range of handling and accident scenarios in the supply chain. Its extremely robust 500 kg construction provides a stable foundation, ensuring all impact energy is focused on the test package for accurate data generation. A motor-driven lift and precision release mechanism guarantee that every test is repeatable with high consistency.
This is the instrument of choice for packaging engineers and quality assurance managers who demand uncompromising accuracy. It is ideal for testing high-value or fragile products such as electronics, medical devices, and industrial components, where precise data is crucial for designing optimal packaging solutions. Gain the highest confidence in your packaging designs with data generated from the purest, most controlled drop simulations.

