Hadirkan solusi pengujian ketahanan luntur warna yang praktis, andal, dan ekonomis ke dalam laboratorium Anda. Manual Rubbing Fastness Tester ini adalah instrumen fundamental yang dirancang khusus untuk mengukur tingkat transfer warna pada berbagai material seperti katun, serat kimia, kain campuran, dan kulit yang diwarnai. Alat ini merupakan pilihan ideal untuk melakukan pengujian standar AATCC secara akurat tanpa memerlukan sumber daya listrik, memberikan fleksibilitas pengujian di mana saja.
Pengoperasian alat ini sangat sederhana dan efisien. Dengan gerakan resiprokal manual, pengguna dapat dengan mudah mengaplikasikan gesekan pada sampel uji. Meskipun dioperasikan secara manual, setiap aspek pengujian tetap terkontrol dengan ketat untuk hasil yang valid. Tekanan kepala gesek (friction head) distandarisasi pada 9N, memastikan tekanan yang konsisten sesuai persyaratan industri. Sebuah penghitung mekanis terintegrasi secara akurat mencatat setiap putaran dari 1 hingga 99.999 kali, memastikan jumlah siklus gesekan selalu tepat.
Fleksibilitas adalah salah satu keunggulan utama dari alat ini. Dilengkapi dengan pilihan kepala gesek, termasuk bentuk bulat berdiameter 16mm dan persegi panjang 19x25mm, instrumen ini dapat beradaptasi dengan berbagai jenis pengujian dan sampel. Didesain untuk memenuhi standar industri seperti AATCC (dengan panjang langkah 105mm) dan GB (100mm), alat ini memastikan hasil pengujian Anda dapat dipertanggungjawabkan. Dengan bobot hanya 3kg, alat ini sangat portabel dan sempurna untuk laboratorium dengan ruang terbatas atau untuk keperluan pengujian di berbagai lokasi.
Jadikan instrumen ini sebagai investasi cerdas untuk fondasi quality control Anda. Alat Uji Gesek Manual ini adalah pilihan sempurna untuk institusi pendidikan, laboratorium skala kecil hingga menengah, atau sebagai alat pendukung di fasilitas pengujian besar. Ini adalah cara yang paling efektif untuk memastikan produk Anda memenuhi standar ketahanan luntur warna, mencegah keluhan pelanggan, dan membangun kepercayaan pada merek Anda dengan cara yang paling efisien.
Introduce a practical, reliable, and economical color fastness testing solution into your laboratory. This Manual Rubbing Fastness Tester is a fundamental instrument specifically designed to measure the degree of color transfer on a wide range of materials, including cotton, chemical fiber, blended fabrics, and dyed leather. It stands as the ideal choice for accurately performing AATCC standard tests without the need for an electrical power source, providing ultimate testing flexibility anywhere.
The operation of this device is incredibly simple and efficient. Through a manual reciprocating stroke, the user can easily apply friction to the test specimen. Although manually operated, every aspect of the test remains strictly controlled for valid results. The friction head pressure is standardized at 9N, ensuring consistent pressure that meets industry requirements. An integrated mechanical counter accurately tracks every cycle from 1 to 99,999, guaranteeing the number of rubbing strokes is always precise.
Versatility is a key advantage of this instrument. Equipped with multiple friction head options, including a 16mm round head and a 19x25mm rectangular one, the device can adapt to various test types and samples. Designed to comply with industry standards like AATCC (with a 105mm stroke length) and GB (100mm), this tester ensures your results are accountable. Weighing just 3kg, the instrument is exceptionally portable and perfect for laboratories with limited space or for testing purposes across different locations.
Make this instrument a smart investment for your quality control foundation. This Manual Rubbing Fastness Tester is the perfect choice for educational institutions, small to medium-sized labs, or as a supplementary tool in larger testing facilities. It is the most effective way to ensure your products meet color fastness standards, prevent customer complaints, and build confidence in your brand in the most efficient manner.

