Ukur dan validasi daya tahan produk Anda dengan Taber Abrasion Tester, instrumen yang diakui secara global untuk pengujian ketahanan aus. Alat ini sangat serbaguna, dirancang untuk mengevaluasi ketahanan abrasi pada berbagai macam material, termasuk kulit, kain, cat, pelapis kertas, lantai, kayu lapis, kaca, hingga karet alam. Bagi departemen riset & pengembangan dan quality control, mesin ini adalah alat fundamental untuk memastikan sebuah produk dapat menahan goresan, gesekan, dan keausan dalam penggunaan nyata.
Mesin ini menggunakan metode pengujian Taber yang khas dan terpercaya. Sampel material ditempatkan pada platform yang berputar (turntable) dengan kecepatan konstan 60 RPM. Dua roda gerinda (grinding wheels) standar dengan beban yang dapat diatur diturunkan ke permukaan sampel. Saat platform berputar, roda gerinda menciptakan pola keausan berbentuk "X" yang unik, menyimulasikan kerusakan akibat gesekan dari berbagai arah. Hasilnya kemudian dapat dievaluasi secara visual atau dengan mengukur kehilangan massa untuk mendapatkan data kuantitatif yang presisi.
Dirancang untuk presisi dan fleksibilitas, alat ini memungkinkan penyesuaian beban uji (250g, 500g, 1000g) dan kompatibel dengan berbagai model roda gerinda standar industri (seperti H18, CS10, CS17, dll.), memastikan Anda dapat memenuhi spesifikasi dari berbagai metode pengujian internasional. Panel kontrol digitalnya memungkinkan Anda untuk mengatur jumlah putaran yang diinginkan hingga 999.999 kali, dengan fitur mati otomatis yang efisien, sehingga pengujian dapat berjalan secara mandiri hingga selesai.
Berinvestasi pada Taber Abrasion Tester berarti berinvestasi pada jaminan kualitas dan durabilitas produk Anda. Instrumen ini sangat penting untuk mengembangkan pelapis yang tahan lama, lantai yang kuat, produk kulit premium, dan material lainnya yang unggul dalam ketahanannya. Pastikan produk Anda tidak hanya terlihat bagus tetapi juga terbukti tangguh. Dapatkan data yang Anda butuhkan untuk membuktikan superioritas produk Anda dan membangun kepercayaan pelanggan yang tak tergoyahkan.
Measure and validate the durability of your products with the Taber Abrasion Tester, a globally recognized instrument for wear resistance testing. This highly versatile machine is designed to evaluate the abrasion resistance of an extensive range of materials, including leather, cloth, paint, paper coatings, flooring, plywood, glass, and natural rubber. For any research & development and quality control department, this is the fundamental tool for ensuring a product can withstand scratching, rubbing, and wear in real-world applications.
This machine employs the distinctive and trusted Taber testing method. A material specimen is placed on a rotating turntable that operates at a constant speed of 60 RPM. Two standardized grinding wheels with adjustable loads are lowered onto the specimen's surface. As the platform rotates, the wheels create a unique "X" pattern of wear, simulating damage from friction from various angles. The results can then be evaluated visually or by measuring mass loss to obtain precise quantitative data.
Engineered for precision and flexibility, this device allows for adjustable test loads (250g, 500g, 1000g) and is compatible with a wide variety of industry-standard grinding wheel models (such as H18, CS10, CS17, etc.), ensuring you can meet the specifications of numerous international test methods. Its digital control panel lets you preset the desired number of rotations up to 999,999, with an efficient automatic shut-down feature, allowing tests to run unattended until completion.
Investing in a Taber Abrasion Tester means investing in the quality assurance and durability of your products. This instrument is essential for developing long-lasting coatings, resilient flooring, premium leather goods, and other materials that excel in their robustness. Ensure your products don't just look good but are proven to be tough. Get the data you need to prove your product's superiority and build unshakeable customer confidence.

