Tingkatkan akurasi dan keandalan setiap pengukuran viskositas Anda dengan Specialized Thermostatic Bath kami. Instrumen ini adalah aksesori pendukung yang krusial dan dirancang khusus untuk digunakan bersama rotational viscometer. Mengingat sifat viskositas yang sangat sensitif terhadap perubahan suhu, alat ini memainkan peran vital dalam menjaga temperatur sampel agar tetap konstan dan stabil selama pengujian. Tanpa kontrol suhu yang presisi, hasil pengukuran viskositas bisa menjadi tidak valid dan sulit direproduksi.
Dibangun untuk performa tingkat tinggi, thermostatic bath ini dilengkapi dengan sistem kontrol mikrokomputer dan penyesuaian PID yang canggih. Teknologi ini mampu mencapai stabilitas suhu yang luar biasa dengan fluktuasi serendah ±0.05°C, memastikan sampel Anda berada dalam kondisi termal yang ideal. Dengan beragam model yang menawarkan rentang temperatur operasional yang sangat luas, mulai dari suhu ruang hingga 300°C, alat ini dapat menggunakan air maupun berbagai jenis minyak silikon sebagai media pemanas untuk memenuhi berbagai kebutuhan pengujian Anda.
Dirancang dengan mempertimbangkan kemudahan alur kerja di laboratorium, alat ini memiliki bukaan melingkar khusus pada bagian atas yang pas untuk menempatkan beaker berukuran 200 ml secara langsung. Fitur ini memungkinkan pengukuran viskositas dilakukan dengan praktis dan efisien. Selain itu, fungsi sirkulasi dengan pompa yang alirannya dapat diatur (adjustable pump flow) memberikan fleksibilitas tambahan, baik untuk menjaga keseragaman suhu di dalam bak maupun untuk mensirkulasikan cairan ke wadah eksternal seperti thermostatic cup.
Berinvestasi dalam thermostatic bath ini adalah langkah esensial untuk memaksimalkan potensi viskometer Anda dan memvalidasi data pengujian Anda. Dengan mengeliminasi variabel temperatur sebagai sumber kesalahan, Anda dapat memperoleh hasil pengukuran viskositas yang benar-benar akurat, konsisten, dan dapat diandalkan. Pastikan setiap produk Anda memenuhi standar kualitas reologi yang ketat dengan menambahkan instrumen kontrol suhu presisi ini ke dalam perlengkapan laboratorium Anda.
Enhance the accuracy and reliability of every viscosity measurement with our Specialized Thermostatic Bath. This instrument is a crucial support accessory specifically designed for use with a rotational viscometer. Given that viscosity is highly sensitive to temperature changes, this bath plays a vital role in maintaining a constant and stable sample temperature throughout the testing process. Without precise temperature control, viscosity readings can become invalid and difficult to reproduce.
Engineered for high-level performance, this thermostatic bath is equipped with a microcomputer control system and advanced PID adjustment. This technology is capable of achieving exceptional temperature stability with fluctuations as low as ±0.05°C, ensuring your sample is kept in the ideal thermal condition. With various models offering an extremely wide operational temperature range, from room temperature up to 300°C, this device can utilize water or different types of silicone oil as the heating medium to meet your diverse testing requirements.
Designed with laboratory workflow convenience in mind, this device features a special circular opening on top that perfectly accommodates a 200 ml beaker directly. This feature allows for practical and efficient viscosity measurements. Furthermore, the circulation function with an adjustable pump flow provides added flexibility, whether for maintaining temperature uniformity within the bath itself or for circulating the liquid to an external vessel like a thermostatic cup.
Investing in this thermostatic bath is an essential step to maximize your viscometer's potential and validate your testing data. By eliminating temperature variation as a source of error, you can obtain viscosity measurement results that are truly accurate, consistent, and reliable. Ensure every one of your products meets stringent rheological quality standards by adding this precision temperature control instrument to your laboratory setup.

