Pastikan keamanan dan kualitas produk gas minyak cair (LPG) Anda dengan Apparatus Penentuan Tekanan Uap kami. Instrumen laboratorium yang sangat terspesialisasi ini dirancang secara eksklusif untuk melakukan pengujian tekanan uap gage pada produk gas petroleum cair, sesuai dengan metodologi standar internasional ASTM D1267. Pengujian ini merupakan parameter quality control yang krusial untuk memastikan LPG memenuhi spesifikasi yang tepat untuk penyimpanan, transportasi, dan penggunaan akhir yang aman.
Presisi dan kinerja yang andal adalah inti dari desain alat ini. Dilengkapi dengan kontroler suhu digital, instrumen ini mampu menjaga suhu bak pemanas (water bath) dengan presisi luar biasa hingga ±0.1°C dalam rentang suhu operasional dari suhu ruang hingga 90°C. Untuk menjamin pemanasan yang merata dan seragam pada sampel, sistem ini menggunakan sirkulasi pump loop yang mengaduk media pemanas secara konstan dan senyap. Hal ini memastikan kedua tabung uji (testing bombs) menerima perlakuan termal yang identik, sebuah syarat mutlak untuk hasil pengujian yang valid.
Keselamatan dan efisiensi adalah prioritas utama, terutama saat bekerja dengan material yang mudah terbakar seperti LPG. Oleh karena itu, output pemanas alat ini dikendalikan oleh solid-state relay (SSR) yang canggih, memberikan operasi yang contactless (tanpa sentuh), sparkless (tanpa percikan api), dan noiseless (tanpa suara), sehingga secara signifikan meningkatkan keamanan di laboratorium. Lebih lanjut, dengan kapasitas untuk memproses dua sampel secara bersamaan menggunakan dua tabung uji, alat ini mampu meningkatkan produktivitas dan efisiensi alur kerja pengujian Anda.
Dibangun untuk penggunaan jangka panjang, elemen pemanas terbuat dari material stainless steel yang tahan lama dan memiliki laju pemanasan yang cepat. Desain keseluruhan yang rasional tidak hanya memberikan tampilan yang menarik tetapi juga memastikan pengoperasian yang mudah dan intuitif melalui panel kontrol digital yang fleksibel. Jadikan alat uji ini sebagai andalan di laboratorium Anda untuk pengujian tekanan uap LPG yang aman, efisien, dan sangat akurat.
Ensure the safety and quality of your liquefied petroleum gas (LPG) products with our Apparatus for Vapor Pressure Determination. This highly specialized laboratory instrument is exclusively designed to perform the gage vapor pressure test on liquefied petroleum gas products, in full conformity with the ASTM D1267 international standard methodology. This test is a crucial quality control parameter to ensure that LPG meets the precise specifications for safe storage, transportation, and end-use.
Precision and reliable performance are at the core of this apparatus's design. Equipped with a digital temperature controller, the instrument is capable of maintaining the heating bath's temperature with outstanding precision of ±0.1°C within an operating range from room temperature up to 90°C. To guarantee even and uniform heating of the samples, the system utilizes a pump loop circulation to stir the heating medium constantly and noiselessly. This ensures that both testing bombs receive identical thermal treatment, an absolute requirement for valid test results.
Safety and efficiency are top priorities, especially when working with flammable materials like LPG. Therefore, the heating output is controlled by an advanced solid-state relay (SSR), providing contactless, sparkless, and noiseless operation, which significantly enhances safety in the laboratory. Furthermore, with the capacity to process two samples simultaneously using two testing bombs, this apparatus is able to improve the productivity and efficiency of your testing workflow.
Built for long-term use, the heating element is made from durable stainless steel material with a fast heating rate. The overall rational design not only provides an attractive appearance but also ensures easy and intuitive operation via the flexible digital control panel. Make this testing apparatus a staple in your laboratory for safe, efficient, and highly accurate LPG vapor pressure testing.

