Tingkatkan standar pengujian biodiesel Anda dengan Automatic Oxidation Stability Apparatus kami, sebuah instrumen laboratorium canggih yang dirancang untuk otomatisasi penuh. Alat ini secara spesifik berfungsi untuk menentukan stabilitas oksidasi dari Fatty Acid Methyl Esters (FAME) atau Biodiesel, sebuah parameter krusial untuk memprediksi masa simpan dan memastikan kualitas produk. Dirancang untuk beroperasi sesuai standar internasional EN 14112, instrumen ini adalah solusi esensial bagi produsen biofuel, kilang minyak, dan laboratorium pengujian untuk menjamin produk biodiesel memenuhi spesifikasi global.
Presisi dalam pengujian dijamin melalui serangkaian komponen berteknologi tinggi. Sistem ini menggunakan kontroler temperatur digital PID impor yang mampu menjaga suhu kerja (hingga 150°C) dengan akurasi dan stabilitas luar biasa, yaitu ±0.1°C. Aliran udara, sebagai elemen kunci dalam uji oksidasi dipercepat, diatur oleh pompa diafragma khusus dan sistem filtrasi udara yang unik. Kombinasi ini memastikan aliran gas yang konstan, terkontrol secara presisi (10L/h), dan bersih, sehingga menghasilkan kondisi pengujian yang ideal dan dapat diulang.
Kecanggihan sesungguhnya terletak pada sistem kontrol dan akuisisi datanya yang sepenuhnya otomatis. Ditenagai oleh PC industrial internal dengan layar liquid crystal yang besar, alat ini mengelola seluruh proses pengujian secara mandiri. Mulai dari mengontrol suhu dan aliran gas, hingga mengukur data konduktivitas secara real-time dan secara otomatis menentukan serta menyimpan hasil induction period. Tampilan grafis dari proses oksidasi dan kurva konduktivitas secara langsung pada layar memudahkan analisis dan mengurangi beban kerja operator secara signifikan.
Efisiensi laboratorium Anda akan meningkat drastis berkat desain dua stasiun kerja (dual work stations). Fitur ini memungkinkan Anda untuk menguji dua sampel secara paralel dan independen, lengkap dengan sistem kontrol suhu terpisah untuk masing-masing sampel. Kemampuan ini secara efektif menggandakan throughput pengujian Anda. Jadikan alat uji otomatis yang andal ini sebagai investasi utama untuk memastikan kualitas, stabilitas, dan kepatuhan standar dari setiap produk biodiesel yang Anda hasilkan.
Elevate your biodiesel testing standards with our Automatic Oxidation Stability Apparatus, a state-of-the-art laboratory instrument designed for full automation. This apparatus is specifically used to determine the oxidation stability of Fatty Acid Methyl Esters (FAME), or Biodiesel, a crucial parameter for predicting storage life and ensuring product quality. Engineered to operate in strict accordance with the EN 14112 international standard, this instrument is an essential solution for biofuel producers, refineries, and testing labs to guarantee that biodiesel products meet global specifications.
Precision in testing is guaranteed through a series of high-tech components. The system utilizes an imported digital PID temperature controller capable of maintaining the working temperature (up to 150°C) with exceptional accuracy and stability of ±0.1°C. The airflow, a key element in the accelerated oxidation test, is regulated by a dedicated diaphragm pump and a unique air filtration system. This combination ensures a constant, precisely controlled (10L/h), and clean gas flow, resulting in ideal and repeatable testing conditions.
The true sophistication lies in its fully automatic control and data acquisition system. Powered by an internal industrial PC with a large liquid crystal display, the apparatus independently manages the entire testing process. This includes controlling temperature and gas flow, measuring conductivity data in real-time, and automatically determining and storing the induction period results. The graphical display of the oxidation process and the conductivity curve directly on the screen facilitates easy analysis and significantly reduces operator workload.
Your laboratory's efficiency will dramatically increase thanks to the dual work station design. This feature allows you to test two samples in parallel and independently, complete with separate temperature control systems for each sample. This capability effectively doubles your testing throughput. Make this reliable, automatic testing apparatus a key investment to ensure the quality, stability, and standard compliance of every biodiesel product you produce.

