Evaluasi performa krusial dari minyak pelumas dan fluida sintetik Anda dengan Apparatus for Water Separability kami. Instrumen ini dirancang secara spesifik untuk mengukur kemampuan minyak dalam memisahkan diri dari air (dikenal sebagai demulsibility), sebuah karakteristik vital terutama untuk oli turbin uap dan pelumas industri lain yang rentan terhadap kontaminasi air dan turbulensi. Alat ini merupakan solusi definitif untuk spesifikasi produk baru dan pemantauan oli yang sedang digunakan (in-service oil), yang sepenuhnya sesuai dengan metode uji standar internasional ASTM D1401.
Presisi dalam pengujian adalah kunci, dan alat ini dirancang untuk itu. Dilengkapi dengan kontroler suhu digital presisi tinggi, instrumen ini mampu menjaga temperatur bak pemanas (bath) dari suhu ruang hingga 100°C dengan akurasi kontrol yang ketat, yaitu ±0.5°C. Untuk menciptakan kondisi pengujian yang standar dan dapat diulang, alat ini menggunakan dua sistem pengaduk motor (motor agitation) terpisah: satu untuk sirkulasi suhu di dalam bak (1200r/min) dan satu lagi untuk mengaduk sampel minyak dengan kecepatan spesifik (1500r/min), yang didukung oleh sensor suhu Pt100 yang andal.
Dirancang untuk efisiensi dan kemudahan observasi di laboratorium, apparatus ini memiliki desain tiga lubang (three-hole) yang memungkinkan operator untuk melakukan beberapa pengujian secara bersamaan, sehingga secara signifikan meningkatkan produktivitas dan throughput. Penggunaan material bak dari kaca transparan (glass bath) merupakan fitur unggulan yang memfasilitasi pengamatan visual secara langsung terhadap proses pemisahan fasa antara minyak dan air. Pengoperasiannya pun disederhanakan dengan adanya timer digital yang dilengkapi alarm.
Bagi produsen pelumas, pembangkit listrik, dan laboratorium pemeliharaan industri, alat uji water separability ini adalah investasi yang sangat penting. Kemampuan minyak untuk melepaskan air dengan cepat sangat krusial untuk mencegah korosi, keausan dini, dan pembentukan lumpur (sludge) di dalam mesin. Instrumen ini menyediakan data yang andal dan terstandarisasi yang Anda butuhkan untuk menjamin kualitas pelumas, memprediksi masa pakai, dan mencegah kegagalan mesin yang mahal.
Evaluate the crucial performance of your petroleum oils and synthetic fluids with our Apparatus for Water Separability. This instrument is specifically designed to measure the ability of oil to separate from water (known as demulsibility), a vital characteristic especially for steam-turbine oils and other industrial lubricants prone to water contamination and turbulence. This apparatus is the definitive solution for the specification of new products and the monitoring of in-service oils, fully conforming to the ASTM D1401 international standard test method.
Precision in testing is key, and this apparatus is engineered for it. Equipped with a high-precision digital temperature controller, the instrument is capable of maintaining the bath temperature from room temperature up to 100°C with a strict control accuracy of ±0.5°C. To create standardized and repeatable test conditions, the device utilizes two separate motor agitation systems: one for temperature circulation within the bath (1200r/min) and another for stirring the oil sample at a specific speed (1500r/min), supported by a reliable Pt100 temperature sensor.
Designed for efficiency and ease of observation in the laboratory, this apparatus features a three-hole design, allowing the operator to conduct multiple tests simultaneously, thereby significantly increasing productivity and throughput. The use of a transparent glass bath is a standout feature that facilitates direct visual observation of the phase separation process between oil and water. Its operation is further simplified by a digital timer equipped with an alarm.
For lubricant manufacturers, power plants, and industrial maintenance laboratories, this water separability test apparatus is a critical investment. The ability of an oil to shed water quickly is crucial for preventing corrosion, premature wear, and sludge formation within machinery. This instrument provides the reliable, standardized data you need to guarantee lubricant quality, predict its service life, and prevent costly machinery failures.

