Pastikan performa superior dari produk pelumas Anda dengan Foaming Characteristic Apparatus kami. Instrumen laboratorium esensial ini dirancang khusus untuk mengevaluasi karakteristik busa pada minyak pelumas, yaitu mengukur kecenderungan pembentukan busa (foaming tendency) dan stabilitas busa yang terbentuk. Kemampuan oli untuk menahan pembentukan busa sangat krusial untuk mencegah kavitasi pompa, oksidasi, dan hilangnya efektivitas pelumasan. Alat ini dirancang untuk menjalankan pengujian secara akurat sesuai dengan metodologi standar internasional ASTM D892.
Presisi dalam pengujian dijamin melalui sistem kontrol temperatur digital yang canggih. Instrumen ini mampu menjaga dua titik suhu pengujian yang disyaratkan oleh standar, yaitu 24°C dan 93.5°C, dengan tingkat presisi yang tinggi (±0.5°C). Didukung oleh sensor Pt100 yang andal dan motor pengaduk elektrik (1250 turns/min) untuk memastikan keseragaman suhu di seluruh bak, alat ini menciptakan kondisi pengujian yang stabil dan dapat diulang. Selain itu, empat grup flowmeter yang terintegrasi memungkinkan operator untuk mengontrol dan mengamati aliran gas eksperimental dengan mudah.
Dirancang untuk produktivitas laboratorium modern, apparatus ini dilengkapi dengan dua lubang (two-hole design), yang memungkinkan pengujian dua sampel secara paralel dan simultan. Fitur ini secara signifikan meningkatkan efisiensi kerja dan throughput laboratorium Anda. Aspek keselamatan juga menjadi prioritas utama; output pemanas dikendalikan oleh solid-state relay (SSR) yang beroperasi tanpa kontak dan tanpa percikan api (sparkless), memberikan keamanan dan keandalan yang sangat penting saat bekerja dengan minyak yang dipanaskan.
Dengan konstruksi yang kokoh, termasuk elemen pemanas berbahan stainless steel untuk pemanasan cepat dan masa pakai yang panjang, alat ini adalah solusi yang andal dan mudah dioperasikan. Panel kontrol digital yang fleksibel membuat pengaturan pengujian menjadi sederhana. Bagi produsen pelumas, pabrikan mesin, dan laboratorium quality control, instrumen ini merupakan perangkat wajib untuk memastikan produk pelumas memberikan perlindungan maksimal tanpa masalah busa yang dapat merusak.
Ensure the superior performance of your lubricant products with our Foaming Characteristic Apparatus. This essential laboratory instrument is specifically designed to evaluate the foaming characteristics of lubricating oils by empirically rating their foaming tendency and the stability of the foam produced. An oil's ability to resist foaming is crucial for preventing pump cavitation, oxidation, and a loss of lubrication effectiveness. This apparatus is engineered to perform tests in strict accordance with the ASTM D892 international standard method.
Precision in testing is guaranteed through an advanced digital temperature control system. The instrument is capable of maintaining the two standard-required test temperatures, 24°C and 93.5°C, with high precision (±0.5°C). Supported by a reliable Pt100 sensor and an electric motor agitator (1250 turns/min) to ensure uniform bath temperature, this device creates stable and repeatable testing conditions. Furthermore, four integrated groups of flowmeters allow the operator to easily control and observe the flow of the experimental gas.
Designed for the modern, productive laboratory, this apparatus is equipped with a two-hole design, enabling the parallel and simultaneous testing of two samples. This feature significantly improves work efficiency and your lab's throughput. Safety is also a top priority; the heating output is controlled by a solid-state relay (SSR) that operates without contact and is sparkless, providing essential safety and reliability when working with heated oils.
With its robust construction, including a stainless steel heating element for fast heating and a long service life, this apparatus is a reliable and easy-to-operate solution. The flexible digital control panel makes test setup straightforward. For lubricant blenders, engine manufacturers, and quality control laboratories, this instrument is a mandatory device to ensure that lubricant products provide maximum protection without detrimental foaming issues.

