Tentukan kandungan air hingga level renik (trace level) dengan presisi tak tertandingi menggunakan Coulometric Karl Fischer Titrator kami. Instrumen canggih ini adalah solusi definitif untuk mengukur kadar air dalam berbagai sampel, terutama dalam minyak mentah (crude oil) di mana akurasi sangat krusial untuk proses penyulingan, jual-beli, dan transfer. Dirancang untuk beroperasi secara penuh sesuai dengan metode uji standar industri seperti ASTM D4377 dan ASTM D4928, alat ini memberikan data yang andal dan dapat dipertanggungjawabkan.
Dibangun untuk sensitivitas dan akurasi superior, titrator ini mampu mengukur kadar air dalam rentang yang sangat luas, dari 1 ppm hingga 100%, dengan sensitivitas luar biasa hingga 0.1µg. Kinerja tinggi ini dicapai melalui metode titrasi coulometric dengan deteksi polarisasi arus konstan menggunakan elektroda platinum ganda. Sistem cerdasnya secara otomatis mendeteksi dan mengurangi arus blanko (blank current) secara real-time, memastikan setiap hasil pengukuran bersih dari interferensi kelembaban reagen.
Pengoperasian menjadi sangat mudah dan intuitif berkat antarmuka modern yang dikendalikan oleh SCM (Single-Chip Microcomputer). Interaksi pengguna dilakukan melalui layar sentuh LCD berwarna yang ramah pengguna, yang juga menampilkan fungsi diagnosis mandiri. Fitur cerdas lainnya termasuk fungsi kompensasi latar belakang arus besar untuk mempersingkat waktu siaga, dan sistem manajemen reagen yang secara otomatis mengingatkan pengguna saat reagen perlu diganti, memastikan efisiensi dan validitas pengujian setiap saat.
Ini adalah solusi analisis dan pelaporan yang lengkap. Dengan kapasitas penyimpanan internal yang besar, alat ini mampu menyimpan hingga 500 set data hasil pengujian yang dapat dengan mudah diakses kembali untuk keperluan audit atau analisis tren. Selain itu, mini-printer termal berefisiensi tinggi yang terintegrasi memungkinkan Anda untuk mencetak laporan hasil pengujian secara langsung di tempat. Jadikan instrumen ini sebagai andalan laboratorium Anda untuk analisis kadar air yang cepat, akurat, dan terdokumentasi dengan baik.
Determine water content down to trace levels with unparalleled precision using our Coulometric Karl Fischer Titrator. This advanced instrument is the definitive solution for measuring moisture content in a wide variety of samples, especially in crude oil where accuracy is crucial for refining, sales, and transfer processes. Designed to operate in full compliance with industry-standard test methods like ASTM D4377 and ASTM D4928, this apparatus provides reliable and accountable data.
Built for superior sensitivity and accuracy, this titrator is capable of measuring water content over a very wide range, from 1 ppm to 100%, with an exceptional sensitivity of 0.1µg. This high performance is achieved through the coulometric titration method with constant current polarization detection using a double platinum electrode. Its intelligent system automatically detects and deducts the blank current in real-time, ensuring every measurement result is free from reagent moisture interference.
Operation is made incredibly easy and intuitive thanks to a modern interface controlled by an SCM (Single-Chip Microcomputer). User interaction is handled via a friendly, color LCD touch screen, which also displays self-diagnosis functions. Other smart features include a large current background compensation function to shorten standby time, and a reagent management system that automatically reminds the user when it's time to replace the reagent, ensuring efficiency and test validity at all times.
This is a complete analysis and reporting solution. With a large built-in storage capacity, the device can store up to 500 sets of test data, which can be easily retrieved for audit trails or trend analysis. Furthermore, an integrated high-efficiency thermal mini-printer allows you to print test reports directly on-site. Make this instrument a staple in your laboratory for fast, accurate, and well-documented moisture analysis.

