Tentukan kandungan energi dari bahan bakar hidrokarbon cair Anda dengan presisi tertinggi menggunakan Automatic Bomb Calorimeter kami. Instrumen canggih ini dirancang khusus untuk mengukur nilai kalor bruto (gross calorific value) dan nilai kalor netto (net calorific value) dari berbagai produk perminyakan, seperti bensin, bahan bakar jet (avtur), minyak solar, dan minyak bakar. Pengujian ini sangat krusial bagi kilang minyak, pembangkit listrik, dan produsen mesin untuk memverifikasi kualitas dan efisiensi energi bahan bakar, yang sepenuhnya sesuai dengan metode uji standar internasional ASTM D240.
Kinerja superior dan otomatisasi penuh adalah inti dari alat ini. Dilengkapi dengan modul pengumpul temperatur berpresisi tinggi dengan resolusi hingga 0.001°C, instrumen ini secara otomatis menjalankan seluruh alur kerja pengujian: mulai dari mengumpulkan data perubahan suhu, merekam, menghitung, hingga menyimpan hasil secara permanen. Salah satu fitur unggulannya adalah oxygen bomb model baru yang dapat mengisi oksigen secara otomatis, menghilangkan kebutuhan inflasi manual yang merepotkan serta meningkatkan keamanan dan konsistensi pengujian.
Dirancang untuk kemudahan operasional di laboratorium modern, alat ini mengadopsi mode operasi melalui layar sentuh (touched screen) yang intuitif. Antarmuka ini memungkinkan operator untuk dengan mudah mengatur parameter, memantau prosedur pengujian, dan melihat hasil secara visual. Seluruh komponen utama, termasuk bomb, terbuat dari material stainless steel berkualitas tinggi yang tahan tekanan tinggi, anti-korosi, dan mudah dibersihkan, menjamin masa pakai yang panjang dan keandalan dalam setiap pengujian.
Untuk kebutuhan laboratorium dengan throughput tinggi, tersedia opsi dengan teknologi PCI canggih yang memungkinkan satu komputer untuk mengontrol beberapa unit kalorimeter atau instrumen lainnya secara bersamaan. Ini adalah solusi "satu mesin dengan kontrol ganda" yang sangat efisien. Jadikan bomb calorimeter otomatis ini sebagai investasi strategis untuk mendapatkan data nilai kalor yang cepat, akurat, dan sangat dapat diulang dengan intervensi operator yang minimal.
Determine the energy content of your liquid hydrocarbon fuels with the highest precision using our Automatic Bomb Calorimeter. This state-of-the-art instrument is specifically designed to measure the gross and net calorific value of various petroleum products, such as gasoline, jet fuel, diesel oil, and heavy oil. This test is crucial for refineries, power plants, and engine manufacturers to verify fuel quality and energy efficiency, in full compliance with the ASTM D240 international standard test method.
Superior performance and full automation are at the core of this device. Equipped with a high-precision temperature collecting module with a resolution of up to 0.001°C, the instrument automatically executes the entire testing workflow: from collecting temperature change data, recording, calculating, to permanently storing the results. One of its standout features is the novelty oxygen bomb with automatic oxygen filling, which eliminates cumbersome manual inflation and improves both safety and test consistency.
Designed for operational ease in the modern laboratory, this apparatus adopts an intuitive touched screen operation mode. This interface allows the operator to easily set up parameters, monitor the test procedure, and view the results visually. All major components, including the bomb, are made from high-quality stainless steel material that is high-pressure resistant, anti-corrosion, and easy to clean, ensuring a long service life and reliability in every test.
For high-throughput laboratory needs, an option with advanced PCI technology is available, enabling a single computer to control multiple calorimeter units or other instruments simultaneously. This is a highly efficient "one machine with multiple controlling" solution. Make this automatic bomb calorimeter a strategic investment to obtain fast, accurate, and highly repeatable calorific value data with minimal operator intervention.

