Tentukan parameter kualitas paling fundamental dari minyak mentah dan produk perminyakan cair Anda dengan Density Determination Apparatus kami. Instrumen laboratorium esensial ini dirancang untuk melakukan penentuan densitas, densitas relatif (berat jenis), atau gravitasi API secara akurat menggunakan metode hidrometer. Pengujian ini sangat krusial untuk transaksi jual-beli (custody transfer), kontrol proses di kilang, dan spesifikasi kualitas produk. Seluruh prosedur dan desain alat ini sepenuhnya sesuai dengan metode uji standar internasional, ASTM D1298.
Akurasi dalam metode hidrometer sangat bergantung pada kontrol suhu yang presisi. Oleh karena itu, apparatus ini dilengkapi dengan sistem pemanas (bath) dengan kontroler suhu digital presisi tinggi dan sensor Pt100 yang andal. Sistem ini mampu menjaga suhu bak dalam rentang yang luas, dari 20°C hingga 95°C, dengan akurasi yang sangat baik yaitu ±0.2°C. Motor pengaduk (1200r/min) memastikan suhu terdistribusi secara merata ke seluruh media, menciptakan lingkungan termal yang stabil dan ideal untuk pembacaan hidrometer yang akurat sebelum dikoreksi ke suhu standar (15°C atau 60°F).
Dirancang untuk efisiensi dan durabilitas, alat ini memiliki desain dua lubang (two-slot holes), yang memungkinkan operator untuk menguji dua sampel secara bersamaan. Kemampuan untuk melakukan pengujian paralel ini secara signifikan meningkatkan produktivitas dan throughput di laboratorium yang sibuk. Elemen pemanas terbuat dari material stainless steel berkualitas tinggi yang anti-korosi, menjamin masa pakai yang panjang dan kinerja yang andal bahkan dalam penggunaan berkelanjutan.
Dengan pengoperasian yang sederhana dan struktur yang elegan, instrumen ini merupakan alat wajib bagi setiap laboratorium di kilang minyak, terminal penyimpanan, dan lembaga inspeksi pihak ketiga. Dengan menyediakan metode yang terstandarisasi dan mudah untuk salah satu parameter kualitas minyak yang paling dasar namun kritis, alat ini membantu memastikan perdagangan yang adil, kontrol proses yang optimal, dan konsistensi kualitas produk dari waktu ke waktu.
Determine the most fundamental quality parameters of your crude petroleum and liquid petroleum products with our Density Determination Apparatus. This essential laboratory instrument is designed for the accurate determination of density, relative density (specific gravity), or API gravity using the hydrometer method. This test is crucial for custody transfer transactions, refinery process control, and product quality specifications. The entire procedure and apparatus design fully conform to the international standard test method, ASTM D1298.
Accuracy in the hydrometer method is critically dependent on precise temperature control. Therefore, this apparatus is equipped with a heating bath system featuring a high-precision digital temperature controller and a reliable Pt100 sensor. This system is capable of maintaining the bath temperature over a wide range, from 20°C to 95°C, with an excellent accuracy of ±0.2°C. A powerful mixing motor (1200r/min) ensures uniform temperature distribution throughout the medium, creating the stable and ideal thermal environment required for accurate hydrometer readings before correction to standard temperatures (15°C or 60°F).
Designed for efficiency and durability, this apparatus features a two-slot hole design, which allows the operator to test two samples simultaneously. This capability for parallel testing significantly improves productivity and throughput in a busy laboratory. The heating element is made from high-quality, anti-corrosion stainless steel, guaranteeing a long service life and reliable performance even with continuous use.
With its simple operation and elegant structure, this instrument is a mandatory tool for any laboratory in refineries, storage terminals, and third-party inspection agencies. By providing a standardized and easy method for one of the most basic yet critical oil quality parameters, this apparatus helps ensure fair trade, optimal process control, and consistent product quality time after time.

