Pastikan produk bahan bakar Anda memenuhi spesifikasi volatilitas yang krusial dengan Reid Vapour Pressure Bath kami. Instrumen fundamental ini dirancang khusus untuk menentukan tekanan uap dari bensin, minyak mentah volatil, dan produk perminyakan volatil lainnya menggunakan Metode Reid. Pengukuran Reid Vapor Pressure (RVP) adalah parameter kunci yang mempengaruhi performa mesin, keamanan penyimpanan, dan regulasi lingkungan. Apparatus ini dirancang dan dibangun untuk menjalankan pengujian secara penuh sesuai dengan standar industri yang esensial, ASTM D323.
Akurasi dan stabilitas adalah kunci utama dalam pengujian RVP. Oleh karena itu, instrumen ini dilengkapi dengan sistem kontrol suhu digital presisi tinggi yang secara konsisten menjaga suhu bak air (water bath) pada titik 37.8°C dengan akurasi luar biasa, yaitu ±0.1°C. Untuk memastikan pemanasan yang merata pada seluruh bagian tabung uji (bomb), sistem ini menggunakan sirkulasi pump loop yang mengaduk air secara teratur dan senyap. Hal ini menjamin tercapainya kondisi ekuilibrium yang stabil untuk pembacaan tekanan uap yang akurat.
Dirancang untuk efisiensi dan keselamatan di laboratorium modern, alat ini memiliki kapasitas untuk melakukan dua grup eksperimen secara bersamaan, memungkinkan Anda menguji hingga dua pasang tabung uji (bombs) secara paralel. Fitur ini secara signifikan meningkatkan produktivitas dan alur kerja laboratorium Anda. Keselamatan ditingkatkan melalui penggunaan solid-state relay (SSR) untuk output pemanas, yang beroperasi tanpa kontak, tanpa percikan api (sparkless), dan tanpa suara, sebuah fitur keamanan yang sangat penting saat menangani sampel yang sangat mudah terbakar.
Dengan pengoperasian yang mudah melalui panel kontrol digital yang jelas dan pembacaan tekanan yang nyaman dari pressure gauge ber-dial besar, instrumen ini menawarkan solusi yang ramah pengguna dan andal. Desainnya yang rasional dan kokoh menjadikannya alat yang tahan lama untuk penggunaan sehari-hari. Bagi kilang minyak, jalur pipa, dan laboratorium quality control, Reid Vapour Pressure Bath ini adalah perangkat wajib untuk memastikan produk bahan bakar memenuhi spesifikasi volatilitas yang paling ketat.
Ensure your fuel products meet crucial volatility specifications with our Reid Vapour Pressure Bath. This fundamental instrument is specifically designed to determine the vapor pressure of gasoline, volatile crude oil, and other volatile petroleum products using the Reid Method. The Reid Vapor Pressure (RVP) measurement is a key parameter that affects engine performance, storage safety, and environmental regulations. This apparatus is designed and built to perform tests in full compliance with the essential industry standard, ASTM D323.
Accuracy and stability are paramount in RVP testing. Therefore, this instrument is equipped with a high-precision digital temperature control system that consistently maintains the water bath temperature at the exact 37.8°C with an exceptional precision of ±0.1°C. To ensure the test bombs are heated evenly, the system utilizes a pump loop circulation to stir the water regularly and noiselessly. This guarantees that a stable equilibrium condition is reached for an accurate vapor pressure reading.
Designed for efficiency and safety in the modern laboratory, this apparatus has the capacity to conduct two groups of experiments at the same time, allowing you to test up to two pairs of bombs in parallel. This feature significantly improves your laboratory's productivity and workflow. Safety is enhanced through the use of a solid-state relay (SSR) for the heating output, which provides contactless, sparkless, and noiseless operation—a critically important safety feature when handling highly flammable samples.
With easy operation via a clear digital control panel and convenient pressure reading from large-dial pressure gauges, this instrument offers a user-friendly and reliable solution. Its rational and robust design makes it a durable tool for daily use. For refineries, pipelines, and quality control laboratories, this Reid Vapour Pressure Bath is a mandatory device to certify that fuel products meet the strictest volatility specifications.

