Memperkenalkan sebuah solusi instrumental terdepan untuk analisis viskositas kinematik pada produk cair, baik yang transparan maupun buram. Perangkat canggih ini dirancang secara khusus untuk memenuhi dan melampaui standar pengujian internasional ASTM D445, menjadikannya aset tak ternilai bagi setiap laboratorium yang mengutamakan presisi dan keandalan. Dengan mengukur waktu yang dibutuhkan oleh volume cairan untuk mengalir di bawah gravitasi melalui viskometer kapiler kaca terkalibrasi, alat ini memberikan data viskositas kinematik yang sangat akurat. Hasil ini menjadi fondasi penting untuk perhitungan viskositas dinamis, memastikan kontrol kualitas produk Anda berada di level tertinggi dalam berbagai kondisi suhu yang konstan dan terkendali.
Keunggulan utama dari aparatus ini terletak pada sistem kontrol temperaturnya yang superior. Dibangun untuk memberikan stabilitas dan presisi, perangkat ini mampu menjaga suhu dalam rentang yang luas, mulai dari 20 hingga 100 derajat Celcius. Kontrol suhu dilakukan melalui panel digital modern yang memungkinkan pengaturan dengan ketelitian luar biasa hingga ±0.01°C. Tingkat akurasi yang fenomenal ini menjamin bahwa setiap pengujian dilakukan dalam kondisi yang identik dan dapat diulang kembali, menghilangkan variabel eksternal dan memastikan hasil yang konsisten serta dapat dipertanggungjawabkan secara ilmiah untuk analisis kualitas produk cair.
Dirancang untuk efisiensi dan produktivitas laboratorium, instrumen ini dilengkapi dengan bak pemanas yang memiliki insulasi termal canggih untuk menjaga kestabilan panas. Desainnya yang elegan dan fungsional memungkinkan penempatan hingga empat viskometer secara bersamaan, didukung oleh dua unit stopwatch digital untuk pencatatan waktu yang presisi. Kemudahan operasional menjadi prioritas, yang diwujudkan melalui klip penjepit viskometer yang inovatif dan canggih, mempermudah proses pemasangan dan pelepasan sampel. Struktur keseluruhan yang kokoh dan mudah dioperasikan memastikan alur kerja yang lebih cepat dan efisien.
Untuk performa optimal, aparatus ini beroperasi pada daya listrik AC 220V dengan output daya sebesar 1800W. Lingkungan operasional yang direkomendasikan adalah pada suhu ruangan antara 10 hingga 40 derajat Celcius dengan tingkat kelembapan tidak melebihi 85%. Spesifikasi teknis ini memastikan bahwa mesin dapat bekerja dengan stabilitas dan keandalan maksimum dalam lingkungan laboratorium pada umumnya. Desain yang rasional dengan struktur elegan tidak hanya menjamin fungsionalitas tetapi juga memberikan nilai estetika pada ruang kerja Anda, menjadikannya investasi cerdas untuk peningkatan kapabilitas dan citra laboratorium Anda.
Introducing a premier instrumental solution for the kinematic viscosity analysis of liquid products, both transparent and opaque. This advanced apparatus is specifically engineered to meet and exceed the international testing standard ASTM D445, making it an invaluable asset for any laboratory that prioritizes precision and reliability. By measuring the time required for a volume of liquid to flow under gravity through a calibrated glass capillary viscometer, this device delivers highly accurate kinematic viscosity data. These results serve as a critical foundation for calculating dynamic viscosity, ensuring your product's quality control is at the highest level under various constant and controlled temperature conditions.
The primary advantage of this apparatus lies in its superior temperature control system. Built for stability and precision, the device can maintain temperatures over a wide range, from 20 to 100 degrees Celsius. Temperature control is managed via a modern digital display panel that allows for exceptionally precise adjustments, achieving an accuracy of up to ±0.01°C. This phenomenal level of precision guarantees that every test is performed under identical and repeatable conditions, eliminating external variables and ensuring consistent, scientifically defensible results for liquid product quality analysis.
Designed for laboratory efficiency and productivity, this instrument is equipped with a heating bath featuring advanced thermal insulation to maintain heat stability. Its elegant and functional design accommodates up to four viscometers simultaneously, supported by two digital stopwatch units for precise timekeeping. Operational ease is a key priority, realized through an innovative and advanced viscometer clip that simplifies the process of mounting and removing samples. The overall robust and user friendly structure ensures a faster and more efficient workflow.
For optimal performance, this apparatus operates on AC 220V electrical power with a power output of 1800W. The recommended operating environment is an ambient temperature between 10 and 40 degrees Celsius with a humidity level not exceeding 85%. These technical specifications ensure that the machine can perform with maximum stability and reliability within typical laboratory settings. Its rational design with an elegant structure not only guarantees functionality but also adds aesthetic value to your workspace, making it a smart investment for enhancing your laboratory's capabilities and image.

