Kami mempersembahkan sebuah aparatus distilasi vakum yang dirancang secara presisi untuk menentukan rentang titik didih pada produk petroleum dan biodiesel di bawah tekanan rendah. Instrumen ini merupakan solusi definitif bagi laboratorium yang menangani senyawa yang dapat terurai pada suhu tinggi di tekanan atmosfer. Dengan mematuhi sepenuhnya standar metode pengujian internasional seperti ASTM D1160 dan ISO 6616, perangkat ini menjamin hasil yang akurat, dapat diulang, dan diakui secara global. Sistem terintegrasi ini terdiri dari kolom distilasi, sistem deteksi tekanan canggih, kabin penerima, pompa vakum, perangkap dingin (cold trap), dan unit refrigerasi, menyediakan semua yang dibutuhkan untuk analisis komprehensif.
Keakuratan pengujian disokong oleh sistem kontrol suhu dan pemanasan yang sangat canggih. Teknologi kontrol suhu PID (Proportional Integral Derivative) memastikan temperatur dapat dijaga dengan presisi luar biasa hingga dalam rentang ±0.1°C, memberikan stabilitas termal yang krusial selama proses distilasi. Perangkat ini dilengkapi dengan bak pemanas yang suhunya dapat diatur dari suhu ruangan hingga 80°C, serta sistem refrigerasi kompresor berperforma tinggi yang mampu mencapai suhu pendinginan ekstrem di -40°C. Kombinasi ini memungkinkan penanganan berbagai jenis sampel dengan karakteristik titik didih yang berbeda secara efektif.
Sistem manajemen tekanan pada unit ini adalah inti dari keunggulannya. Menggantikan pengukur hidragirum konvensional, alat ini menggunakan pengukur tekanan diferensial vakum diafragma tipis berpresisi tinggi yang modern dan aman. Sistem ini mampu mengukur dalam rentang tekanan yang sangat lebar, dari 130Pa hingga 6.7KPa, dengan tingkat kestabilan yang impresif, yaitu di bawah 0.01KPa untuk tekanan rendah. Pengaturan tekanan dilakukan secara intuitif melalui katup jarum presisi tinggi dan kenop pengatur, memberikan kontrol penuh kepada operator untuk mencapai kondisi vakum yang diinginkan.
Dirancang dengan fokus pada pengalaman pengguna, semua hasil dan parameter pengujian ditampilkan dengan jelas pada layar LCD digital yang modern. Kemudahan operasional ditingkatkan lebih lanjut dengan adanya perangkat pengatur tungku listrik tipe portabel yang praktis. Receiver atau penampung hasil distilasi juga dilengkapi dengan flow nappe yang didesain khusus untuk membuat laju aliran menjadi lebih merata dan terkontrol. Untuk operasionalnya, instrumen ini memerlukan daya sebesar 3KW dan tegangan listrik standar AC 220V 50Hz, menjadikannya kompatibel dengan sebagian besar infrastruktur laboratorium modern.
We present a precision-engineered vacuum distillation apparatus for determining the boiling point range of petroleum products and biodiesel under reduced pressure. This instrument is the definitive solution for laboratories handling compounds that may decompose at high temperatures under atmospheric pressure. By fully adhering to international test method standards such as ASTM D1160 and ISO 6616, this device guarantees results that are accurate, repeatable, and globally recognized. The integrated system comprises a distillation column, an advanced pressure detection system, a receiver cabin, a vacuum pump, a cold trap, and a refrigeration unit, providing everything needed for comprehensive analysis.
The accuracy of the testing is supported by a highly sophisticated temperature and heating control system. Proportional Integral Derivative (PID) temperature control technology ensures that the temperature can be maintained with outstanding precision, within a range of ±0.1°C, providing crucial thermal stability during the distillation process. The device is equipped with a warm bath whose temperature can be adjusted from room temperature up to 80°C, as well as a high-performance compressor refrigeration system capable of reaching extreme cooling temperatures of -40°C. This combination allows for the effective handling of various sample types with different boiling point characteristics.
The pressure management system in this unit is at the core of its excellence. Replacing conventional hydrargyrum gauges, this instrument utilizes a modern and safe high-precision thin diaphragm vacuum differential pressure gauge. The system is capable of measuring across a very wide pressure range, from 130Pa to 6.7KPa, with an impressive stability level of below 0.01KPa at low pressures. Pressure adjustment is intuitively handled via a high-precision needle valve and a regulating knob, giving the operator full control to achieve the desired vacuum conditions.
Designed with a focus on the user experience, all results and testing parameters are clearly displayed on a modern digital LCD screen. Operational ease is further enhanced by a practical, portable-type electric furnace regulation device. The distillate receiver is also equipped with a specially designed flow nappe to make the flow rate more even and controlled. For its operation, the instrument requires a power of 3KW and a standard electrical voltage of AC 220V 50Hz, making it compatible with most modern laboratory infrastructures.

