Memperkenalkan sebuah sistem uji getar elektromagnetik berperforma tinggi, solusi definitif untuk pengujian keandalan dan durabilitas produk di berbagai sektor industri. Instrumen canggih ini dirancang untuk mensimulasikan kondisi getaran yang kompleks—mulai dari guncangan saat transportasi hingga tegangan operasional frekuensi tinggi—guna mengevaluasi integritas struktural dan fungsional suatu produk. Dengan kemampuan pengujian multi-axis yang dapat beralih secara otomatis antara getaran vertikal, horizontal, depan, dan belakang, sistem ini memberikan analisis yang komprehensif dan realistis. Ini adalah alat yang sangat diperlukan bagi departemen R&D dan Quality Assurance di industri elektronik, otomotif, dirgantara, dan pengemasan untuk memvalidasi desain dan memastikan kualitas produk sebelum diluncurkan ke pasar.
Sistem ini menawarkan kinerja dinamis yang luar biasa pada meja uji berukuran 500x500 mm. Mampu menghasilkan akselerasi maksimum hingga 20g, perangkat ini dapat menciptakan kondisi pengujian yang ekstrem untuk aplikasi yang paling menuntut. Rentang frekuensi sapuan (sweep frequency) yang sangat lebar, dari 1Hz hingga 600Hz, dapat diatur secara bebas, memungkinkan simulasi berbagai skenario getaran. Amplitudo getaran yang dapat disesuaikan dengan mudah dari 0 hingga 5mm memberikan fleksibilitas tambahan untuk menyesuaikan intensitas pengujian sesuai dengan standar atau kebutuhan spesifik, memastikan cakupan pengujian yang lengkap dari getaran level rendah hingga level tinggi.
Kecanggihan sesungguhnya dari sistem ini terletak pada kontroler presisi tinggi dan kemampuan pemrograman yang luas. Dengan presisi frekuensi hingga 0.1Hz, setiap parameter pengujian dapat diatur dengan sangat akurat. Fungsi terprogram memungkinkan pengguna untuk merancang siklus pengujian yang kompleks hingga 8 segmen, di mana setiap segmen dapat memiliki frekuensi dan durasi yang ditentukan secara individual. Lebih lanjut, mode sapuan lanjutan seperti sapuan logaritmik dan perkalian (multiplier work) memungkinkan replikasi profil getaran yang sangat spesifik dan dapat diulang, memberikan hasil pengujian yang konsisten dan dapat dipertanggungjawabkan secara ilmiah.
Dirancang untuk efisiensi dan kemudahan penggunaan di lingkungan laboratorium modern, sistem ini dilengkapi dengan antarmuka operasi yang intuitif dan konektivitas USB untuk kemudahan ekspor data dan pemuatan profil uji. Panel kontrol yang jelas memungkinkan operator untuk dengan mudah memilih mode operasi, termasuk frekuensi tetap, sapuan, dan program yang telah ditentukan. Menghasilkan gelombang getaran sinusoidal (sine wave) yang bersih, sistem ini tidak hanya kuat dan serbaguna, tetapi juga merupakan platform yang andal dan efisien untuk melakukan validasi produk yang paling kritis, memastikan produk Anda tangguh dan andal di dunia nyata.
Introducing a high-performance electromagnetic vibration testing system, the definitive solution for product reliability and durability testing across a multitude of industries. This advanced instrument is designed to simulate complex vibration conditions—from transportation shocks to high-frequency operational stresses—to evaluate a product's structural and functional integrity. With multi-axis testing capabilities that can automatically switch between vertical, horizontal, front, and rear vibrations, this system provides a comprehensive and realistic analysis. It is an indispensable tool for R&D and Quality Assurance departments in the electronics, automotive, aerospace, and packaging industries to validate designs and ensure product quality before market launch.
This system offers exceptional dynamic performance on a spacious 500x500 mm test table. Capable of generating a maximum acceleration of up to 20g, the device can create extreme test conditions for the most demanding applications. The extremely wide sweep frequency range, from 1Hz to 600Hz, can be set arbitrarily, allowing for the simulation of diverse vibration scenarios. An easily adjustable vibration amplitude from 0 to 5mm provides additional flexibility to tailor the test intensity according to specific standards or needs, ensuring complete test coverage from low to high-level vibrations.
The true sophistication of this system lies in its high-precision controller and extensive programming capabilities. With a frequency precision of up to 0.1Hz, every test parameter can be set with extreme accuracy. The programmable function allows users to design complex test cycles of up to 8 segments, where each segment can have an individually defined frequency and duration. Furthermore, advanced sweep modes such as logarithmic and multiplier work sweeps enable the replication of highly specific and repeatable vibration profiles, delivering consistent and scientifically defensible test results.
Designed for efficiency and ease of use in a modern laboratory environment, the system is equipped with an intuitive operation interface and USB connectivity for easy data export and test profile loading. The clear control panel allows operators to effortlessly select operation modes, including fixed frequency, sweep, and predefined programs. Generating a clean sinusoidal (sine wave) vibration waveform, this system is not only powerful and versatile but also a reliable and efficient platform for conducting the most critical product validations, ensuring your products are robust and dependable in the real world.

