Memperkenalkan sebuah solusi instrumental yang krusial bagi setiap bisnis manufaktur dan distribusi: Mesin Uji Getar Simulasi Transportasi. Perangkat ini adalah garda terdepan Anda dalam memerangi kerugian akibat kerusakan produk selama pengiriman. Dirancang khusus untuk menguji ketahanan getaran dari berbagai barang dalam kemasan—mulai dari elektronik, furnitur, keramik, mainan, hingga peralatan industri—alat ini secara akurat mereplikasi guncangan dan getaran yang terjadi di perjalanan darat. Dengan melakukan pengujian sesuai standar transportasi Amerika dan Uni Eropa (ASTM, IEC), Anda dapat memvalidasi desain kemasan, mengidentifikasi titik lemah produk, dan mengambil tindakan korektif sebelum produk Anda meninggalkan gudang, secara efektif melindungi investasi dan reputasi merek Anda.
Keunggulan utama dari mesin ini adalah kemampuannya meniru kondisi transportasi nyata melalui mode getaran yang unik. Menggunakan gerakan resiprokal berjenis gyratory (sering diibaratkan seperti "pacuan kuda"), alat ini menghasilkan guncangan acak dan tidak monoton yang sangat mirip dengan getaran yang dialami paket di atas truk. Pengujian dijalankan pada amplitudo standar industri 25.4mm (1 inci) dengan kecepatan rotasi yang dapat disesuaikan antara 150 hingga 300 RPM. Kombinasi gerakan dan parameter yang terkontrol ini memastikan setiap sesi pengujian bersifat realistis, dapat diulang, dan sepenuhnya sesuai dengan protokol pengujian transportasi internasional.
Dirancang untuk fleksibilitas dan penggunaan industri jangka panjang, sistem ini tersedia dalam berbagai konfigurasi untuk memenuhi kebutuhan spesifik Anda. Pilihan kapasitas beban yang sangat luas, mulai dari 100 kg hingga 1000 kg, serta beragam ukuran meja kerja efektif hingga 1500x1500 mm, memastikan Anda dapat menguji segala sesuatu mulai dari paket kecil hingga barang besar yang dipalletkan. Konstruksinya yang tangguh, dengan rangka berlapis powder coating dan meja kerja stainless steel yang dilengkapi rel aluminium, menjamin daya tahan dan keandalan bahkan dalam penggunaan volume tinggi. Timer pengujian yang dapat diatur hingga 999 jam juga memungkinkan dilakukannya uji ketahanan jangka panjang.
Meskipun memiliki kemampuan yang kuat, mesin ini dirancang dengan mempertimbangkan kemudahan penggunaan dan lingkungan kerja. Desainnya yang unik memastikan operasi yang sederhana, sementara fungsi peredam (buffering function) berkontribusi pada tingkat kebisingan yang rendah, menjadikannya cocok untuk berbagai lingkungan laboratorium atau kontrol kualitas. Dengan berinvestasi pada alat uji simulasi transportasi ini, Anda tidak hanya membeli sebuah mesin, tetapi juga membeli ketenangan pikiran, kepuasan pelanggan yang lebih tinggi, dan penghematan biaya yang signifikan dari penurunan klaim kerusakan.
Introducing a crucial instrumental solution for every manufacturing and distribution business: the Simulated Transport Vibration Tester. This device is your frontline defense in the fight against losses from product damage during shipping. Specifically designed to test the vibration resistance of various packaged goods—from electronics, furniture, ceramics, and toys, to industrial equipment—this machine accurately replicates the shocks and vibrations encountered during land transit. By testing in accordance with American and EU transport standards (ASTM, IEC), you can validate packaging designs, identify product weaknesses, and take corrective action before your products leave the warehouse, effectively protecting your investment and brand reputation.
The primary advantage of this machine is its ability to mimic real-world transport conditions through a unique vibration mode. Utilizing a reciprocating, gyratory motion (often compared to "horse racing"), it produces random, non-monotonic jolts that closely resemble the vibrations a package experiences on a truck. Tests are run at a fixed, industry-standard amplitude of 25.4mm (1 inch) with an adjustable rotating speed between 150 and 300 RPM. This combination of controlled motion and parameters ensures every test session is realistic, repeatable, and fully compliant with international transport testing protocols.
Engineered for flexibility and long-term industrial use, this system is available in a wide range of configurations to meet your specific needs. An extensive selection of load capacities, scaling from 100 kg up to a massive 1000 kg, and various effective table sizes up to 1500x1500 mm, ensure you can test everything from small parcels to large, palletized goods. Its robust construction, featuring a powder-coated frame and a stainless steel working table with aluminum alloy rail tracks, guarantees durability and reliability even in high-volume usage. A test timer adjustable up to 999 hours also allows for extended, long-duration endurance tests.
Despite its powerful capabilities, the machine is designed with user-friendliness and the work environment in mind. Its unique design ensures simple operation, while a buffering function contributes to low-noise levels, making it suitable for various lab or quality control settings. By investing in this simulated transport tester, you are not just buying a machine; you are buying peace of mind, higher customer satisfaction, and significant cost savings from reduced damage claims.

