Memperkenalkan sebuah instrumen analisis termal yang canggih dan esensial, HDT & Vicat Tester otomatis, yang dirancang untuk memberikan data paling akurat mengenai kinerja material non-logam pada suhu tinggi. Perangkat ini memiliki fungsi ganda yang krusial: menentukan Suhu Distorsi Panas (Heat Distortion Temperature - HDT) dan Suhu Titik Lunak Vicat (Vicat Softening Point Temperature). Aplikasinya sangat luas, mencakup pengujian pada plastik, karet, nilon, dan berbagai bahan isolasi listrik. Yang terpenting, instrumen ini sepenuhnya memenuhi persyaratan dari puluhan standar internasional terkemuka, termasuk ASTM D648 (HDT), ASTM D1525 (Vicat), ISO 75, ISO 306, dan DIN, menjadikannya pilihan terpercaya untuk validasi produk di pasar global.
Dioperasikan melalui pengontrol layar sentuh (touch screen) yang modern dan intuitif, instrumen ini dirancang untuk kemudahan penggunaan, performa yang stabil, dan presisi yang tak tertandingi. Selama pengujian, operator dapat memantau suhu dan deformasi sampel secara real-time, dengan visualisasi kurva uji yang jelas. Tingkat presisi yang luar biasa tercermin pada akurasi kontrol suhu ±0.5°C dan kesalahan indikasi deformasi maksimum yang sangat rendah, yaitu ±0.001mm. Sistem cerdas ini secara otomatis menghentikan pemanasan setelah pengujian selesai, memastikan konsistensi dan repetabilitas hasil sekaligus menyederhanakan alur kerja di laboratorium.
Sistem termal pada perangkat ini direkayasa untuk kepatuhan standar yang ketat dan efisiensi. Dengan rentang kontrol suhu yang lebar dari suhu ruangan hingga 300°C, alat ini mampu menguji sebagian besar jenis polimer. Dua mode laju pemanasan standar industri—120°C/jam (2°C/menit) dan 50°C/jam—dapat dipilih untuk memenuhi protokol pengujian spesifik ASTM maupun ISO. Proses pendinginan setelah pengujian juga dioptimalkan, menggunakan pendinginan alami atau air untuk menurunkan suhu media pemanas (minyak silikon metil) secara efisien, mempersingkat waktu tunggu antar pengujian.
Dirancang untuk produktivitas laboratorium, alat ini dilengkapi dengan tiga rak pengujian yang memungkinkan pengujian beberapa sampel secara bersamaan. Salah satu fitur yang paling praktis adalah adanya printer internal (built-in). Fitur ini memungkinkan operator untuk mencetak data dan hasil pengujian secara langsung dari mesin tanpa memerlukan koneksi ke komputer atau perangkat lunak eksternal. Dengan kombinasi presisi tinggi, otomatisasi cerdas, dan kepatuhan standar yang luas, HDT Vicat Tester ini merupakan instrumen vital bagi unit inspeksi kualitas, universitas, dan perusahaan manufaktur untuk memvalidasi dan menjamin sifat termal dari material mereka.
Introducing an advanced and essential thermal analysis instrument, the automatic HDT & Vicat Tester, designed to provide the most accurate data on the high-temperature performance of non-metallic materials. This device serves a crucial dual function: determining the Heat Distortion Temperature (HDT) and the Vicat Softening Point Temperature. Its applications are extensive, covering tests on plastics, rubber, nylon, and various electrical insulation materials. Most importantly, this instrument fully complies with the requirements of dozens of leading international standards, including ASTM D648 (HDT), ASTM D1525 (Vicat), ISO 75, ISO 306, and DIN, making it a trusted choice for product validation in the global market.
Operated via a modern and intuitive touch screen controller, this instrument is designed for ease of use, stable performance, and unparalleled precision. During the test, operators can monitor the sample's temperature and deformation in real-time, with a clear visualization of the test curve. The exceptional level of precision is reflected in its ±0.5°C temperature control accuracy and an extremely low maximum deformation indication error of just ±0.001mm. The intelligent system automatically stops heating upon test completion, ensuring consistency and repeatability of results while simplifying the laboratory workflow.
The thermal system in this device is engineered for strict standard compliance and efficiency. With a wide temperature control range from ambient up to 300°C, it can test a vast majority of polymer types. Two industry-standard heating rates—120°C/h (2°C/min) and 50°C/h—are selectable to meet specific ASTM or ISO testing protocols. The post-test cooling process is also optimized, utilizing natural or water cooling to efficiently lower the temperature of the heating medium (methyl silicone oil), shortening the turnaround time between tests.
Designed for laboratory productivity, the device is equipped with three experimental racks, allowing for the simultaneous testing of multiple samples. One of its most practical features is the built-in printer. This feature allows operators to print data and test results directly from the machine without needing a connection to a computer or external software. With its combination of high precision, smart automation, and broad standards compliance, this HDT Vicat Tester is a vital instrument for quality inspection units, universities, and manufacturing enterprises to validate and guarantee the thermal properties of their materials.

