Memperkenalkan sebuah sistem pengujian termal polimer yang sangat cerdas dan sepenuhnya terkomputerisasi, dirancang untuk analisis mendalam terhadap Suhu Distorsi Panas (Heat Distortion Temperature - HDT) dan Suhu Titik Lunak Vicat (Vicat Softening Point). Instrumen ini merupakan solusi ideal bagi universitas, unit riset ilmiah, dan departemen pengawasan kualitas yang membutuhkan tidak hanya hasil pengujian, tetapi juga analisis data yang komprehensif. Dengan kepatuhan penuh terhadap serangkaian standar internasional—termasuk ASTM D648, ASTM D1525, ISO 75, ISO 306, GB/T1633, dan banyak lagi—sistem ini menjamin validitas dan pengakuan global atas data pengujian Anda pada material seperti plastik, karet, dan nilon.
Direkayasa untuk presisi dan stabilitas, instrumen ini memiliki struktur kabinet vertikal yang kokoh dengan sistem pengadukan otomatis heliks ganda di dalam bak media suhu konstan, memastikan keseragaman suhu yang luar biasa dengan akurasi ±0.5°C. Salah satu keunggulan utamanya adalah otomatisasi mekanis yang canggih; ketiga rak sampel dilengkapi dengan fungsi pengangkatan otomatis (atas dan bawah), menyederhanakan persiapan pengujian dan meningkatkan efisiensi alur kerja. Sensor perpindahan (displacement sensor) presisi tinggi dengan metode penyesuaian ganda menjamin pengukuran deformasi yang akurat, sementara sistem pengangkatan terintegrasi dirancang untuk operasi yang hening.
Kekuatan sebenarnya dari sistem ini terletak pada perangkat lunak (software) kontrolnya yang kuat dan intuitif. Beroperasi pada platform Windows, software ini mengubah mesin menjadi stasiun kerja analitis yang lengkap. Operator dapat memantau tren suhu dan deformasi secara real-time, dengan kurva uji yang digambar secara dinamis di layar. Lebih dari itu, perangkat lunak ini memungkinkan penyimpanan data historis, memberikan kemampuan tak ternilai untuk mengambil kembali pengujian sebelumnya, melakukan studi perbandingan antara berbagai batch atau material, dan mencetak laporan pengujian yang komprehensif kapan saja.
Sistem ini dirancang sebagai platform pengujian yang cerdas dan fleksibel. Perangkat lunak disertakan sebagai bagian dari paket, sementara unit Komputer PC dan Printer ditawarkan sebagai komponen opsional, memungkinkan laboratorium untuk mengintegrasikan instrumen dengan perangkat keras yang sudah ada. Fitur keselamatan seperti tombol berhenti darurat juga disertakan. Dengan kombinasi kontrol komputer canggih, analisis data mendalam, dan otomatisasi mekanis, HDT Vicat Tester ini adalah pilihan superior untuk penelitian polimer tingkat lanjut dan kontrol kualitas yang paling ketat.
Introducing a highly intelligent and fully computerized polymer thermal testing system, designed for in-depth analysis of Heat Distortion Temperature (HDT) and Vicat Softening Point Temperature. This instrument is the ideal solution for universities, scientific research units, and quality supervision departments that require not just test results, but also comprehensive data analysis. With full compliance to a vast array of international standards—including ASTM D648, ASTM D1525, ISO 75, ISO 306, GB/T1633, and more—this system guarantees the validity and global recognition of your test data on materials like plastics, rubber, and nylon.
Engineered for precision and stability, the instrument features a robust vertical cabinet structure with a double-helix automatic stirring system in the constant temperature medium bath, ensuring exceptional temperature uniformity with an accuracy of ±0.5°C. A key advantage is its advanced mechanical automation; the three sample racks are equipped with an automatic lifting function (up and down), simplifying test preparation and improving workflow efficiency. The high-precision displacement sensor with dual-adjustment methods ensures accurate deformation measurement, while the integrated lifting system is designed for quiet operation.
The true power of this system lies in its powerful and intuitive control software. Operating on a Windows platform, the software transforms the machine into a complete analytical workstation. Operators can monitor temperature and deformation trends in real-time, with test curves dynamically plotted on the screen. Furthermore, the software enables historical data storage, providing the invaluable ability to retrieve past tests, perform comparative studies between different batches or materials, and print comprehensive test reports at any time.
This system is designed as an intelligent and flexible testing platform. The software is included as part of the package, while the Computer PC unit and Printer are offered as optional components, allowing laboratories to integrate the tester with their existing hardware. Safety features such as an emergency stop switch are also included. With its combination of advanced computer control, in-depth data analysis, and mechanical automation, this PC-controlled HDT Vicat Tester is the superior choice for advanced polymer research and the most stringent quality control.

