Memperkenalkan sebuah solusi instrumental yang esensial untuk riset dan kontrol kualitas: Ruang Uji Penuaan Ozon (Ozone Aging Test Chamber). Perangkat canggih ini dirancang khusus untuk mensimulasikan dan mempercepat efek penuaan yang disebabkan oleh paparan ozon atmosferik pada material karet dan elastomer. Dengan mengontrol dan mengatur secara presisi konsentrasi ozon dan suhu di dalam ruang uji, instrumen ini memungkinkan Anda untuk secara akurat menentukan sifat anti-ozon dan karakteristik ketahanan retak dari spesimen. Kepatuhan penuh terhadap standar internasional terkemuka seperti ASTM D1149, ISO 1431, JISK6259, dan lainnya, menjadikannya alat validasi yang tak ternilai untuk memprediksi masa pakai dan memastikan keandalan produk di dunia nyata.
Inti dari keandalan pengujian ini terletak pada kemampuannya untuk menciptakan dan mempertahankan lingkungan yang terkontrol dengan sangat akurat. Chamber ini mampu mengatur suhu dalam rentang dari Suhu Ruangan+15°C hingga +65°C dengan akurasi kontrol ±0.5°C dan keseragaman distribusi suhu yang sangat baik. Didukung oleh generator ozon tipe silent discharge tube yang efisien, konsentrasi ozon di dalam ruang dapat dikelola secara stabil dalam rentang hingga 100 pphm dengan deviasi rendah (≤ 10%). Tingkat presisi ganda pada parameter suhu dan ozon ini memastikan bahwa setiap pengujian bersifat konsisten, dapat diulang, dan menghasilkan data yang valid secara ilmiah.
Direkayasa untuk daya tahan dan kinerja jangka panjang di lingkungan laboratorium yang menuntut, konstruksi chamber ini menggunakan material berkualitas tinggi. Ruang internal terbuat dari baja tahan karat SUS 304 yang sangat tahan terhadap korosi akibat ozon, sementara boks eksternal yang kokoh terbuat dari baja berkualitas dengan lapisan cat pelindung. Isolasi termal berperforma tinggi menggunakan busa poliuretan dan serat kaca memastikan stabilitas suhu dan efisiensi energi. Untuk mengakomodasi berbagai ukuran dan jumlah spesimen, chamber ini tersedia dalam beragam pilihan dimensi internal, mulai dari unit yang lebih ringkas hingga ruang berkapasitas besar.
Prioritas utama juga diberikan pada keamanan dan keandalan operasional. Sistem ini dilengkapi dengan berbagai fitur proteksi keamanan terintegrasi, termasuk perlindungan terhadap kebocoran listrik, arus pendek, dan arus berlebih, memberikan ketenangan pikiran selama pengujian jangka panjang yang mungkin berlangsung berjam-jam atau berhari-hari. Dengan kemampuannya yang canggih, Ozone Aging Test Chamber ini bukan sekadar alat uji, melainkan sebuah investasi strategis bagi industri yang bergantung pada durabilitas komponen karet seperti otomotif, dirgantara, kabel, dan manufaktur seal untuk mencegah kegagalan produk prematur di lapangan.
Introducing an essential instrumental solution for research and quality control: the Ozone Aging Test Chamber. This advanced device is specifically designed to simulate and accelerate the aging effects caused by atmospheric ozone exposure on rubber and elastomeric materials. By precisely controlling and adjusting the ozone concentration and temperature within the test chamber, this instrument allows you to accurately determine the anti-ozonant properties and crack-resistance characteristics of your specimens. Full compliance with leading international standards such as ASTM D1149, ISO 1431, JISK6259, and others, makes it an invaluable validation tool for predicting service life and ensuring real-world product reliability.
At the core of this test's reliability is its ability to create and maintain a highly accurate controlled environment. The chamber can regulate temperatures in the range of Room Temperature+15°C to +65°C with a control accuracy of ±0.5°C and excellent temperature distribution uniformity. Powered by an efficient silent discharge tube type ozone generator, the ozone concentration within the chamber can be stably managed in a range up to 100 pphm with a low deviation (≤ 10%). This dual precision on both temperature and ozone parameters ensures that every test is consistent, repeatable, and yields scientifically valid data.
Engineered for durability and long-term performance in demanding laboratory environments, the chamber's construction utilizes high-quality materials. The internal chamber is made from SUS 304 stainless steel, which is highly resistant to ozone-induced corrosion, while the robust external box is made from quality steel with a protective paint coating. High-performance thermal insulation using polyurethane foam and glass fiber ensures temperature stability and energy efficiency. To accommodate various specimen sizes and quantities, this chamber is available in a variety of internal dimensions, from more compact units to large-capacity chambers.
Top priority is also given to operational safety and reliability. The system is equipped with multiple integrated safety protection features, including protection against electrical leakage, short circuits, and over-current events, providing peace of mind during long-duration tests that may last for many hours or days. With its advanced capabilities, the Ozone Aging Test Chamber is not just a testing device, but a strategic investment for industries reliant on the durability of rubber components, such as automotive, aerospace, cable, and seal manufacturing, to prevent premature product failures in the field.

