Memperkenalkan sebuah terobosan dalam efisiensi laboratorium: Viskometer Kinematik Otomatis. Instrumen canggih ini dirancang untuk menyederhanakan dan mengotomatiskan sepenuhnya proses pengujian viskositas untuk berbagai produk perminyakan, termasuk oli pelumas, oli diesel, dan oli trafo. Dengan kepatuhan penuh terhadap standar industri paling krusial seperti ASTM D445, GB265-88, dan IP71, alat ini tidak hanya memberikan hasil yang akurat tetapi juga menjamin bahwa data Anda diakui secara global. Sistem cerdas ini mengambil alih seluruh alur kerja—mulai dari pengaturan waktu, kalkulasi, hingga pencetakan laporan—membebaskan waktu operator dan secara drastis mengurangi potensi kesalahan manusia.
Inti dari keunggulan instrumen ini adalah presisi yang tak tertandingi dan kontrol suhu yang cerdas. Ditenagai oleh Advanced SCM, sistem ini menawarkan kontrol suhu yang sangat stabil dalam rentang dari suhu ruangan hingga 100°C. Fitur utamanya adalah akurasi suhu yang dapat dipilih (selectable), memungkinkan pengguna untuk beralih ke mode presisi tinggi hingga ±0.01°C untuk pengujian yang paling sensitif. Stabilitas ini dicapai melalui penangas homoeotermik (homoeothermic bath) 10 liter berlapis ganda, yang dilengkapi dengan pemanas dan komponen stainless steel anti-korosi serta pengaduk bertenaga 1520 putaran/menit untuk menjamin keseragaman suhu yang sempurna.
Alur kerja laboratorium Anda akan ditransformasi oleh fitur otomatisasi penuh dari perangkat ini. Sistem ini mampu menguji hingga empat sampel secara bersamaan, memaksimalkan produktivitas. Proses pengujian disederhanakan dengan fungsi auto-timing yang memiliki akurasi ±0.1 detik, diikuti dengan auto-calculation untuk menentukan nilai viskositas kinematik secara instan. Lebih dari itu, instrumen ini juga akan secara otomatis menghitung nilai rata-rata dari hasil pengujian, menyajikan data akhir yang siap untuk dianalisis dan dilaporkan, semuanya tanpa intervensi manual.
Dioperasikan melalui layar LCD berwarna 7 inci yang besar dan jernih, pengguna dapat dengan mudah memantau semua kondisi kerja dan parameter secara real-time. Desainnya yang cerdas mencakup kopling kapilarimeter tiga titik vertikal yang fleksibel dan andal untuk pemasangan sampel yang mudah. Menawarkan nilai tambah yang luar biasa, instrumen ini juga memiliki fungsi ganda dan dapat digunakan sebagai penangas air homoeotermik presisi tinggi untuk aplikasi laboratorium lainnya. Siklus kerja yang sepenuhnya otomatis diakhiri dengan auto-printing hasil melalui printer thermal berkecepatan tinggi yang terintegrasi, menjadikan alat ini solusi "walk-away" yang benar-benar efisien.
Introducing a breakthrough in laboratory efficiency: the Automatic Kinematic Viscometer. This advanced instrument is designed to completely simplify and automate the viscosity testing process for a wide range of petroleum products, including lubricating oils, diesel oils, and transformer oils. With full compliance to the most crucial industry standards like ASTM D445, GB265-88, and IP71, this device not only delivers accurate results but also ensures your data is globally recognized. The intelligent system takes over the entire workflow—from timing and calculation to report printing—freeing up operator time and drastically reducing the potential for human error.
At the core of this instrument's excellence is its unparalleled precision and intelligent temperature control. Powered by an Advanced SCM, the system offers highly stable temperature control in the range from room temperature up to 100°C. A key feature is its selectable temperature accuracy, allowing users to switch to a high-precision mode of up to ±0.01°C for the most sensitive tests. This stability is achieved through a 10-liter, double-layer homoeothermic bath, equipped with an anti-corrosion stainless steel heater and components, and a powerful 1520 rounds/min stirrer to guarantee perfect temperature uniformity.
Your laboratory's workflow will be transformed by the full automation features of this device. The system can test up to four samples simultaneously, maximizing productivity. The testing process is streamlined with an auto-timing function accurate to ±0.1 seconds, followed by auto-calculation to instantly determine the kinematic viscosity value. Furthermore, the instrument will also automatically calculate the average value of test results, presenting final data that is ready for analysis and reporting, all without manual intervention.
Operated via a large and clear 7-inch color LCD screen, users can easily monitor all working conditions and parameters in real-time. The smart design includes a flexible and reliable three-point vertical capillarimeter clutch for easy sample installation. Offering exceptional added value, this instrument also has a dual function and can be used as a standalone high-precision homoeothermic water bath for other laboratory applications. The fully automated work cycle is completed with auto-printing of results via the integrated high-speed thermal printer, making this a truly efficient, "walk-away" solution.

