Memperkenalkan sebuah instrumen fundamental untuk rekayasa kualitas dan desain kemasan: Mesin Uji Jatuh (Drop Tester) industrial. Perangkat heavy-duty ini adalah solusi definitif untuk mensimulasikan dan menganalisis secara sistematis dampak dari kejatuhan yang tak terhindarkan selama proses penanganan, penyimpanan, dan transportasi. Dengan mereplikasi berbagai skenario kejatuhan secara presisi di lingkungan laboratorium yang terkontrol, mesin ini memungkinkan para insinyur dan manajer kualitas untuk secara proaktif mengidentifikasi titik lemah pada produk dan kemasannya. Ini adalah alat esensial untuk mengoptimalkan desain kemasan protektif, memvalidasi durabilitas produk, mengurangi biaya akibat kerusakan saat pengiriman, dan pada akhirnya melindungi kepuasan pelanggan serta reputasi merek.
Dirancang untuk menangani berbagai macam produk, mesin uji jatuh ini menawarkan kapasitas yang besar dan fleksibilitas yang luar biasa. Mampu mengakomodasi sampel uji dengan berat maksimum hingga 100 kg dan dimensi maksimum hingga 2000x800x800 mm, alat ini sangat cocok untuk menguji segalanya mulai dari barang elektronik konsumen, peralatan rumah tangga, hingga unit industri dalam kemasannya. Fleksibilitas pengujian ditingkatkan dengan ketinggian jatuh yang dapat diatur sepenuhnya (adjustable), dengan rentang dari hampir nol hingga 1500 mm, memberikan kemampuan untuk melakukan pengujian dampak energi rendah hingga tinggi sesuai dengan standar pengujian internasional atau protokol R&D internal.
Keunggulan utama dari instrumen ini adalah kemampuannya untuk melakukan simulasi dampak yang sangat realistis melalui berbagai metode jatuhan. Tidak terbatas pada jatuhan datar sederhana, mekanisme pelepasan canggihnya dirancang untuk dapat melakukan pengujian tumbukan secara presisi pada permukaan (face), tepi (edge), dan sudut (angle/corner) dari sampel uji. Kemampuan multi-metode ini sangat krusial untuk meniru berbagai jenis benturan yang mungkin terjadi di dunia nyata. Selain itu, kapabilitas "Zero Drop" memastikan jatuhan horizontal yang sempurna tanpa terguling, menyediakan kondisi uji yang bersih dan dapat diulang untuk evaluasi dampak permukaan secara akurat.
Dibangun untuk stabilitas, keamanan, dan keandalan jangka panjang, mesin uji jatuh ini memiliki konstruksi industrial yang sangat kokoh, tercermin dari bobotnya yang mencapai sekitar 1500 kg. Landasan uji yang besar dan rangka yang kuat memastikan keamanan operasional bahkan saat melakukan pengujian pada ketinggian dan beban maksimum. Ditenagai oleh sumber daya listrik 3 fasa, performanya yang konsisten menjadikannya aset yang dapat diandalkan di lingkungan pengujian yang paling menuntut. Dengan berinvestasi pada alat ini, perusahaan Anda menunjukkan komitmen yang tak tergoyahkan terhadap kualitas dan ketahanan produk.
Introducing a fundamental instrument for quality engineering and packaging design: the industrial Drop Test machine. This heavy-duty device is the definitive solution for systematically simulating and analyzing the effects of inevitable drops during handling, storage, and transit. By precisely replicating various drop scenarios in a controlled laboratory environment, this machine enables engineers and quality managers to proactively identify weaknesses in both their products and packaging. It is an essential tool for optimizing protective packaging designs, validating product durability, reducing costs associated with shipping damage, and ultimately protecting customer satisfaction and brand reputation.
Designed to handle a wide variety of products, this drop test machine offers a large capacity and outstanding flexibility. Capable of accommodating test samples with a maximum weight of up to 100 kg and maximum dimensions of up to 2000x800x800 mm, it is perfectly suited for testing everything from consumer electronics and home appliances to larger industrial units in their packaging. Testing flexibility is enhanced by a fully adjustable drop height, ranging from near-zero up to 1500 mm, providing the ability to conduct a full spectrum of low to high-energy impact tests in accordance with international testing standards or internal R&D protocols.
The primary advantage of this instrument is its ability to perform highly realistic impact simulations through various drop methods. Not limited to simple flat drops, its advanced release mechanism is engineered to precisely conduct impact tests on the face, edge, and corner (angle) of the test sample. This multi-method capability is crucial for mimicking the diverse types of impacts that can occur in the real world. Furthermore, its "Zero Drop" capability ensures a perfect, horizontal impact without tumbling, providing a clean and repeatable test condition for accurate surface impact evaluation.
Built for stability, safety, and long-term reliability, this drop test machine features an extremely robust industrial construction, reflected in its substantial weight of approximately 1500 kg. The large test bench and strong frame ensure operational safety even when conducting tests at maximum height and load. Powered by a 3-phase electrical supply, its consistent performance makes it a dependable asset in the most demanding testing environments. By investing in this machine, your company demonstrates an unwavering commitment to product quality and resilience.

