Memperkenalkan platform pengujian ban yang paling mutakhir, sebuah sistem uji kecepatan tinggi, durabilitas, dan performa tekanan rendah dengan dua posisi uji independen. Instrumen heavy-duty ini dirancang secara spesifik untuk memenuhi dan melampaui tuntutan pengujian yang paling ketat dari industri otomotif global. Dengan kepatuhan penuh terhadap serangkaian standar internasional yang krusial—termasuk SAE, ECE, ISO, dan FMVSS—mesin ini adalah solusi definitif bagi produsen ban dan lembaga riset untuk melakukan validasi desain, sertifikasi produk, dan kontrol kualitas. Kemampuannya yang serbaguna memungkinkan pengujian untuk berbagai jenis ban, mulai dari ban mobil penumpang (PCR) hingga ban truk dan bus radial (TBR).
Inti dari mesin ini adalah performa ekstrem dan efisiensi yang tak tertandingi. Ditenagai oleh motor penggerak bertenaga, drum uji berdiameter sekitar 1.7 meter mampu mencapai kecepatan hingga 400 km/jam, sementara sistem servo hidrolik loop tertutup (hydraulic close-loop servo) dapat memberikan beban radial hingga 100 KN dengan akurasi tinggi. Fitur unggulan dari platform ini adalah desain dua posisi uji (two positions), yang memungkinkan pengujian dua ban secara bersamaan. Kapabilitas ini secara drastis meningkatkan produktivitas laboratorium, memungkinkan kombinasi kecepatan dan beban yang berbeda untuk dijalankan secara paralel, dan memfasilitasi studi perbandingan yang efisien.
Lebih dari sekadar uji ketahanan standar, instrumen ini adalah laboratorium analisis dinamis yang lengkap. Platform ini secara unik mendukung fungsi penyesuaian sudut slip (slip angle) dan sudut camber (camber angle), memungkinkan simulasi yang sangat realistis terhadap gaya menikung dan berbagai kondisi pengendaraan yang kompleks. Rangkaian opsi pengukurannya yang luas mencakup pengukuran radius muatan statis dan dinamis, radius putar per kilometer, serta pemantauan suhu pada telapak (tread) dan dinding samping (sidewall) ban, memberikan data komprehensif untuk analisis performa yang mendalam.
Inovasi menjadi jantung dari sistem ini, yang dilengkapi dengan berbagai teknologi paten yang canggih. Sebuah sistem pengukuran suhu dan tekanan internal ban yang revolusioner memberikan data kritis langsung dari dalam ban selama pengujian kecepatan tinggi. Proses kerja juga dipermudah dan diamankan dengan perangkat pengangkat rakitan ban dan velg yang telah dipatenkan. Seluruh proses diawasi melalui sistem pemantauan real-time yang canggih. Didesain untuk operasi yang hemat energi, rendah getaran, dan rendah kebisingan, platform pengujian ini adalah investasi strategis untuk memimpin dalam inovasi dan kualitas di industri ban.
Introducing the ultimate tire testing platform: a state-of-the-art, two-position high-speed, endurance, and low-pressure performance testing machine. This heavy-duty instrument is specifically designed to meet and exceed the most rigorous testing demands of the global automotive industry. With full compliance to a crucial array of international standards—including SAE, ECE, ISO, and FMVSS—this machine is the definitive solution for tire manufacturers and research institutions to conduct design validation, product certification, and quality control. Its versatile capabilities accommodate tests for a wide range of tires, from Passenger Car Radials (PCR) to Truck and Bus Radials (TBR).
At the core of this machine lies its extreme performance and unmatched efficiency. Powered by a high-output driving motor, the massive drum (approximately 1.7m in diameter) can achieve speeds of up to 400 km/h, while a sophisticated hydraulic close-loop servo system can apply radial loads of up to 100 KN with high accuracy. The standout feature of this platform is its two-position design, which allows for the simultaneous testing of two tires. This capability drastically increases laboratory throughput, enables different speed and load combinations to be run in parallel, and facilitates efficient comparative studies.
More than just a standard endurance tester, this instrument is a complete dynamic analysis laboratory. The platform uniquely supports slip angle and camber angle adjustment functions, allowing for highly realistic simulations of cornering forces and complex driving dynamics. Its extensive range of optional measurements includes static and dynamic loaded radius, rolling radius per kilometer, and temperature monitoring across the tire's tread and sidewall, providing comprehensive data for in-depth performance analysis.
Innovation is at the heart of this system, which is equipped with various advanced patented technologies. A revolutionary internal tire temperature and pressure measurement system provides critical data directly from inside the tire during high-speed testing. The workflow is also made easier and safer with a patented tire and rim assembly lifting device. The entire process is supervised through an advanced real-time monitoring system. Designed for energy-saving, low-vibration, and low-noise operation, this testing platform is a strategic investment for leading the way in innovation and quality within the tire industry.

