Ini adalah Mesin Uji Kekuatan Tarik Single Pole dengan Kontrol Mikro Komputer, sebuah sistem pengujian material universal yang andal, serbaguna, dan mudah dioperasikan. Dirancang untuk melakukan serangkaian pengujian kekuatan fundamental—termasuk tarik, tekan, geser, kupas, dan sobek—alat ini adalah solusi ideal dan bernilai tinggi untuk laboratorium kontrol kualitas (QC), inspeksi fisik, dan pengembangan material. Berikut adalah rincian spesifikasi teknis dan kemampuannya.
Sistem penggerak mesin ini menggunakan motor AC dengan variable frequency drive, yang memberikan kinerja yang stabil dan andal untuk berbagai pengujian. Instrumen ini menawarkan fleksibilitas kapasitas beban yang dapat dipilih sesuai kebutuhan, mulai dari 5 kg hingga 200 kg, dengan resolusi beban 1/100.000 dan akurasi beban yang sangat baik, yaitu kurang dari ±0.5%. Kecepatan pengujian dapat dipilih dalam rentang 50 hingga 300 mm/menit, dan didukung oleh stroke (jarak tempuh) yang panjang hingga 900mm (atau dapat disesuaikan), memungkinkan pengujian pada spesimen dengan tingkat elongasi yang tinggi.
Salah satu fitur utamanya adalah fleksibilitas dalam pengoperasian. Mesin ini dapat dioperasikan secara standalone melalui panel kontrol mikro komputer dengan layar LCD terintegrasi, memungkinkan pengujian langsung tanpa perlu terhubung ke komputer. Namun, untuk analisis yang lebih mendalam, instrumen ini juga dapat dihubungkan ke PC (PC linkable). Saat terhubung, pengguna dapat memanfaatkan kekuatan penuh dari perangkat lunak berbasis Windows untuk kontrol, akuisisi data, dan analisis yang lebih canggih, menjadikannya investasi yang fleksibel dan siap untuk kebutuhan di masa depan.
Saat dioperasikan dengan perangkat lunak di PC, kemampuannya meningkat secara signifikan. Software ini menyediakan fungsi analisis data eksperimental, mode komparatif untuk menampilkan dan membandingkan beberapa kurva uji secara bersamaan, dan kemampuan untuk mendesain format laporan sesuai kebutuhan. Aplikasinya sangat luas, mencakup pengujian pada karet, plastik, logam, nilon, kain, kertas, komponen otomotif, dan banyak lagi, menjadikannya mesin uji universal "workhorse" yang sesungguhnya untuk setiap laboratorium.
This is a Micro Computer Single Pole Tensile Strength Tester, a reliable, versatile, and easy-to-operate universal material testing system. Designed to perform a fundamental range of strength tests—including tension, compression, shearing, peeling, and tear—this instrument is an ideal, high-value solution for quality control (QC) labs, physical inspection, and material development. The following are its detailed technical specifications and capabilities.
The machine's drive system utilizes an AC motor with a variable frequency drive, which provides stable and reliable performance for a variety of tests. The instrument offers flexible, selectable load capacities to suit specific needs, ranging from 5 kg up to 200 kg, with a load resolution of 1/100,000 and an excellent load accuracy of less than ±0.5%. The test speed is selectable within the range of 50 to 300 mm/min, and is supported by a long stroke of up to 900mm (or customizable), allowing for tests on specimens with high elongation.
One of its key features is its operational flexibility. The machine can be operated in a standalone mode via its integrated micro computer control panel with an LCD display, allowing for direct testing without needing to be connected to a computer. However, for more in-depth analysis, the instrument is also PC linkable. When connected, users can leverage the full power of the Windows-based software for more advanced control, data acquisition, and analysis, making it a flexible, future-ready investment.
When operated with the PC software, its capabilities are significantly enhanced. The software provides an experimental data analysis function, a comparative mode to display and compare multiple test curves simultaneously, and the ability to design custom report formats as needed. Its applications are extremely broad, covering tests on rubber, plastic, metal, nylon, fabric, paper, automotive components, and much more, making it a true "workhorse" universal testing machine for any laboratory.

