Ini adalah Ruang Uji Lampu UV (UV Lamp Tester), sebuah sistem uji pelapukan dipercepat yang dirancang untuk mensimulasikan kerusakan material akibat paparan sinar matahari, embun, dan hujan dalam lingkungan laboratorium yang terkontrol. Alat ini sangat penting untuk pengujian ketahanan dan prediksi masa pakai produk non-logam. Berikut adalah rincian spesifikasi teknis dan kemampuannya yang komprehensif.
Sistem ini mampu mensimulasikan siklus cuaca yang realistis dan lengkap. Sumber radiasi utamanya adalah sistem lampu UV yang dapat dikonfigurasi dengan pilihan lampu UV-A (rentang panjang gelombang 315-400mm) atau UV-B (280-315mm) untuk meniru spektrum UV yang berbeda sesuai dengan standar pengujian yang beragam. Selain radiasi UV, alat ini juga dapat mensimulasikan siklus embun (kondensasi) dengan menghasilkan uap dari air yang dipanaskan di dasar chamber, serta siklus hujan melalui sistem semprotan (spray nozzle) terintegrasi, memberikan kemampuan uji pelapukan yang menyeluruh.
Kontrol kondisi lingkungan yang presisi adalah kunci untuk hasil yang dapat diandalkan. Chamber ini menawarkan rentang suhu operasional dari Suhu Ruangan+10°C hingga 70°C dengan fluktuasi hanya ±0.5°C dan keseragaman ±2°C. Rentang kelembapan dapat dipertahankan pada tingkat saturasi tinggi dari 90% hingga 99% RH untuk siklus kondensasi yang efektif. Parameter kritis, Suhu Papan Tulis Hitam (Blackboard Temperature), dapat dikontrol secara spesifik dalam rentang 50°C hingga 70°C. Durasi pengujian dapat diprogram dan diatur secara fleksibel hingga 999 jam.
Dirancang untuk aplikasi yang luas, instrumen ini memiliki ruang kerja yang lapang dengan area radiasi efektif 1100x400 mm. Alat ini sangat vital untuk memprediksi dan menganalisis berbagai jenis degradasi material, termasuk pemudaran warna (bleaching), penurunan kecerahan, keretakan (cracking), menjadi rapuh (brittle), pengelupasan (powdering), dan oksidasi. Oleh karena itu, instrumen ini menjadi aset tak ternilai bagi kontrol kualitas dan R&D di berbagai industri seperti cat, pelapisan (coatings), plastik, otomotif, perekat, percetakan, dan material bangunan.
This is a UV Lamp Tester, an accelerated weathering test system designed to simulate material degradation caused by sunlight, dew, and rain in a controlled laboratory environment. This instrument is essential for testing the durability and predicting the service life of non-metallic products. The following are its detailed and comprehensive technical specifications and capabilities.
This system is capable of simulating realistic and complete weather cycles. Its primary radiation source is a UV lamp system that can be configured with a choice of UV-A (wavelength range 315-400mm) or UV-B (280-315mm) lamps to mimic different solar spectrums according to various testing standards. In addition to UV radiation, the device can also simulate a dew cycle (condensation) by generating vapor from heated water at the base of the chamber, as well as a rain cycle through an integrated spray nozzle system, providing comprehensive weathering test capabilities.
Precise control of environmental conditions is key to reliable results. The chamber offers an operational temperature range from Room Temperature+10°C to 70°C with a fluctuation of only ±0.5°C and uniformity of ±2°C. The humidity range can be maintained at high saturation levels from 90% to 99% RH for an effective condensation cycle. A critical parameter, the Blackboard Temperature, can be specifically controlled within the range of 50°C to 70°C. The test duration is programmable and flexibly adjustable up to 999 hours.
Designed for broad applications, this instrument features a spacious working chamber with an effective radiation area of 1100x400 mm. It is vital for predicting and analyzing various types of material degradation, including color fading (bleaching), brightness down, cracking, becoming brittle, powdering, and oxidation. Therefore, this instrument is an invaluable asset for quality control and R&D in numerous industries such as paints, coatings, plastics, automotive, adhesives, printing, and building materials.

