Kami menyediakan rangkaian lengkap Penangas Air Laboratorium (Laboratory Water Bath), sebuah solusi fundamental untuk semua kebutuhan pemanasan termostatik yang presisi. Portofolio kami mencakup berbagai tipe yang dirancang untuk aplikasi di bidang medis, farmasi, industri kimia, biologi, dan riset ilmiah, ideal untuk proses distilasi, pengeringan, konsentrasi, dan inkubasi. Berikut adalah rincian spesifikasi dan konfigurasi yang tersedia dalam portofolio kami.
Portofolio kami menawarkan beragam konfigurasi untuk memenuhi setiap kebutuhan laboratorium. Tersedia Penangas Air Multi-Lubang (Multi-Hole Water Bath) dengan pilihan 1, 2, 4, 6, hingga 8 lubang, memungkinkan pemrosesan beberapa sampel secara bersamaan untuk efisiensi maksimal. Selain itu, kami juga menawarkan Penangas Air Tangki Kaca dengan Pengaduk (Glass Tank Water Bath with Stirrer). Tipe ini sangat ideal untuk aplikasi yang membutuhkan homogenitas suhu tertinggi dan kemampuan untuk mengamati sampel secara visual selama proses berlangsung, dengan kecepatan pengaduk yang dapat diatur dari 0 hingga 2500 RPM.
Seluruh rangkaian produk kami dilengkapi dengan sistem kontrol suhu yang presisi untuk kinerja yang andal. Opsi kontrol mencakup pengontrol digital dengan sistem PID canggih dan sensor PT100 yang responsif, memastikan akurasi dan stabilitas suhu yang tinggi. Rentang suhu operasional pada umumnya adalah dari suhu ruangan hingga 100°C, dengan tingkat fluktuasi suhu yang sangat rendah, serendah <0.5°C. Pemanasan yang efisien dan seragam dijamin oleh elemen pemanas imersi berbentuk U yang dirancang untuk transfer panas yang optimal.
Setiap unit dalam rangkaian ini dibangun dengan material berkualitas tinggi untuk daya tahan jangka panjang. Konstruksi tangki internal dan penutup atas menggunakan baja tahan karat (stainless steel) yang kuat dan sangat tahan terhadap korosi. Model-model tertentu menampilkan teknologi cetak satu langkah (one-step molding) yang inovatif, menghasilkan tangki tanpa sambungan yang anti-bocor dan sangat awet. Eksterior yang kokoh terbuat dari pelat baja cold-rolled dengan lapisan pelindung, memastikan setiap penangas air kami siap untuk penggunaan intensif di lingkungan laboratorium manapun.
We provide a complete range of Laboratory Water Baths, a fundamental solution for all precise thermostatic heating needs. Our portfolio includes various types designed for applications in the medical, pharmaceutical, chemical, biological, and scientific research fields, ideal for distillation, drying, concentration, and incubation processes. The following are the detailed specifications and configurations available in our portfolio.
Our portfolio offers a variety of configurations to meet every laboratory requirement. We have Multi-Hole Water Baths available with a choice of 1, 2, 4, 6, or up to 8 holes, allowing for the simultaneous processing of multiple samples for maximum efficiency. Additionally, we also offer a Glass Tank Water Bath with an Integrated Stirrer. This type is ideal for applications requiring the highest temperature homogeneity and the ability to visually observe the sample during the process, with an adjustable stirrer speed from 0 to 2500 RPM.
Our entire product line is equipped with precision temperature control systems for reliable performance. Control options include digital controllers with an advanced PID system and a responsive PT100 sensor, ensuring high temperature accuracy and stability. The typical operating temperature range is from room temperature up to 100°C, with an extremely low temperature fluctuation rate, as low as <0.5°C. Efficient and uniform heating is guaranteed by U-shaped immersion heating elements designed for optimal heat transfer.
Every unit in this range is built with high-quality materials for long-term durability. The construction of the internal tank and top cover utilizes strong and highly corrosion-resistant stainless steel. Select models feature innovative one-step molding technology, resulting in a seamless, anti-leakage tank for enhanced safety and longevity. The robust exterior is made of cold-rolled steel plate with a protective coating, ensuring that every one of our water baths is ready for intensive use in any laboratory environment.

