Ini adalah Alat Analisa Permeabilitas Uap Air, sebuah sistem pengujian presisi tinggi untuk mengukur Laju Transmisi Uap Air (Water Vapor Transmission Rate - WVTR) pada berbagai jenis film kemasan dan material barrier. Instrumen ini sepenuhnya memenuhi persyaratan dari puluhan standar internasional terkemuka, termasuk ASTM E96, ISO 2528, dan TAPPI T464, menjadikannya alat vital untuk kontrol kualitas di industri makanan, farmasi, dan elektronik. Berikut adalah rincian spesifikasi teknis dan kemampuannya.
Instrumen ini beroperasi menggunakan metode gravimetri yang sangat akurat, dilengkapi dengan sel penimbangan keseimbangan elektromagnetik (electromagnetic balance weighing cell) resolusi tinggi 0.0001g dari merek terkemuka Eropa. Keunggulan utamanya adalah desain dua ruang uji (dual test chamber), di mana setiap ruang memiliki sensor terpisah, memungkinkan pengujian dua sampel secara simultan dan independen untuk memaksimalkan produktivitas laboratorium. Dengan rentang pengukuran yang sangat luas dari 0.02 hingga 10000 g/m²·24jam dan presisi pengujian 0.001g/m²·24jam, alat ini mampu menguji dari material high-barrier hingga low-barrier.
Sistem ini menawarkan kontrol kondisi lingkungan pengujian yang sangat akurat dan stabil. Rentang suhu pengujian dapat diatur dari 10°C hingga 50°C dengan presisi kontrol ±0.1°C, sementara rentang kelembapan dapat diatur dari 0% hingga 90% RH dengan presisi ±2%RH. Proses pengujian berjalan sepenuhnya otomatis, mulai dari penguncian parameter, penilaian otomatis (auto-judging), hingga penyimpanan data otomatis, yang secara signifikan mengurangi beban kerja operator dan memastikan konsistensi hasil.
Fleksibilitas operasional adalah kunci dari desain sistem ini. Instrumen ini dapat berfungsi sebagai unit standalone yang dioperasikan melalui layar sentuh berwarna (color touch screen), atau dapat dihubungkan ke komputer melalui port USB untuk fungsionalitas yang lebih luas. Saat terhubung, perangkat lunak yang canggih menyediakan antarmuka visual dengan tampilan kurva dinamis secara real-time, penyimpanan data yang luas untuk analisis historis, dan kemampuan untuk mengekspor data dengan mudah untuk keperluan pelaporan dan pencetakan, menjadikannya solusi pengujian WVTR yang lengkap dan serbaguna.
This is a Water Vapor Permeability Analyzer, a high-precision testing system for measuring the Water Vapor Transmission Rate (WVTR) of various packaging films and barrier materials. This instrument fully complies with the requirements of dozens of leading international standards, including ASTM E96, ISO 2528, and TAPPI T464, making it a vital tool for quality control in the food, pharmaceutical, and electronics industries. The following are its detailed technical specifications and capabilities.
The instrument operates using the highly accurate gravimetric method, equipped with a high-resolution 0.0001g electromagnetic balance weighing cell from a leading European brand. Its key advantage is the dual test chamber design, where each chamber has a separate sensor, allowing for the simultaneous and independent testing of two samples to maximize laboratory productivity. With an extremely wide measuring range from 0.02 to 10000 g/m²·24h and a testing precision of 0.001g/m²·24h, it can test everything from high-barrier to low-barrier materials.
This system offers extremely accurate and stable control of the test environment conditions. The testing temperature range is adjustable from 10°C to 50°C with a control precision of ±0.1°C, while the humidity range is adjustable from 0% to 90% RH with a precision of ±2%RH. The testing process is fully automatic, from parameter locking and auto-judging to auto-storage of data, which significantly reduces operator workload and ensures result consistency.
Operational flexibility is key to this system's design. The instrument can function as a standalone unit operated via its color touch screen, or it can be connected to a computer via a USB port for expanded functionality. When connected, the advanced software provides a visual interface with real-time dynamic curve display, extensive data storage for historical analysis, and the ability to easily export data for reporting and printing purposes, making it a complete and versatile WVTR testing solution.

