Ini adalah Alat Uji Puntir Benang Digital (Digital Reeling Twist Tester), sebuah instrumen presisi yang dirancang untuk menentukan jumlah puntiran pada benang tunggal (single) maupun benang gintir (plied). Alat ini sepenuhnya memenuhi persyaratan metode pengujian dalam standar industri tekstil internasional seperti ISO 2061 dan ASTM D1422/1423. Instrumen ini adalah perangkat esensial untuk kontrol kualitas di industri pemintalan dan tekstil. Berikut adalah rincian spesifikasi teknis dan kemampuannya.
Instrumen ini menawarkan fleksibilitas pengujian yang superior dengan dukungan untuk dua metode pengujian utama: Metode Hitung Langsung (Direct Counting Method) dan Metode Lepas-Puntir-Puntir-Ulang (Untwist-Retwist Method). Digerakkan oleh motor elektrik, mesin ini memiliki kecepatan rotasi yang dapat diatur dalam rentang 300 hingga 1200 putaran per menit, memungkinkan pengujian yang efisien. Pengujian dapat dilakukan pada berbagai panjang sampel standar yang dapat dipilih, termasuk 25, 50, 100, 250, dan 500 mm, untuk mengakomodasi berbagai jenis benang dan persyaratan metode uji.
Dirancang untuk akurasi dan kemudahan penggunaan, semua hasil dan parameter ditampilkan pada layar digital yang jernih. Alat ini mampu menghitung jumlah puntiran dalam rentang yang sangat lebar, dari 1 hingga 9999.9 puntiran. Akurasi skala untuk pengaturan panjang sampel adalah 1mm, memastikan persiapan sampel yang presisi. Instrumen ini mampu menangani berbagai jenis ukuran benang, dari yang halus hingga kasar, dalam rentang 1 hingga 499.9 tex, menjadikannya sangat serbaguna untuk berbagai aplikasi di laboratorium tekstil.
Sebagai alat fundamental untuk kontrol kualitas tekstil, mesin uji puntir ini sangat penting bagi pabrik pemintalan (spinning mills), pabrik tenun/rajut, dan laboratorium riset. Dengan secara akurat menentukan jumlah puntiran per inci (TPI) atau puntiran per meter (TPM), produsen dapat memastikan konsistensi, kekuatan, penampilan, dan rasa (feel) dari benang dan kain yang dihasilkan. Operasi yang sederhana dan hasil yang andal menjadikannya investasi vital untuk menjaga standar kualitas produk.
This is a Digital Reeling Twist Tester, a precision instrument designed to determine the number of twists in both single and plied yarns. This instrument fully complies with the test method requirements of international textile industry standards such as ISO 2061 and ASTM D1422/1423. It is an essential device for quality control in the spinning and textile industries. The following are its detailed technical specifications and capabilities.
This instrument offers superior testing flexibility with support for the two primary standard methods: the Direct Counting Method and the Untwist-Retwist Method. Driven by an electric motor, the machine features a variable rotational speed adjustable in the range of 300 to 1200 revolutions per minute, allowing for efficient testing. Tests can be conducted on various selectable standard sample lengths, including 25, 50, 100, 250, and 500 mm, to accommodate different yarn types and test method requirements.
Designed for accuracy and ease of use, all results and parameters are shown on a clear digital display. The device can count twists over a very wide range, from 1 to 9999.9 twists. The scale accuracy for setting the sample length is 1mm, ensuring precise sample preparation. The instrument is capable of handling a wide variety of yarn sizes, from fine to coarse, within a range of 1 to 499.9 tex, making it highly versatile for numerous applications in a textile laboratory.
As a fundamental tool for textile quality control, this twist tester is crucial for spinning mills, weaving/knitting factories, and research laboratories. By accurately determining the twists per inch (TPI) or twists per meter (TPM), manufacturers can ensure the consistency, strength, appearance, and feel of their yarn and the final fabric. Its simple operation and reliable results make it a vital investment for maintaining product quality standards.

