Ini adalah Digital Tension Meter, sebuah instrumen portabel presisi tinggi yang dirancang untuk mengukur secara akurat tegangan pada material linier yang bergerak maupun statis, seperti benang, kawat halus, dan fiber optik. Alat ini sangat penting untuk kontrol kualitas (QC) secara real-time di lini produksi pada berbagai industri. Berikut adalah rincian spesifikasi teknis dan kemampuannya.
Instrumen ini memberikan kinerja pengukuran presisi tinggi, menggabungkan teknologi mikroprosesor terbaru dengan mekanisme tiga rol pemandu (three guide rollers) yang andal. Sistem ini mampu menghasilkan pengukuran dengan akurasi hingga 0.1cN dan didukung oleh tingkat pengambilan sampel internal yang sangat tinggi (sekitar 5 kHz) untuk menangkap fluktuasi tegangan secara akurat. Tersedia dalam berbagai konfigurasi, alat ini dapat mengukur spektrum tegangan yang luas, dari beberapa centiNewton hingga 2000cN (20N), untuk memenuhi kebutuhan aplikasi yang berbeda.
Dirancang untuk keserbagunaan di lingkungan industri yang dinamis, alat ini dapat diadaptasi untuk berbagai jenis material. Opsi untuk rol pemandu yang dapat disesuaikan—seperti keramik untuk benang halus, V-groove untuk kawat, atau aluminium solid—memastikan kontak yang optimal dan pengukuran yang akurat tanpa merusak material yang diuji. Kemampuannya yang luar biasa untuk aplikasi berkecepatan tinggi memungkinkannya mengukur tegangan secara akurat pada jalur produksi yang bergerak dengan kecepatan hingga 2000 meter per menit, dengan defleksi material yang minimal (maksimum 0.5mm).
Dibangun untuk kemudahan penggunaan dan daya tahan di lapangan, desainnya yang ringan dan portabel ditenagai oleh baterai AA standar, memudahkan teknisi untuk melakukan pengecekan di berbagai titik pada mesin produksi. Tampilan digital yang jernih dengan laju pembaruan yang cepat (sekitar 4 kali per detik) memastikan pembacaan hasil yang mudah dan instan. Untuk menjamin masa pakai yang panjang, instrumen ini dilengkapi dengan perlindungan beban berlebih (overload protection) hingga 150% dari rentang tegangannya, melindungi sensor presisi tinggi dari kerusakan yang tidak disengaja.
This is a Digital Tension Meter, a high-precision portable instrument designed to accurately measure the tension in moving or static linear materials, such as yarn, fine wire, and optical fiber. This tool is essential for real-time quality control (QC) on the production line across a variety of industries. The following are its detailed technical specifications and capabilities.
This instrument delivers high-precision measurement performance, combining the latest microprocessor technology with a reliable three-guide-roller mechanism. The system is capable of producing measurements with an accuracy of up to 0.1cN and is supported by a very high internal sampling rate (approx. 5 kHz) to accurately capture tension fluctuations. Available in various configurations, this tool can measure a wide spectrum of tensions, from a few centiNewtons up to 2000cN (20N), to meet different application needs.
Designed for versatility in a dynamic industrial environment, this tool can be adapted for various material types. Options for customizable guide rollers—such as ceramic for fine yarns, V-groove for wires, or solidified aluminum—ensure optimal contact and accurate measurement without damaging the material under test. Its outstanding capability for high-speed applications allows it to accurately measure tension on production lines moving at speeds of up to 2000 meters per minute, with minimal material deflection (0.5mm max).
Built for ease of use and durability in the field, its lightweight and portable design is powered by standard AA batteries, making it easy for technicians to perform checks at various points on production machinery. The clear digital display with a fast update rate (approx. 4 times per second) ensures easy and instant reading of results. To guarantee a long service life, the instrument is equipped with overload protection of up to 150% of its tension range, protecting the high-precision sensor from accidental damage.

