Kami menyediakan rangkaian lengkap alat ukur presisi untuk analisis kecepatan dan inspeksi gerak, yang mencakup Stroboscope dan Digital Tachometer. Peralatan portabel ini sangat penting untuk pemeliharaan prediktif (predictive maintenance), kontrol kualitas, dan riset & pengembangan di berbagai aplikasi industri mesin. Berikut adalah rincian spesifikasi teknis dan kemampuan dari kedua instrumen ini.
Stroboscope dirancang untuk analisis gerak visual secara non-kontak. Dengan memancarkan kilatan cahaya berfrekuensi tinggi yang dapat diatur, alat ini mampu "membekukan" atau "memperlambat" gerakan objek yang berputar atau bergetar dengan cepat. Ini memungkinkan operator untuk melakukan inspeksi visual secara detail terhadap komponen mesin seperti roda gigi, kipas, atau poros saat sedang beroperasi, untuk mendeteksi adanya ketidakseimbangan, getaran, atau cacat lainnya. Instrumen ini memiliki rentang pengujian yang sangat lebar, dari 50 hingga 40,000 FPM (Flashes Per Minute), cocok untuk mesin berkecepatan rendah hingga sangat tinggi.
Digital Tachometer adalah alat serbaguna untuk pengukuran kecepatan yang akurat. Instrumen ini dilengkapi dengan beberapa mode pengukuran. Mode Optik (Laser/Foto) memungkinkan pengukuran RPM non-kontak yang aman dan cepat dengan rentang sangat lebar dari 2.5 hingga 99,999 RPM. Untuk pengukuran langsung, Mode Kontak dapat digunakan untuk mengukur kecepatan rotasi dari 0.5 hingga 19,999 RPM. Selain itu, alat ini juga memiliki Mode Kecepatan Permukaan (Contact Wire-Speed) untuk mengukur kecepatan linier, seperti pada ban berjalan atau sabuk konveyor, dalam rentang 0.05 hingga 1999 meter per menit.
Kedua instrumen ini dirancang untuk penggunaan praktis di lingkungan industri. Tachometer Digital ditenagai oleh baterai atau adaptor DC eksternal, menjadikannya sangat portabel untuk dibawa ke mana saja. Stroboscope yang ringkas ditenagai oleh listrik AC standar untuk operasi yang stabil. Keduanya merupakan pasangan yang ideal: gunakan Tachometer untuk mendapatkan pembacaan RPM numerik yang presisi, kemudian atur Stroboscope pada frekuensi yang sama untuk melakukan inspeksi visual yang mendalam. Keduanya adalah alat vital untuk teknisi di industri manufaktur, otomotif, percetakan, dan tekstil.
We provide a complete range of precision measuring tools for speed analysis and motion inspection, which includes a Stroboscope and a Digital Tachometer. These portable instruments are essential for predictive maintenance, quality control, and R&D in a wide variety of industrial machinery applications. The following are the detailed technical specifications and capabilities of both instruments.
The Stroboscope is designed for non-contact visual motion analysis. By emitting high-frequency, adjustable flashes of light, this tool can "freeze" or "slow down" the motion of rapidly rotating or vibrating objects. This allows operators to perform detailed visual inspections of machine components like gears, fans, or shafts while they are in operation, to detect imbalances, vibrations, or other defects. This instrument features a very wide testing range, from 50 to 40,000 FPM (Flashes Per Minute), suitable for very low to very high-speed machinery.
The Digital Tachometer is a versatile tool for accurate speed measurement. This instrument is equipped with multiple measurement modes. The Optical (Laser/Photo) Mode allows for safe and fast non-contact RPM measurement with a very wide range from 2.5 to 99,999 RPM. for direct measurement, the Contact Mode can be used to measure rotational speed from 0.5 to 19,999 RPM. Additionally, it also features a Surface Speed (Contact Wire-Speed) Mode to measure linear velocity, such as on conveyor belts, in the range of 0.05 to 1999 meters per minute.
Both instruments are designed for practical use in industrial environments. The Digital Tachometer is powered by batteries or an external DC adapter, making it highly portable. The compact Stroboscope is powered by standard AC for stable operation. They are an ideal pair: use the Tachometer to get a precise numerical RPM reading, then set the Stroboscope to the same frequency to perform an in-depth visual inspection. Both are vital tools for technicians in the manufacturing, automotive, printing, and textile industries.

