Ini adalah rangkaian Mesin Gerinda dan Poles Piringan Ganda (Double Disc Grinding and Polishing Machine), sebuah solusi berefisiensi tinggi yang dirancang khusus untuk laboratorium preparasi sampel metalografi dengan volume kerja tinggi. Dengan memiliki dua piringan kerja, rangkaian ini memungkinkan beberapa tahap preparasi dilakukan secara simultan, secara drastis mengurangi waktu pengerjaan dan meningkatkan throughput laboratorium. Berikut adalah rincian spesifikasi teknis dan kemampuannya.
Fitur utama dari rangkaian ini adalah konfigurasi piringan ganda (double-disc). Model tercanggih dalam seri ini dilengkapi dengan dua motor independen dan sistem operasi terpisah untuk setiap piringan. Keunggulan ini memberikan fleksibilitas maksimal, memungkinkan operator untuk melakukan dua proses yang berbeda (misalnya, penggerindaan di satu sisi dan pemolesan di sisi lain) secara bersamaan tanpa interupsi. Rangkaian ini menawarkan pilihan diameter piringan yang serbaguna, termasuk 200mm, 230mm, dan 250mm.
Untuk memberikan kontrol proses yang optimal, mesin-mesin ini dilengkapi dengan berbagai pilihan kontrol kecepatan. Beberapa model menawarkan kecepatan putar ganda (dual-speed) yang dapat dipilih, seperti 150/300 RPM atau 450/600 RPM, yang ideal untuk prosedur standar dua tahap. Untuk fleksibilitas tertinggi, tersedia juga model dengan rentang kecepatan yang dapat diatur secara variabel dari 50 hingga 600 RPM, memungkinkan penyesuaian yang sangat presisi untuk berbagai jenis material dan bahan habis pakai (consumables) metalografi.
Setiap unit dalam rangkaian piringan ganda ini dirancang untuk proses preparasi basah (wet preparation) yang berkelanjutan, lengkap dengan selang pemasukan dan pembuangan air untuk setiap piringan guna memastikan pendinginan yang efektif dan kebersihan area kerja. Dengan konstruksi yang kokoh dan berat (hingga 75 kg), mesin ini menjamin operasi yang sangat stabil dan bebas getaran, bahkan saat kedua piringan beroperasi secara bersamaan. Rangkaian ini adalah pilihan utama untuk laboratorium yang memprioritaskan kecepatan, efisiensi, dan hasil preparasi sampel yang konsisten.
This is a series of Double Disc Grinding and Polishing Machines, a high-efficiency solution designed specifically for high-volume metallographic sample preparation laboratories. By featuring two working discs, this series allows for multiple preparation stages to be performed simultaneously, drastically reducing turnaround time and increasing laboratory throughput. The following are its detailed technical specifications and capabilities.
The core feature of this series is its double-disc configuration. The most advanced model in this series is equipped with two independent motors and a separate operation system for each disc. This advantage provides maximum flexibility, allowing an operator to perform two different processes (e.g., grinding on one side and polishing on the other) at the same time without interruption. The series offers versatile disc diameter options, including 200mm, 230mm, and 250mm.
To provide optimal process control, these machines are equipped with various speed control options. Some models offer selectable dual-speeds, such as 150/300 RPM or 450/600 RPM, which are ideal for standardized two-step procedures. For the ultimate in flexibility, a model with a wide, variably adjustable speed range from 50 to 600 RPM is also available, allowing for extremely precise adjustments for a wide variety of materials and metallographic consumables.
Every unit in this double-disc series is designed for a continuous wet preparation process, and comes complete with inlet and outlet water hoses for each disc to ensure effective cooling and a clean work area. With a robust and heavy construction (up to 75 kg), these machines guarantee highly stable, vibration-free operation, even when both discs are running simultaneously. This series is the premier choice for laboratories that prioritize speed, efficiency, and consistent, high-quality sample preparation results.

