Tingkatkan standar kontrol kualitas dan riset material Anda ke level tertinggi dengan mesin uji kekerasan dual fungsi yang dirancang untuk memberikan hasil presisi tak tertandingi. Perangkat canggih ini mengintegrasikan metode pengujian Brinell dan Vickers dalam satu unit yang kokoh, menjadikannya solusi ideal untuk berbagai aplikasi industri. Dari analisis baja, logam non fero, hingga keramik, alat ini mampu memberikan data kekerasan yang akurat dan dapat diandalkan. Kemampuannya yang superior juga mencakup pengujian lapisan permukaan metal yang telah melalui proses perlakuan panas seperti karburisasi, nitridasi, dan pengerasan, memastikan setiap komponen memenuhi spesifikasi yang paling ketat sekalipun.
Keunggulan utama dari instrumen ini terletak pada proses pengujian yang sepenuhnya otomatis, yang secara efektif mengeliminasi potensi kesalahan manusia dan menjamin konsistensi hasil pengujian setiap saat. Dengan kepatuhan penuh terhadap standar internasional terkemuka seperti ISO dan ASTM, Anda dapat memiliki keyakinan mutlak pada setiap angka yang dihasilkan. Alat ini juga sangat ideal untuk mengukur kekerasan Vickers pada komponen berukuran mikro dan super tipis, serta kekerasan Brinell pada logam lunak dan partikel kecil, menunjukkan fleksibilitasnya yang luar biasa. Pengoperasian yang efisien dan hasil yang cepat menjadikannya aset tak ternilai untuk meningkatkan produktivitas di laboratorium atau lini produksi Anda.
Dilengkapi dengan sistem optik berpresisi tinggi yang menawarkan magnifikasi hingga 500X, pengukuran jejak indentasi menjadi lebih jelas dan akurat. Mikrometer optik dengan nilai skala minimum 0.25μm memastikan tidak ada detail yang terlewatkan. Dengan rentang kekuatan uji yang luas dari 1 hingga 30 kgf, mesin ini dapat mengakomodasi pengujian pada beragam jenis material dengan tingkat kekerasan yang berbeda beda. Desain throat yang dalam dan ketinggian uji yang memadai memungkinkan pengujian sampel dengan berbagai ukuran dan bentuk, memberikan keleluasaan maksimal dalam setiap aplikasi pengujian.
Setiap unit disertai dengan rangkaian aksesoris standar yang lengkap untuk mendukung semua kebutuhan pengujian Anda sejak awal. Paket ini mencakup berbagai jenis meja uji seperti meja koordinat, meja besar, medium, dan bentuk V, memastikan stabilitas untuk berbagai bentuk sampel. Juga disertakan penetrator bola tungsten carbide dan penetrator piramida intan, beserta blok standar kekerasan Brinell dan Vickers untuk kalibrasi yang mudah dan akurat. Ini adalah solusi pengujian kekerasan yang komprehensif, dirancang untuk memberikan performa, keandalan, dan efisiensi sejak hari pertama penggunaan.
Elevate your quality control and material research standards to the highest level with a dual function hardness testing machine engineered for unparalleled precision. This advanced device integrates both Brinell and Vickers testing methods into a single, robust unit, making it the ideal solution for a vast range of industrial applications. From analyzing steel and non ferrous metals to ceramics, this machine delivers accurate and dependable hardness data. Its superior capabilities also extend to testing treated metal surface layers that have undergone processes like carburizing, nitriding, and hardening, ensuring every component meets the most stringent specifications.
The primary advantage of this instrument lies in its fully automatic testing process, which effectively eliminates the potential for human error and guarantees consistent test results every time. With full compliance to leading international standards such as ISO and ASTM, you can have absolute confidence in every figure generated. The device is also perfectly suited for determining the Vickers hardness of micro and super thin parts, as well as the Brinell hardness of soft metals and small components, demonstrating its exceptional versatility. Efficient operation and rapid results make it an invaluable asset for boosting productivity in your laboratory or production line.
Equipped with a high precision optical system offering magnifications up to 500X, the measurement of indentation traces becomes clearer and more accurate. An optical micrometer with a minimum scale value of 0.25μm ensures that no detail is overlooked. With a wide test force range from 1 to 30 kgf, this machine can accommodate testing on a diverse array of materials with varying hardness levels. The deep throat design and adequate maximum test piece height allow for the testing of samples in various sizes and shapes, providing maximum flexibility in every testing application.
Each unit comes with a complete set of standard accessories to support all your testing needs right from the start. The package includes various test tables such as a coordinate anvil, large, medium, and V shape tables, ensuring stability for different sample geometries. Also included are a tungsten carbide ball penetrator and a diamond pyramid penetrator, along with Brinell and Vickers standard hardness blocks for easy and accurate calibration. This is a comprehensive hardness testing solution, designed to deliver performance, reliability, and efficiency from the very first day of use.

