Saat menguji material lunak, presisi adalah segalanya. Mesin Uji Kekerasan Rockwell ini dirancang secara khusus untuk menjawab tantangan unik dalam mengukur kekerasan plastik keras, karet keras, resin sintetis, dan berbagai material non-logam lainnya. Tidak seperti penguji logam standar, instrumen ini direkayasa untuk memberikan hasil yang akurat dan dapat diandalkan tanpa merusak atau menembus permukaan spesimen, menjadikannya alat yang sangat diperlukan untuk produsen polimer, fasilitas R&D, dan laboratorium kontrol kualitas di berbagai industri.
Keunggulan utama alat ini terletak pada metode pengujian bermotor dan pemilihan skala Rockwell yang sesuai. Siklus pengujian—termasuk pembebanan, penahanan (dwelling), dan pelepasan beban—berjalan sepenuhnya otomatis. Sistem bermotor ini menjamin penerapan gaya yang konsisten setiap saat, menghilangkan variabel dan kesalahan yang disebabkan oleh operator, yang sangat krusial saat bekerja dengan polimer di mana hasil dapat sangat dipengaruhi oleh teknik pengujian. Dengan menggunakan skala Rockwell khusus seperti HRE, HRL, HRM, dan HRR, serta indenter bola berdiameter besar, alat ini memastikan pengukuran yang representatif terhadap kekerasan material, bukan sekadar ketahanan terhadap tusukan.
Meskipun dirancang untuk plastik, fleksibilitasnya sangat luas. Instrumen ini juga sangat efektif untuk menguji logam lunak seperti aluminium, timah, dan tembaga, serta baja lunak dan material gesek. Ini menjadikannya solusi serbaguna untuk fasilitas yang menangani berbagai jenis material lunak. Pengoperasiannya sederhana, dengan hasil pengujian yang ditampilkan dengan jelas pada dial indikator presisi yang besar dan mudah dibaca, memberikan pembacaan yang cepat dan andal bahkan di lingkungan produksi yang sibuk.
Dibangun untuk daya tahan dan keandalan, mesin ini merupakan aset kerja keras untuk laboratorium atau lantai produksi Anda. Setiap unit dilengkapi dengan set aksesoris standar yang diperlukan, termasuk berbagai ukuran indenter bola, meja uji besar, medium, dan berbentuk V, serta blok kekerasan standar untuk memastikan kalibrasi dan akurasi yang berkelanjutan. Percayakan kontrol kualitas material lunak Anda pada instrumen yang dirancang khusus untuk tugas tersebut.
When testing soft materials, precision is everything. This Rockwell Hardness Tester is specifically designed to meet the unique challenges of measuring the hardness of hard plastics, hard rubbers, synthetic resins, and a variety of other non-metallic materials. Unlike standard metal testers, this instrument is engineered to deliver accurate, reliable results without damaging or piercing the specimen surface, making it an indispensable tool for polymer manufacturers, R&D facilities, and quality control labs across multiple industries.
The core advantages of this tester lie in its motorized testing method and appropriate Rockwell scale selection. The entire testing cycle—including the loading, dwelling, and unloading of the test force—is fully automatic. This motorized system guarantees a consistent application of force every time, eliminating operator-induced variables and errors, which is critical when working with polymers where results can be highly influenced by testing technique. By utilizing specialized Rockwell scales such as HRE, HRL, HRM, and HRR, along with large-diameter ball indenters, this machine ensures a representative measurement of the material's hardness, not just its puncture resistance.
Though designed for plastics, its flexibility is extensive. This instrument is also highly effective for testing soft metals like aluminum, tin, and copper, as well as soft steel and friction materials. This makes it a versatile solution for facilities that handle a wide range of softer materials. Operation is straightforward, with test results clearly displayed on a large, easy-to-read precision dial indicator, providing quick and reliable readings even in a busy production environment.
Built for durability and reliability, this machine is a workhorse asset for your laboratory or production floor. Each unit comes equipped with the necessary standard accessories, including various sizes of ball indenters, large, medium, and V-shaped testing tables, and standard hardness blocks to ensure continuous calibration and accuracy. Trust your soft material quality control to an instrument that is purpose-built for the task.

