Analisis kandungan garam dalam minyak mentah adalah prosedur krusial yang menjadi garda terdepan dalam melindungi integritas operasional kilang minyak. Instrumen ini dirancang secara spesifik untuk menyediakan metode yang andal dan akurat dalam menentukan konsentrasi klorida atau garam dalam sampel minyak mentah. Dengan beroperasi sesuai standar industri yang diakui secara global, yaitu ASTM D3230 dan IP 265, alat ini memberikan jaminan bahwa setiap hasil pengujian dapat diandalkan untuk pengambilan keputusan penting terkait proses desalinasi dan pencegahan korosi. Pengukuran yang tepat adalah kunci untuk menghindari kerusakan peralatan vital seperti penukar panas, kolom distilasi, dan sistem perpipaan yang bernilai tinggi.
Perangkat ini memanfaatkan rakitan elektroda yang sensitif dan test lead yang terhubung ke meter digital auto ranging modern. Teknologi ini memungkinkan pembacaan voltase dan arus secara otomatis dan presisi, yang menjadi dasar untuk menghitung kandungan garam. Kemampuannya untuk mengukur dalam rentang konsentrasi yang luas, dari 0 hingga 500 mg/kg atau setara dengan 0 hingga 150 lb/1000 bbl, menjadikannya sangat fleksibel untuk menganalisis berbagai jenis minyak mentah dari sumber yang berbeda. Rentang pengukuran yang lebar ini memastikan bahwa alat ini relevan untuk digunakan mulai dari tahap eksplorasi hingga proses penyulingan.
Desain instrumen ini mengutamakan kemudahan penggunaan dan stabilitas selama pengujian. Dilengkapi dengan penyangga dan penahan yang kokoh, seluruh set peralatan gelas, termasuk ekstraktor dan botol segitiga, dapat dirangkai dengan aman untuk memastikan proses ekstraksi dan pengukuran berjalan tanpa gangguan. Unit kontrol utama memiliki antarmuka yang sederhana, memungkinkan operator untuk fokus pada persiapan sampel dan pencatatan hasil dengan efisiensi maksimal. Desain yang ergonomis ini meminimalkan waktu penyiapan dan memaksimalkan produktivitas laboratorium.
Setiap unit dikirimkan sebagai solusi turnkey yang komprehensif, mencakup semua aksesori yang diperlukan untuk segera memulai pengujian. Dalam paket pembelian sudah termasuk komponen utama, peralatan gelas esensial, sekering cadangan, serta sertifikasi dan manual penggunaan yang detail. Semua komponen ini dikemas secara aman dalam peti kayu yang telah diberi perlakuan khusus, memberikan perlindungan maksimal selama transportasi. Hal ini memastikan bahwa instrumen yang sangat sensitif ini tiba di lokasi dalam kondisi optimal, siap untuk memberikan kinerja terbaiknya sejak hari pertama.
Implementasi alat uji kandungan garam ini dalam protokol kontrol kualitas merupakan investasi strategis yang memberikan keuntungan jangka panjang. Dengan memonitor tingkat garam secara akurat, kilang dapat mengoptimalkan kinerja unit desalter, mengurangi penggunaan bahan kimia, meminimalkan waktu henti akibat perawatan, dan memperpanjang umur aset operasional. Pada akhirnya, kontrol yang ketat terhadap kontaminan garam memastikan bahwa minyak mentah yang diproses memenuhi spesifikasi yang disyaratkan, menghasilkan produk akhir yang lebih berkualitas dan menjaga profitabilitas perusahaan di pasar yang sangat kompetitif.
The analysis of salt content in crude oil is a crucial procedure that serves as the frontline defense in protecting the operational integrity of oil refineries. This instrument is specifically designed to provide a reliable and accurate method for determining the concentration of chlorides or salts in crude oil samples. By operating in accordance with globally recognized industry standards, namely ASTM D3230 and IP 265, this device ensures that every test result is dependable for making critical decisions regarding desalination processes and corrosion prevention. Precise measurement is key to avoiding damage to vital and high value equipment such as heat exchangers, distillation columns, and piping systems.
The device utilizes a sensitive electrode assembly and test leads connected to a modern digital auto ranging meter. This technology allows for a precise and automatic reading of voltage and current, which forms the basis for calculating salt content. Its capability to measure across a wide concentration range, from 0 to 500 mg/kg or equivalent to 0 to 150 lb/1000 bbl, makes it highly flexible for analyzing various types of crude oil from different sources. This broad measurement range ensures the instrument is relevant for use from the exploration stage through to the refining process.
The instrument's design prioritizes ease of use and stability during testing. Equipped with a sturdy supporter and holder, the entire glassware set, including the extractor and triangle bottle, can be securely assembled to ensure the extraction and measurement process runs smoothly. The main control unit features a simple interface, allowing operators to focus on sample preparation and result logging with maximum efficiency. This ergonomic design minimizes setup time and maximizes laboratory productivity.
Each unit is delivered as a comprehensive turnkey solution, including all the necessary accessories to begin testing immediately. The purchase package includes the main part, essential glassware, spare fuses, as well as a detailed certification and user manual. All these components are securely packed in a specially treated wooden crate, providing maximum protection during transit. This ensures that this highly sensitive instrument arrives on site in optimal condition, ready to deliver its best performance from day one.
Implementing this salt content tester in quality control protocols is a strategic investment that yields long term benefits. By accurately monitoring salt levels, refineries can optimize desalter unit performance, reduce chemical usage, minimize downtime due to maintenance, and extend the life of operational assets. Ultimately, strict control over salt contaminants ensures that the processed crude oil meets required specifications, resulting in higher quality final products and safeguarding company profitability in a highly competitive market.

