Memperkenalkan sebuah ekosistem akuisisi data (DAQ) yang revolusioner dan sepenuhnya modular dirancang untuk membawa setiap laboratorium eksperimental ke era digital Paket standar modul umum ini menyediakan perangkat yang fleksibel dan kuat untuk mengubah eksperimen fisika tradisional menjadi penyelidikan berbasis data yang modern dan akurat Sistem ini memungkinkan pengumpulan analisis dan pemrosesan data sensor dengan cara yang sebelumnya hanya mungkin dilakukan di laboratorium penelitian canggih
Inti dari ekosistem ini adalah Data Logger M01 yang ringkas dan bertenaga Ini berfungsi sebagai pusat komando yang berkomunikasi dengan PC melalui koneksi USB tunggal yang juga menyediakan daya sehingga tidak memerlukan sumber daya eksternal Dengan laju sampling maksimum hingga 80K Data Logger ini mampu menangkap fenomena fisika yang cepat dengan presisi tinggi dan mendukung pengumpulan data paralel hingga empat kanal secara bersamaan
Fleksibilitas adalah kekuatan terbesar dari sistem modular ini Pengguna dapat memilih antara koneksi kabel yang andal atau kebebasan nirkabel Antarmuka BT M02 memungkinkan koneksi hot-plug hingga empat sensor secara bersamaan melalui kabel Untuk kebebasan total Antarmuka Nirkabel M03 dan Pemancar Nirkabel M04 memungkinkan komunikasi tanpa kabel antara sensor dan Data Logger ideal untuk eksperimen yang melibatkan objek bergerak atau untuk mengurangi kerumitan kabel di meja lab
Sistem ini mendukung pengumpulan data multi-kanal yang komprehensif Baik antarmuka kabel maupun nirkabel dapat terhubung dengan hingga empat sensor yang berbeda secara serentak Hal ini membuka kemungkinan tak terbatas bagi mahasiswa untuk menyelidiki hubungan antara berbagai besaran fisika secara real-time misalnya mengukur posisi kecepatan dan percepatan dari suatu objek bergerak secara simultan untuk verifikasi hukum gerak secara mendalam
Alur kerja data dirancang untuk efisiensi dan portabilitas Modul Tampilan Data M05 yang ditenagai baterai dapat terhubung langsung ke sensor secara otomatis mengidentifikasi jenisnya dan menyimpan data eksperimen di lapangan Kemudian data yang tersimpan ini dapat dengan mudah ditransfer ke PC menggunakan Konektor Input Data M06 untuk analisis mendalam menggunakan perangkat lunak yang disertakan
Secara keseluruhan paket modul umum ini adalah toolkit utama untuk memodernisasi laboratorium pengajaran Kombinasi kinerja tinggi fleksibilitas kabel atau nirkabel dukungan multi-kanal dan fitur ramah pengguna seperti hot-plugging dan port self-locking menjadikannya investasi yang kuat terukur dan tahan masa depan untuk setiap institusi yang berkomitmen untuk mengajarkan metode eksperimental ilmiah kontemporer
Introducing a revolutionary and fully modular data acquisition (DAQ) ecosystem designed to bring any experimental laboratory into the digital age This standard package of common modules provides a flexible and powerful toolkit to transform traditional physics experiments into modern accurate data-driven investigations This system enables the collection analysis and processing of sensor data in a way previously only possible in advanced research laboratories
The core of this ecosystem is the compact and powerful M01 Data Logger It serves as the central hub communicating with a PC via a single USB connection which also provides its power eliminating the need for an external power source With a maximum sampling rate of up to 80K this Data Logger is capable of capturing fast physical phenomena with high precision and supports parallel data collection on up to four channels simultaneously
Flexibility is the greatest strength of this modular system Users can choose between a reliable wired connection or the freedom of wireless The M02 BT Interface allows for the hot-plug connection of up to four different sensors simultaneously via cable For total freedom the M03 Wireless Interface and M04 Wireless Transmitter enable cable-free communication between the sensors and the Data Logger ideal for experiments involving moving objects or for reducing cable clutter on the lab bench
The system supports comprehensive multi-channel data collection Both the wired and wireless interfaces can connect with up to four different sensors at once This opens up limitless possibilities for students to investigate the relationships between various physical quantities in real-time for example measuring the position velocity and acceleration of a moving object simultaneously for an in-depth verification of the laws of motion
The data workflow is designed for efficiency and portability The battery-powered M05 Data Display Module can connect directly to a sensor automatically identify its type and save experimental data in the field Then this stored data can be easily transferred to a PC using the M06 Data Input Connector for in-depth analysis using the assorted software
Overall this package of common modules is the ultimate toolkit for modernizing a teaching laboratory The combination of high performance wired or wireless flexibility multi-channel support and user-friendly features like hot-plugging and self-locking ports makes it a powerful scalable and future-proof investment for any institution committed to teaching contemporary scientific experimental methods

