Dalam industri alas kaki yang sangat kompetitif, terutama pada segmen sepatu hak tinggi wanita, reputasi sebuah merek bergantung pada keamanan dan daya tahan produknya. Sebuah hak sepatu yang patah tidak hanya menyebabkan ketidaknyamanan, tetapi juga berisiko mencederai pengguna dan merusak kepercayaan konsumen secara permanen. Untuk menjawab tantangan krusial ini, kami menyediakan sebuah mesin uji benturan dan kelelahan hak sepatu. Alat ini merupakan solusi rekayasa yang dirancang untuk secara sistematis menguji integritas struktural dan ketahanan hak sepatu melalui benturan berulang yang terkontrol, memastikan setiap pasang sepatu yang diproduksi memenuhi standar kualitas dan keamanan tertinggi sebelum sampai ke tangan konsumen.
Peralatan pengujian ini secara spesifik mensimulasikan tekanan dan guncangan yang dialami hak sepatu selama penggunaan sehari-hari. Dengan frekuensi dan energi benturan yang telah ditentukan, mesin ini secara terus menerus memukul hak sepatu hingga titik retak atau kegagalan struktural terjadi. Melalui proses ini, produsen dapat memperoleh data kuantitatif mengenai indeks ketahanan benturan dan umur pakai dari desain hak sepatu mereka. Informasi ini sangat berharga dalam tahap riset dan pengembangan untuk inovasi material, perbaikan desain, serta sebagai alat kontrol kualitas esensial pada lini produksi massal untuk menjamin konsistensi mutu.
Dirancang untuk presisi dan kemudahan operasional, mesin uji ini dilengkapi dengan penghitung digital LCD yang akurat untuk memonitor jumlah siklus benturan hingga jutaan kali. Fleksibilitas pengujian dijamin melalui rentang penyesuaian spesimen yang luas, memungkinkan pengaturan posisi, ketinggian, dan sudut pengujian dari 0 hingga 180 derajat untuk mengakomodasi beragam model dan desain hak sepatu. Kepatuhannya terhadap standar industri terkemuka seperti BS-5131 dan SATRA PM20 memastikan bahwa setiap hasil pengujian yang didapatkan memiliki validitas dan pengakuan internasional, memberikan keunggulan kompetitif dan mempermudah proses sertifikasi produk untuk pasar global.
Mengintegrasikan mesin uji ketahanan hak sepatu ini ke dalam proses quality assurance Anda adalah sebuah investasi strategis dalam melindungi nilai merek dan kepuasan pelanggan. Ini adalah komitmen nyata untuk tidak hanya menciptakan desain yang estetis tetapi juga produk yang aman, andal, dan tahan lama. Dengan data uji yang solid, Anda dapat dengan percaya diri mengklaim keunggulan produk, mengurangi tingkat pengembalian barang, dan membangun loyalitas pelanggan yang kuat. Pastikan setiap langkah pelanggan Anda aman dan penuh gaya dengan produk yang telah teruji ketahanannya secara menyeluruh.
In the highly competitive footwear industry, particularly in the women's high-heeled shoe segment, a brand's reputation hinges on the safety and durability of its products. A broken heel not only causes discomfort but also risks injuring the user and permanently damaging consumer trust. To address this crucial challenge, we provide a shoe heel impact and fatigue testing machine. This instrument is an engineered solution designed to systematically test the structural integrity and endurance of shoe heels through controlled, repetitive impacts, ensuring every pair produced meets the highest quality and safety standards before reaching the consumer.
This testing equipment specifically simulates the stress and shocks a shoe heel experiences during daily use. With a predetermined impact frequency and energy, the machine continuously strikes the heel until a crack or structural failure occurs. Through this process, manufacturers can obtain quantitative data on the impact resistance index and the service life of their heel designs. This information is invaluable during the research and development phase for material innovation, design improvements, and as an essential quality control tool on the mass production line to guarantee consistent quality.
Designed for precision and operational ease, this testing machine is equipped with an accurate LCD digital counter to monitor impact cycles up to the millions. Testing flexibility is assured through a wide specimen adjustment range, allowing for positional, height, and angular adjustments from 0 to 180 degrees to accommodate various heel models and designs. Its compliance with leading industry standards such as BS-5131 and SATRA PM20 ensures that every test result obtained has international validity and recognition, providing a competitive edge and simplifying the product certification process for the global market.
Integrating this shoe heel resistance tester into your quality assurance process is a strategic investment in protecting your brand value and customer satisfaction. It represents a tangible commitment to creating not only aesthetically pleasing designs but also safe, reliable, and durable products. With solid test data, you can confidently claim product superiority, reduce return rates, and build strong customer loyalty. Ensure every step your customers take is safe and stylish with a product that has been thoroughly tested for its endurance.

