Memastikan setiap langkah yang diambil pelanggan adalah langkah yang aman dan nyaman merupakan prioritas utama dalam industri alas kaki. Kualitas sebuah sepatu seringkali dinilai dari daya tahannya, terutama pada bagian sol dalam yang menjadi tumpuan utama. Kami menghadirkan sebuah solusi rekayasa presisi tinggi, sebuah mesin pengujian yang dirancang khusus untuk mensimulasikan penggunaan berulang kali dan mengukur ketahanan lentur fiberboard sol dalam secara akurat. Alat ini adalah garda terdepan Anda dalam menjaga reputasi merek dan memastikan setiap produk yang keluar dari lini produksi Anda memenuhi standar kualitas tertinggi. Dengan kemampuan pengujian yang ketat, Anda dapat dengan percaya diri memberikan jaminan durabilitas kepada pasar.
Mesin ini bekerja dengan meniru gerakan menekuk dinamis hingga sudut 90 derajat secara konstan dan berulang pada spesimen sol dalam. Pengujian ini dilakukan tanpa henti hingga titik di mana material mengalami kerusakan atau patah. Jumlah siklus tekukan yang berhasil dilalui sebelum terjadi kerusakan menjadi data kuantitatif yang sangat berharga untuk menilai performa ketahanan lentur material. Dengan kecepatan 60 siklus per menit, proses pengujian berlangsung efisien, memungkinkan Anda mendapatkan hasil dalam waktu singkat. Ini bukan sekadar pengujian, melainkan sebuah proses validasi untuk memastikan material yang Anda gunakan mampu menahan tekanan penggunaan sehari hari, dari sepatu kulit formal hingga sepatu kasual yang dinamis.
Dirancang untuk efisiensi maksimal di lingkungan industri, alat ini dilengkapi dengan enam stasiun pengujian yang beroperasi secara simultan. Kapasitas ini memungkinkan Anda menguji hingga enam sampel sekaligus, secara drastis mengurangi waktu yang dibutuhkan untuk kontrol kualitas dan mempercepat proses pengembangan produk. Setiap stasiun pengujian dilengkapi dengan grip atas dan beban presisi seberat 2 kilogram pada grip bawah, memastikan kondisi pengujian yang seragam dan dapat diandalkan. Didukung oleh motor DC yang stabil dan hening, serta penghitung digital LCD canggih yang mampu merekam hingga 999,999 siklus untuk tujuh grup data, setiap detail pengujian tercatat dengan akurasi tanpa kompromi.
Keandalan operasional adalah kunci. Dengan bobot 149 kilogram, mesin ini menawarkan stabilitas superior selama pengoperasian, menghilangkan getaran yang dapat mempengaruhi hasil tes. Dimensi mesin yang terukur memastikan alat ini dapat diintegrasikan dengan mudah ke dalam ruang laboratorium atau area kontrol kualitas Anda tanpa memakan banyak tempat. Beroperasi pada daya listrik standar AC 220V, instalasi dan penggunaannya menjadi sangat praktis. Investasi pada perangkat ini bukan hanya tentang membeli sebuah mesin, tetapi tentang membangun fondasi kepercayaan pelanggan melalui produk alas kaki yang terbukti andal, kuat, dan tahan lama.
Ensuring that every step a customer takes is safe and comfortable is a top priority in the footwear industry. The quality of a shoe is often judged by its durability, especially the insole which serves as the primary foundation. We present a high precision engineered solution, a testing machine specifically designed to simulate repeated use and accurately measure the flexing resistance of insole fiberboard. This instrument is your frontline defense in protecting brand reputation and ensuring every product leaving your production line meets the highest quality standards. With its rigorous testing capabilities, you can confidently provide a guarantee of durability to the market.
This machine operates by mimicking a dynamic 90 degree bending motion constantly and repeatedly on insole specimens. This test is performed relentlessly until the point of material failure or breakage. The number of flexing cycles successfully completed before failure becomes invaluable quantitative data for assessing the material's flexing resistance performance. With a speed of 60 cycles per minute, the testing process is efficient, allowing you to obtain results in a short amount of time. This is not just a test; it is a validation process to ensure the materials you use can withstand the pressures of daily wear, from formal leather shoes to dynamic leisure shoes.
Engineered for maximum efficiency in an industrial setting, this device is equipped with six testing stations that operate simultaneously. This capacity allows you to test up to six samples at once, drastically reducing quality control time and accelerating your product development cycle. Each testing station is fitted with an upper grip and a precise 2 kilogram weight on the lower grip, ensuring uniform and reliable testing conditions. Powered by a stable and quiet DC motor, and featuring an advanced LCD digital counter capable of recording up to 999,999 cycles for seven data groups, every detail of the test is captured with uncompromising accuracy.
Operational reliability is key. Weighing 149 kilograms, this machine offers superior stability during operation, eliminating vibrations that could affect test results. Its measured dimensions ensure that the instrument can be easily integrated into your laboratory or quality control area without occupying excessive space. Operating on standard AC 220V power, its installation and use are incredibly practical. Investing in this device is not just about buying a machine; it's about building a foundation of customer trust through footwear products that are proven to be reliable, strong, and long lasting.

