Di setiap lingkungan, baik itu area kerja industri, fasilitas medis, maupun area publik, keamanan pengguna adalah hal yang tidak bisa ditawar. Risiko tergelincir dan jatuh menjadi perhatian utama, dan fondasi dari keamanan tersebut terletak pada daya cengkeram alas kaki. Kami mempersembahkan sebuah perangkat pengujian esensial yang dirancang untuk mengukur secara kuantitatif tingkat ketahanan slip atau gesekan pada sol dan hak sepatu. Mesin ini bukan sekadar alat, melainkan sebuah komitmen terhadap keselamatan konsumen dan integritas merek Anda. Dengan melakukan pengujian sesuai standar industri global yang diakui, Anda dapat dengan penuh percaya diri menyatakan bahwa produk Anda aman dan andal.
Fungsi utama dari alat ini adalah untuk menentukan koefisien gesek, memberikan data akurat tentang seberapa baik performa sol dan hak sepatu di berbagai permukaan. Yang terpenting, seluruh prosedur pengujiannya dirancang untuk memenuhi standar internasional ASTM F 609. Kepatuhan terhadap standar ini memastikan bahwa hasil pengujian Anda valid, dapat dipertanggungjawabkan, dan diakui secara global. Ini adalah elemen krusial untuk menembus pasar yang kompetitif, memenuhi regulasi keselamatan, dan melindungi perusahaan dari potensi tuntutan hukum akibat kecelakaan produk.
Keunggulan teknis menjadi inti dari perangkat ini. Dengan kapasitas pengukuran gaya hingga 50 Kg (setara Newton) dan akurasi beban yang luar biasa hingga 0.01 Kg, setiap pengujian menghasilkan data yang sangat presisi. Resolusi tinggi 1/1000 menjamin tidak ada detail performa gesekan yang terlewatkan. Proses pengujian dilakukan pada kecepatan yang terkontrol dan terstandarisasi, yaitu 3.5±0.5 inci per menit, memastikan setiap tes dapat direplikasi dengan hasil yang konsisten. Semua data penting, termasuk nilai pengujian saat ini dan nilai puncak (peak value), ditampilkan dengan jelas pada layar digital, memudahkan operator untuk analisis dan pencatatan.
Dibangun dengan kokoh dan bobot 80 Kg, mesin ini menawarkan stabilitas maksimal selama pengujian, sebuah faktor penting untuk mendapatkan hasil yang tidak bias. Desainnya yang ringkas memungkinkan penempatan yang efisien di dalam laboratorium atau area kontrol kualitas. Beroperasi dengan daya listrik standar AC 220V, alat ini siap digunakan untuk mendukung proses riset dan pengembangan, verifikasi material baru, serta audit kualitas rutin pada lini produksi Anda. Berinvestasi pada mesin uji ketahanan slip ini adalah langkah strategis untuk membangun reputasi sebagai produsen yang serius dalam mengutamakan keselamatan dan kualitas.
In any environment, whether it's an industrial workspace, a medical facility, or a public area, user safety is non negotiable. The risk of slips and falls is a primary concern, and the foundation of that safety lies in the grip performance of footwear. We present an essential testing device engineered to quantitatively measure the slide resistance or friction level of shoe soles and heels. This machine is more than just an instrument; it is a commitment to consumer safety and your brand's integrity. By conducting tests that comply with globally recognized industry standards, you can confidently declare your products as safe and reliable.
The core function of this device is to determine the coefficient of friction, providing precise data on how well shoe soles and heels perform on various surfaces. Most importantly, its entire testing procedure is designed to meet the international standard ASTM F 609. Compliance with this standard ensures that your test results are valid, accountable, and globally recognized. This is a crucial element for penetrating competitive markets, meeting safety regulations, and protecting your company from potential liability claims arising from product related accidents.
Technical excellence is at the heart of this device. With a force measurement capacity of up to 50 Kg (or its Newton equivalent) and an exceptional load accuracy of 0.01 Kg, every test yields highly precise data. A high resolution of 1/1000 guarantees that no detail of the frictional performance is missed. The testing process is conducted at a controlled and standardized speed of 3.5±0.5 inches per minute, ensuring that every test is replicable with consistent outcomes. All critical data, including the current testing value and the peak value, is clearly displayed on a digital screen, facilitating easy analysis and recording for the operator.
Built robustly with a weight of 80 Kg, this machine offers maximum stability during testing, a vital factor for obtaining unbiased results. Its compact design allows for efficient placement within a laboratory or quality control area. Operating on standard AC 220V power, this device is ready to support your research and development processes, new material verifications, and routine quality audits on your production line. Investing in this slip resistance tester is a strategic move to build a reputation as a manufacturer that seriously prioritizes safety and quality.

