Sebuah sepatu lebih dari sekadar gabungan sol, bagian atas, dan tali; ia adalah sebuah sistem terintegrasi yang harus mampu menahan tekanan dinamis dari setiap langkah. Kegagalan satu komponen dapat merusak keseluruhan produk dan reputasi merek. Untuk itu, kami menghadirkan solusi pengujian tingkat lanjut yang melampaui tes material individual. Ini adalah mesin pengujian ketahanan untuk sepatu jadi, yang dirancang untuk mensimulasikan kondisi berjalan kaki seseorang secara realistis. Alat ini secara akurat menentukan daya tahan kelelahan (fatigue durability) dan memprediksi umur pakai sepatu dengan subjecting produk jadi ke siklus lentur yang berulang-ulang, memungkinkan Anda melihat dengan tepat bagaimana performa produk di dunia nyata.
Dengan beroperasi sesuai standar desain internasional SATRA-TM92, mesin ini memberikan hasil yang tidak hanya andal tetapi juga diakui di seluruh industri alas kaki global. Fungsinya adalah untuk secara proaktif mengidentifikasi titik-titik lemah dalam desain dan konstruksi. Setelah ribuan siklus pengujian, Anda dapat mengobservasi secara detail kondisi kerusakan, posisi retakan pada sol, atau kelemahan pada sambungan. Informasi ini sangat krusial bagi tim riset dan pengembangan untuk melakukan perbaikan, meningkatkan kualitas, dan pada akhirnya, menciptakan produk yang superior yang mampu melampaui ekspektasi pelanggan.
Efisiensi dan fleksibilitas adalah inti dari desain rekayasa mesin ini. Dengan kapasitas untuk menguji empat sepatu secara simultan, Anda dapat secara signifikan mempercepat proses kontrol kualitas dan validasi produk. Kemampuan untuk menyesuaikan sudut lentur (30°, 54°, 50°, 60°, 90°) dan kecepatan tes (50-150 siklus per menit) memberikan fleksibilitas tak tertandingi untuk menguji berbagai jenis sepatu, mulai dari sepatu lari yang fleksibel hingga sepatu bot kerja yang kaku, sesuai dengan standar pengujian yang berbeda. Alat ini dapat mengakomodasi sepatu dengan panjang 150 hingga 400 mm, mencakup hampir semua ukuran sepatu dewasa.
Didukung oleh motor DC 1/2HP yang bertenaga dan stabil, serta dibangun di atas rangka kokoh dengan berat sekitar 236 Kg, mesin ini menjamin operasi yang bebas getaran untuk hasil yang konsisten. Penghitung digital LCD presisi tinggi mampu merekam hingga 999,999 siklus lentur, memungkinkan Anda melakukan tes daya tahan jangka panjang yang komprehensif. Menempatkan mesin ini sebagai bagian dari proses jaminan kualitas Anda adalah sebuah pernyataan tegas. Ini menunjukkan komitmen Anda untuk tidak hanya menjual sepatu, tetapi juga untuk memberikan jaminan daya tahan, kenyamanan, dan keandalan dalam setiap pasang produk yang Anda kirimkan ke pasar.
A shoe is more than just a combination of a sole, an upper, and laces; it is an integrated system that must withstand the dynamic stresses of every single step. The failure of one component can compromise the entire product and a brand's reputation. To address this, we introduce an advanced testing solution that goes beyond individual material tests. This is a flexing tester for finished shoes, designed to realistically simulate a person's walking state. It accurately determines fatigue durability and predicts the service life of shoes by subjecting the final product to repeated flexing cycles, allowing you to see exactly how it will perform in the real world.
By operating in accordance with the international design standard SATRA-TM92, this machine provides results that are not only reliable but also recognized throughout the global footwear industry. Its function is to proactively identify weak points in design and construction. After thousands of test cycles, you can observe in detail any damage conditions, the position of cracks on the sole, or weaknesses in joints. This information is invaluable for R&D teams to make improvements, enhance quality, and ultimately, create a superior product that exceeds customer expectations.
Efficiency and versatility are at the core of this machine's engineering. With the capacity to test four shoes simultaneously, you can significantly accelerate your quality control and product validation processes. The ability to adjust the flexing angle (30°, 54°, 50°, 60°, 90°) and test speed (50-150 cycles per minute) provides unparalleled flexibility to test a wide variety of footwear, from flexible running shoes to rigid work boots, according to different testing standards. The device accommodates shoe lengths from 150 to 400 mm, covering nearly all adult shoe sizes.
Powered by a robust and stable 1/2HP DC motor and built on a solid frame weighing approximately 236 Kg, this machine ensures vibration-free operation for consistent results. A high-precision LCD digital counter can record up to 999,999 flexing cycles, enabling you to conduct comprehensive long-term endurance tests. Placing this machine as a cornerstone of your quality assurance process is a powerful statement. It demonstrates your commitment not just to selling shoes, but to delivering guaranteed durability, comfort, and reliability in every pair you send to market.

