Warna adalah elemen paling vital dari identitas produk, namun persepsinya dapat berubah secara drastis di bawah kondisi pencahayaan yang berbeda. Kesalahan pencocokan warna antara produksi, pemasok, dan titik penjualan dapat menyebabkan penolakan produk yang mahal dan merusak citra merek. Kami menghadirkan solusi definitif: sebuah kabinet evaluasi warna yang menyediakan lingkungan pencahayaan yang terstandarisasi dan terkontrol. Alat ini adalah instrumen fundamental bagi desainer, produsen, dan manajer quality control untuk membuat penilaian warna visual secara objektif, memastikan konsistensi warna dari konsep hingga ke tangan konsumen.
Fungsi utama dari kabinet ini adalah untuk secara akurat mensimulasikan berbagai lingkungan pencahayaan, memungkinkan Anda untuk membandingkan variasi warna dan corak dengan presisi. Yang terpenting, alat ini adalah senjata ampuh untuk mendeteksi metamerisme—sebuah fenomena di mana dua warna tampak cocok di bawah satu jenis cahaya, tetapi terlihat berbeda di bawah cahaya lain. Dengan dilengkapi enam sumber cahaya standar industri (termasuk D65, TL84, UV, F, CWF, U30), Anda dapat dengan cepat memverifikasi apakah warna produk Anda akan tetap konsisten di siang hari, di dalam toko ritel Eropa, di bawah lampu kantor Amerika, atau di rumah. Kepatuhannya terhadap standar internasional utama seperti ASTM D1729 dan ISO 3664 memberikan jaminan bahwa evaluasi Anda sah dan diakui secara global.
Efisiensi dan akurasi operasional menjadi inti dari desainnya. Teknologi start elektronik frekuensi tinggi memastikan cahaya menyala secara instan tanpa berkedip, memberikan penilaian warna yang nyaman dan cepat. Timer individual untuk setiap sumber cahaya secara otomatis melacak masa pakai lampu, memberi tahu Anda waktu yang tepat untuk penggantian guna menjaga akurasi spektral. Fitur ini sangat penting untuk hasil yang konsisten dari waktu ke waktu. Sumber cahaya UV yang disertakan juga krusial untuk mengidentifikasi adanya pencerah optik (OBA) pada tekstil, kertas, dan plastik, yang tidak terlihat di bawah cahaya normal.
Aplikasi alat ini sangat luas, menjadikannya aset tak ternilai di berbagai industri termasuk tekstil, pencelupan, percetakan, pengemasan, plastik, kulit, cat, tinta, otomotif, dan keramik. Dengan mengintegrasikan kabinet evaluasi warna ini ke dalam alur kerja Anda, Anda tidak lagi menebak-nebak. Anda mengeliminasi perselisihan warna, mempercepat proses persetujuan, dan menjaga integritas merek Anda. Ini adalah investasi esensial untuk memastikan bahwa warna yang Anda rancang dengan cermat adalah warna yang dilihat oleh seluruh dunia.
Color is the most vital element of product identity, yet its perception can change dramatically under different lighting conditions. A color mismatch between production, suppliers, and the point of sale can lead to costly product rejections and damage a brand's image. We present the definitive solution: a color assessment cabinet that provides a standardized and controlled lighting environment. This is the fundamental instrument for designers, manufacturers, and quality control managers to make objective visual color assessments, ensuring color consistency from concept to consumer.
The primary function of this cabinet is to accurately simulate various lighting environments, allowing you to compare color and shade variations with precision. Most importantly, it is a powerful tool for detecting metamerism—a phenomenon where two colors appear to match under one light source but look different under another. Equipped with six industry-standard light sources (including D65, TL84, UV, F, CWF, U30), you can quickly verify if your product's color will remain consistent in daylight, within a European retail store, under an American office light, or in a home setting. Its compliance with major international standards like ASTM D1729 and ISO 3664 provides assurance that your evaluations are legitimate and globally recognized.
Operational efficiency and accuracy are at the core of its design. Electronic high-frequency start technology ensures instant, flicker-free illumination for comfortable and rapid color judgment. Individual timers for each light source automatically track lamp life, prompting you for timely replacement to maintain spectral accuracy—a critical feature for consistent results over time. The included UV light source is also crucial for identifying the presence of optical brightening agents (OBAs) in textiles, papers, and plastics, which are invisible under normal light.
The application of this tool is vast, making it an invaluable asset across numerous industries including textiles, dyeing, printing, packaging, plastics, leather, paints, inks, automotive, and ceramics. By integrating this color assessment cabinet into your workflow, you are no longer guessing. You are eliminating color disputes, accelerating approval processes, and safeguarding your brand's integrity. It is an essential investment to ensure the color you meticulously designed is the color the world sees.

