Di dunia nyata, produk karet dan elastomer secara konstan diserang oleh musuh tak terlihat di atmosfer: ozon. Paparan jangka panjang, bahkan pada konsentrasi rendah, dapat menyebabkan keretakan yang merusak, mengurangi umur pakai produk, dan berpotensi menyebabkan kegagalan fungsi yang berbahaya. Kami mempersembahkan sebuah solusi rekayasa canggih, Ozone Aging Test Chamber, yang berfungsi sebagai "mesin waktu" untuk material Anda. Alat ini mensimulasikan efek penuaan akibat ozon selama bertahun-tahun hanya dalam hitungan hari atau minggu, memberikan Anda data penting untuk memprediksi durabilitas dan memastikan keandalan produk Anda di lapangan.
Kredibilitas pengujian Anda adalah prioritas utama. Oleh karena itu, chamber ini dirancang untuk melakukan pengujian sesuai dengan serangkaian lengkap standar internasional yang paling dihormati dan umum digunakan dalam industri karet. Ini termasuk, namun tidak terbatas pada, ASTM D1149, ISO 1431, JIS K 6259, dan DIN 53509. Kemampuan untuk menguji sesuai standar global ini memastikan bahwa hasil Anda valid, dapat direplikasi, dan diakui oleh pelanggan di seluruh dunia. Chamber ini menciptakan lingkungan yang sangat terkontrol dengan konsentrasi ozon, suhu, dan aliran udara yang presisi, memungkinkan Anda mengevaluasi ketahanan retak material dalam kondisi statis maupun dinamis.
Dilengkapi dengan teknologi modern untuk pengoperasian yang mudah dan hasil yang akurat, chamber ini dikendalikan oleh kontroler layar sentuh yang dapat diprogram. Fitur ini memungkinkan Anda untuk dengan mudah mengatur siklus pengujian yang kompleks dan membiarkannya berjalan secara otomatis. Interior yang terbuat dari baja tahan karat SUS 304 memastikan daya tahan terhadap lingkungan ozon yang korosif dan tidak akan mengganggu hasil pengujian. Rak sampel yang berputar menjamin bahwa setiap bagian dari spesimen uji menerima paparan ozon yang seragam, menghilangkan variabel dan meningkatkan keandalan data Anda. Tersedia dalam berbagai ukuran, chamber ini dapat memenuhi kebutuhan dari laboratorium riset dan pengembangan hingga fasilitas kontrol kualitas produksi skala besar.
Alat ini merupakan instrumen yang tak ternilai bagi produsen di berbagai sektor, termasuk otomotif (selang, seal, sabuk), industri ban, kabel, alas kaki, dan komponen karet teknis lainnya. Dengan menggunakan ozone aging test chamber, Anda dapat mempercepat pengembangan formulasi kompon baru, melakukan audit kualitas pada bahan baku yang masuk, dan memberikan jaminan performa jangka panjang kepada pelanggan Anda. Ini adalah investasi strategis dalam kualitas, keandalan, dan reputasi merek Anda di pasar yang kompetitif.
In the real world, rubber and elastomer products are under constant attack from an invisible enemy in the atmosphere: ozone. Long-term exposure, even to low concentrations, can cause devastating cracking, reducing a product's service life and potentially leading to dangerous functional failures. We present an advanced engineering solution, the Ozone Aging Test Chamber, which acts as a "time machine" for your materials. This chamber simulates the aging effects of years of ozone exposure in a matter of days or weeks, providing you with the critical data to predict durability and ensure the reliability of your products in the field.
The credibility of your testing is paramount. Therefore, this chamber is designed to perform tests in accordance with a comprehensive suite of the most respected and widely used international standards in the rubber industry. These include, but are not limited to, ASTM D1149, ISO 1431, JIS K 6259, and DIN 53509. The ability to test to these global standards ensures your results are valid, replicable, and recognized by customers worldwide. The chamber creates a highly controlled environment with precise ozone concentration, temperature, and airflow, allowing you to evaluate the crack resistance of materials under both static and dynamic conditions.
Equipped with modern technology for easy operation and accurate results, the chamber is managed by a programmable touch screen controller. This feature allows you to effortlessly set up complex test cycles and let them run automatically. The interior, constructed from SUS 304 stainless steel, ensures durability against the corrosive ozone environment and will not interfere with test results. A rotating sample shelf guarantees that every part of the test specimen receives uniform ozone exposure, eliminating variables and increasing the reliability of your data. Available in various sizes, this chamber can meet the needs of small R&D labs to large-scale production quality control facilities.
This instrument is invaluable for manufacturers across numerous sectors, including automotive (hoses, seals, belts), the tire industry, cables, footwear, and other technical rubber components. By using an ozone aging test chamber, you can accelerate the development of new compound formulations, perform quality audits on incoming raw materials, and provide a long-term performance guarantee to your customers. It is a strategic investment in the quality, reliability, and reputation of your brand in a competitive market.

