Tingkatkan standar kualitas produk Anda dengan mesin uji ketahanan tekuk kami yang dirancang secara superior. Alat ini merupakan solusi fundamental untuk mengevaluasi kekuatan dan daya tahan esensial dari berbagai material pada suhu ruangan. Diciptakan khusus untuk industri yang mengandalkan kualitas bahan seperti kulit, lapisan kain, dan material sejenis lainnya, mesin ini secara akurat mengidentifikasi ketahanan material terhadap goresan, retakan, dan kelelahan akibat penggunaan berulang, memastikan setiap produk yang Anda hasilkan memenuhi ekspektasi tertinggi.
Mekanisme pengujian pada alat ini sangat efisien dan mudah dioperasikan. Sampel material dipasang dengan cermat pada fixture, di mana satu sisi berfungsi sebagai permukaan dalam dan sisi lainnya sebagai permukaan luar untuk mereplikasi kondisi pemakaian nyata. Mesin kemudian secara konsisten melakukan gerakan tekukan berulang pada sampel. Anda memiliki fleksibilitas untuk menentukan durasi pengujian atau secara aktif mengamati jumlah siklus yang dibutuhkan hingga material mencapai titik kerusakan, memberikan data yang akurat dan dapat diandalkan.
Keunggulan teknis menjadi inti dari performa alat ini, dilengkapi dengan layar LCD digital canggih yang menampilkan penghitungan siklus secara presisi hingga 999999 kali dan didukung fitur mati otomatis untuk efisiensi. Dengan kecepatan pengujian stabil 100±5 putaran per menit dan sudut tekuk optimal 22.5 derajat, setiap hasil uji dijamin konsisten. Fleksibilitas pengujian ditingkatkan dengan opsi konfigurasi untuk 6 atau 12 grup spesimen secara bersamaan, memungkinkan Anda mempercepat proses kontrol kualitas secara signifikan.
Jadikan mesin ini sebagai investasi strategis untuk menjamin keunggulan kompetitif produk Anda di pasar. Dengan konstruksi yang solid dan didukung oleh power AC220V 20A, alat ini dirancang untuk penggunaan jangka panjang dalam lingkungan industri yang dinamis. Pemenuhan standar desain internasional yang ketat seperti BS 3144 dan JIB K6545 menegaskan komitmen kami pada kualitas dan presisi. Pastikan hanya material dengan daya tahan teruji yang menjadi bagian dari produk akhir Anda, membangun reputasi merek yang identik dengan kualitas superior.
Elevate your product's quality standards with our superbly engineered flexing resistance tester. This machine is the fundamental solution for evaluating the essential strength and durability of various materials at room temperature. Created specifically for industries that depend on the quality of materials like leather, lining, fabric, and other similar items, this machine accurately identifies a material's resistance to scratching, cracking, and fatigue from repeated use, ensuring every product you create meets the highest expectations.
The testing mechanism on this device is highly efficient and user friendly. A material sample is carefully mounted onto the fixture, where one side acts as the inner surface and the other as the outer to replicate real world conditions. The machine then consistently performs repetitive bending motions on the sample. You have the flexibility to set the test duration or actively observe the number of cycles required until the material reaches its failure point, providing accurate and dependable data.
Technical excellence is at the core of this machine's performance, equipped with an advanced digital LCD that precisely displays the cycle count up to 999999 and is supported by an automatic shutdown feature for efficiency. With a stable testing speed of 100±5 cycles per minute and an optimal bending angle of 22.5 degrees, every test result is guaranteed to be consistent. Testing flexibility is enhanced with configuration options for 6 or 12 specimen groups simultaneously, allowing you to significantly accelerate your quality control process.
Make this machine a strategic investment to secure your product's competitive edge in the market. With a solid construction and powered by AC220V 20A, this device is designed for long term use in a dynamic industrial environment. Its compliance with strict international design standards such as BS 3144 and JIB K6545 confirms our commitment to quality and precision. Ensure that only materials with proven durability become part of your final product, building a brand reputation synonymous with superior quality.

