Hadirkan standar kualitas tertinggi pada setiap produk Anda dengan alat uji kelembutan yang dirancang untuk presisi mutlak. Instrumen ini adalah perangkat fundamental bagi industri kulit dan tekstil, ideal untuk mengukur tingkat kelembutan pada kain berlapis, kulit, dan berbagai material lunak lainnya. Mengetahui tingkat kelembutan secara akurat adalah kunci untuk memastikan konsistensi produk, kenyamanan pengguna, dan nilai estetika, menjadikan alat ini investasi krusial untuk menjaga reputasi brand Anda.
Cara kerja alat ini didasarkan pada metode pengujian yang terstandardisasi dan sangat andal. Sampel material yang akan diuji dijepit dengan aman di atas sebuah lubang dengan diameter yang telah ditentukan. Selanjutnya, sebuah beban spesifik sebesar 500g diaplikasikan secara vertikal melalui pin berdiameter lebih kecil. Defleksi atau tingkat lenturan yang terjadi pada material akibat tekanan tersebut diukur secara presisi oleh alat, memberikan data kuantitatif yang jelas mengenai tingkat kelembutannya.
Setiap detail dari instrumen ini dirancang untuk kemudahan dan akurasi. Dengan rentang pengukuran dial dari 0.1 hingga 110mm, alat ini mampu mengakomodasi berbagai jenis material dengan tingkat kelembutan yang berbeda. Dimensinya yang ringkas (140 x 500 x 170 mm) dan bobotnya yang hanya 5kg membuatnya mudah ditempatkan di laboratorium mana pun tanpa memakan banyak ruang. Yang terpenting, alat ini sepenuhnya mematuhi standar internasional IULTCS IU P/36 dan ISO 17235, menjamin bahwa setiap hasil pengujian Anda valid dan diakui secara global.
Jangan kompromikan kualitas sentuhan akhir produk Anda. Dengan menggunakan alat penguji kelembutan ini, Anda mendapatkan kontrol penuh atas salah satu atribut terpenting dari material Anda. Baik untuk riset dan pengembangan, kontrol kualitas bahan baku, maupun inspeksi produk jadi, instrumen ini memberikan data yang Anda butuhkan untuk membuat keputusan yang tepat. Pastikan setiap produk yang keluar dari lini produksi Anda memiliki tingkat kelembutan yang sempurna dan konsisten sesuai standar.
Introduce the highest standard of quality to every product with our softness tester, designed for absolute precision. This instrument is a fundamental device for the leather and textile industries, ideal for measuring the softness level of coated fabrics, leather, and various other soft materials. Accurately determining the degree of softness is key to ensuring product consistency, user comfort, and aesthetic value, making this tool a crucial investment for protecting your brand's reputation.
The operation of this device is based on a standardized and highly reliable testing method. The material sample to be tested is securely clamped over an aperture of a known diameter. Subsequently, a specific 500g load is applied vertically through a pin of a smaller diameter. The deflection or flex of the material resulting from this pressure is precisely measured by the instrument, providing clear quantitative data on its softness level.
Every detail of this instrument is engineered for convenience and accuracy. With a dial measurement range from 0.1 to 110mm, it can accommodate a wide variety of materials with different softness characteristics. Its compact dimensions (140 x 500 x 170 mm) and light weight of just 5kg make it easy to place in any laboratory without occupying much space. Most importantly, this device fully complies with international standards IULTCS IU P/36 and ISO 17235, guaranteeing that your test results are valid and globally recognized.
Do not compromise on the final touch and feel of your products. By using this softness tester, you gain complete control over one of the most critical attributes of your materials. Whether for research and development, raw material quality control, or final product inspection, this instrument provides the data you need to make informed decisions. Ensure every product leaving your production line has the perfect and consistent level of softness that meets the standard.


