Tentukan standar daya tahan dan kualitas estetika kain Anda dengan Digital Martindale Abrasion and Pilling Machine. Diakui secara global sebagai metode pengujian fundamental, instrumen ini dirancang untuk secara akurat menilai ketahanan kain, terutama tenunan, terhadap abrasi (keausan) dan pilling (timbulnya bulu-bulu halus di permukaan). Untuk produsen furnitur, garmen, tekstil rumah tangga, dan pakaian kerja, mesin ini adalah perangkat esensial untuk menjamin umur panjang dan penampilan produk.
Mesin Martindale secara unik menyimulasikan keausan alami melalui gerakan abrasi multi-arah yang terkontrol. Sampel kain dipasang pada salah satu kepala uji dan digosokkan pada kain abrading standar di bawah tekanan yang ditentukan. Proses ini berlanjut hingga benang putus atau terjadi perubahan warna dan penampilan yang signifikan. Kemampuan gandanya untuk melakukan uji abrasi dan uji pilling menjadikan alat ini investasi yang sangat efisien untuk laboratorium kontrol kualitas mana pun.
Dirancang untuk produktivitas tinggi, mesin ini tersedia dalam konfigurasi 4, 6, atau 9 kepala uji, memungkinkan Anda menguji beberapa sampel secara bersamaan dan mempercepat proses pengembangan produk. Layar digitalnya yang canggih memungkinkan pengaturan jumlah siklus yang presisi dan menampilkan total akumulatif, memberikan kontrol penuh atas proses pengujian. Dilengkapi dengan set lengkap beban dan pemberat standar untuk berbagai aplikasi, mulai dari kain pakaian ringan hingga kain pelapis (upholstery) yang kuat, memastikan setiap pengujian sesuai dengan standar internasional.
Jangan biarkan kualitas kain Anda menjadi teka-teki. Dengan berinvestasi pada Martindale Tester, Anda mendapatkan data kuantitatif yang andal untuk memvalidasi spesifikasi material, melakukan riset dan pengembangan, serta menjamin produk akhir Anda dapat bertahan dari kerasnya penggunaan sehari-hari. Ini bukan sekadar mesin uji, melainkan sebuah jaminan kualitas yang melindungi reputasi merek Anda dan memastikan kepuasan pelanggan tingkat tertinggi.
Define the durability and aesthetic quality standards of your fabrics with the Digital Martindale Abrasion and Pilling Machine. Globally recognized as a fundamental testing method, this instrument is designed to accurately assess the resistance of fabrics, particularly woven textiles, to both abrasion (wear) and pilling (the formation of fuzzy balls on the surface). For manufacturers of furniture, apparel, household textiles, and workwear, this machine is an essential device for guaranteeing product longevity and appearance.
The Martindale machine uniquely simulates natural wear and tear through a controlled, multi-directional abrasion motion. A fabric sample is mounted on a testing head and rubbed against a standard abrading fabric under a specified pressure. This process continues until thread breakdown occurs or there is a significant change in color and appearance. Its powerful dual capability to perform both abrasion and pilling tests makes it a highly efficient investment for any quality control laboratory.
Engineered for high productivity, this machine is available in 4, 6, or 9 working position configurations, allowing you to test multiple samples simultaneously and significantly accelerate your product development timeline. Its advanced digital display enables precise presetting of cycle counts and shows the accumulative total, giving you complete control over the testing process. It comes equipped with a full set of standardized loads and weights for various applications, from light apparel fabrics to heavy-duty upholstery, ensuring every test complies with international standards.
Do not leave your fabric's quality to chance. By investing in a Martindale Tester, you acquire reliable, quantitative data to validate material specifications, conduct research and development, and ensure your final products can withstand the rigors of daily use. This is more than just a testing machine; it is a quality guarantee that protects your brand's reputation and ensures the highest level of customer satisfaction.

